{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["GAS DETECTION LIST(2頁目以降)"],"not_rendered":{"defined_names":2},"read":"whole","date_system":"1900"}

{"sheet":"GAS DETECTION LIST(2頁目以降)","index":0,"n_rows":4602,"n_cols":10,"rows_kept":4602,"merged":[[0,0,1,5],[2,0,4,9],[9,0,9,3],[9,4,9,9]]}
["RIKEN KEIKI Co.,Ltd."]
[]
["GAS DETECTION LIST"]
[]
[]
[]
[]
[]
[]
["GAS DATA",{"$nulls":3},"DETECTION DATA"]
["Detection Gas","Gas Cymbol","CAS Number","Chemical Formula","Principle","Sensor","Portable/Fixed","Detector","Measuring Rang","Rmarks"]
["(2-Methoxymethylethoxy)propanol","DPGME","34590-94-8","C7H16O3","HW","HW-6212","Fixed","GD-A80-70  Series","0～100%LEL"]
["1,1,1,1,3,3-Pentafluoropropane","R-245fa","460-73-1","C3H3F5","SG","SGU-8511","Fixed","GD-70D Series","0～5000ppm"]
["1,1,1,1,3,3-Pentafluoropropane","R-245fa","460-73-1","C3H3F5","SG","SGU-8511","Fixed","TP-70D","0～5000ppm"]
["1,1,1,1,3,3-Pentafluoropropane","R-245fa","460-73-1","C3H3F5","RI","DE-2113-35","Fixed","RI-257","0～5000ppm"]
["1,1,1,1,3,3-Pentafluoropropane","R-245fa","460-73-1","C3H3F5","SG","SG-8511","Fixed","GD-A80V Series","0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["1,1,1,1,3,3-Pentafluoropropane","R-245fa","460-73-1","C3H3F5","SG","SG-8511","Fixed","GD-D58・GH Series","0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["1,1,1,1,3,3-Pentafluoropropane","R-245fa","460-73-1","C3H3F5","SG","SG-8511","Fixed","SD-1GH Series","0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["1,1,1,1,3,3-Pentafluoropropane","R-245fa","460-73-1","C3H3F5","SG","SG-8511","Fixed","SD-D58・GH Series","0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["1,1,1,2,2,3,3,4,4,5,5,6,6-Tridecafluorooctane","C8H5F13","80793-17-5","C8H5F13","RI","DE-2113-35","Fixed","RI-257","0～10000ppm"]
["1,1,1,2,2,3,3,4,4,5,5,6,6-Tridecafluorooctane","C8H5F13","80793-17-5","C8H5F13","SG","SG-8562","Fixed","GD-A80V Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["1,1,1,2,2,3,3,4,4,5,5,6,6-Tridecafluorooctane","C8H5F13","80793-17-5","C8H5F13","SG","SG-8562","Fixed","GD-D58・GH Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["1,1,1,2,2,3,3,4,4,5,5,6,6-Tridecafluorooctane","C8H5F13","80793-17-5","C8H5F13","SG","SG-8562","Fixed","SD-1GH Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["1,1,1,2,2,3,3,4,4,5,5,6,6-Tridecafluorooctane","C8H5F13","80793-17-5","C8H5F13","SG","SG-8562","Fixed","SD-D58・GH Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["1,1,1,2,2-Pentafluoroethane","R-125","354-33-6","C2HF5","RI","DE-2113-35","Fixed","RI-257","0～5000ppm"]
["1,1,1,2-Tetrafluoroethane","R-134a","811-97-2","C2H2F4","SH","SH-8662","Portable","SP-220(TYPE SC)","0～250ppm"]
["1,1,1,2-Tetrafluoroethane","R-134a","811-97-2","C2H2F4","SH","SH-8661","Portable","SP-220(TYPE F)","0～10000ppm"]
["1,1,1,2-Tetrafluoroethane","R-134a","811-97-2","C2H2F4","SH","SH-8661","Portable","SP-220(TYPE H2)","0～10000ppm"]
["1,1,1,2-Tetrafluoroethane","R-134a","811-97-2","C2H2F4","SG","SGU-8524","Fixed","GD-70D Series","0～5000ppm"]
["1,1,1,2-Tetrafluoroethane","R-134a","811-97-2","C2H2F4","SG","SGU-8524","Fixed","TP-70D","0～5000ppm"]
["1,1,1,2-Tetrafluoroethane","R-134a","811-97-2","C2H2F4","RI","DE-2113-35","Fixed","RI-257","0～5000ppm"]
["1,1,1,2-Tetrafluoroethane","R-134a","811-97-2","C2H2F4","SG","SG-8524","Fixed","GD-A80V Series","0～5000ppm"]
["1,1,1,2-Tetrafluoroethane","R-134a","811-97-2","C2H2F4","SG","SG-8524","Fixed","GD-D58・GH Series","0～5000ppm"]
["1,1,1,2-Tetrafluoroethane","R-134a","811-97-2","C2H2F4","SG","SG-8524","Fixed","SD-1GH Series","0～5000ppm"]
["1,1,1,2-Tetrafluoroethane","R-134a","811-97-2","C2H2F4","SG","SG-8524","Fixed","SD-D58・GH Series","0～5000ppm"]
["1,1,1,3,3,3-Hexamethyldisilazane","HMDS","999-97-3","C6H18NSi2","ES","ESU-23RVM","Fixed","GD-70D Series","0～30ppm","Updated against electrolyte reduction"]
["1,1,1,3,3,3-Hexamethyldisilazane","HMDS","999-97-3","C6H18NSi2","ES","ESU-23RVM","Fixed","TP-70D","0～30ppm","Updated against electrolyte reduction"]
["1,1,1,3,3,3-Hexamethyldisilazane","HMDS","999-97-3","C6H18NSi2","SS","SSU-1925","Fixed","GD-70D+PLU Series","0～6ppm","PLU-70 required"]
["1,1,1,3,3,3-Hexamethyldisilazane","HMDS","999-97-3","C6H18NSi2","SS","SSU-1925","Fixed","GD-70DG","0～6ppm","PLU-70 required"]
["1,1,1,3,3,3-Hexamethyldisilazane","HMDS","999-97-3","C6H18NSi2","SG","SG-8511","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["1,1,1,3,3,3-Hexamethyldisilazane","HMDS","999-97-3","C6H18NSi2","SG","SG-8511","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["1,1,1,3,3,3-Hexamethyldisilazane","HMDS","999-97-3","C6H18NSi2","SG","SG-8511","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["1,1,1,3,3,3-Hexamethyldisilazane","HMDS","999-97-3","C6H18NSi2","SG","SG-8511","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["1,1,1,3,3-Pentafluorobutane","R365mfc","406-58-6","C4H5F5","SG","SG-8563","Fixed","GD-A80V Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["1,1,1,3,3-Pentafluorobutane","R365mfc","406-58-6","C4H5F5","SG","SG-8563","Fixed","GD-D58・GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["1,1,1,3,3-Pentafluorobutane","R365mfc","406-58-6","C4H5F5","SG","SG-8563","Fixed","SD-1GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["1,1,1,3,3-Pentafluorobutane","R365mfc","406-58-6","C4H5F5","SG","SG-8563","Fixed","SD-D58・GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["1,1,1-Trichloroethane ","C2H3CL3","71-55-6","C2H3CL3","SG","SGU-8523","Fixed","GD-70D Series","0～2000ppm"]
["1,1,1-Trichloroethane ","C2H3CL3","71-55-6","C2H3CL3","SG","SGU-8523","Fixed","TP-70D","0～2000ppm"]
["1,1,1-Trichloroethane ","C2H3CL3","71-55-6","C2H3CL3","SG","SG-8523","Fixed","GD-A80V Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm"]
["1,1,1-Trichloroethane ","C2H3CL3","71-55-6","C2H3CL3","SG","SG-8523","Fixed","GD-D58・GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm"]
["1,1,1-Trichloroethane ","C2H3CL3","71-55-6","C2H3CL3","SG","SG-8523","Fixed","SD-1GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm"]
["1,1,1-Trichloroethane ","C2H3CL3","71-55-6","C2H3CL3","SG","SG-8523","Fixed","SD-D58・GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm"]
["1,1,1-Trichloroethane ","C2H3CL3","71-55-6","C2H3CL3","SG","SG-8523","Fixed","GD-A80V Series","0～600ppm"]
["1,1,1-Trichloroethane ","C2H3CL3","71-55-6","C2H3CL3","SG","SG-8523","Fixed","GD-D58・GH Series","0～600ppm"]
["1,1,1-Trichloroethane ","C2H3CL3","71-55-6","C2H3CL3","SG","SG-8523","Fixed","SD-1GH Series","0～600ppm"]
["1,1,1-Trichloroethane ","C2H3CL3","71-55-6","C2H3CL3","SG","SG-8523","Fixed","SD-D58・GH Series","0～600ppm"]
["1,1,2,2-Tetrachloro-1,2-difluoroethane","R-112","76-12-0","C2F2CL4","SG","SG-8513","Fixed","GD-A80V Series","0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["1,1,2,2-Tetrachloro-1,2-difluoroethane","R-112","76-12-0","C2F2CL4","SG","SG-8513","Fixed","GD-D58・GH Series","0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["1,1,2,2-Tetrachloro-1,2-difluoroethane","R-112","76-12-0","C2F2CL4","SG","SG-8513","Fixed","SD-1GH Series","0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["1,1,2,2-Tetrachloro-1,2-difluoroethane","R-112","76-12-0","C2F2CL4","SG","SG-8513","Fixed","SD-D58・GH Series","0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["1,1,2,2-Tetrafluoroethyl 2,2,2-Trifluoroethyl Ether","C4H3OF7","406-78-0","C4H3OF7","RI","DE-2113-35","Fixed","RI-257","0～5000ppm"]
["1,1,2,2-Tetrafluoroethyl 2,2,2-Trifluoroethyl Ether","C4H3OF7","406-78-0","C4H3OF7","SG","SG-8521","Fixed","GD-A80V Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["1,1,2,2-Tetrafluoroethyl 2,2,2-Trifluoroethyl Ether","C4H3OF7","406-78-0","C4H3OF7","SG","SG-8521","Fixed","GD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["1,1,2,2-Tetrafluoroethyl 2,2,2-Trifluoroethyl Ether","C4H3OF7","406-78-0","C4H3OF7","SG","SG-8521","Fixed","SD-1GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["1,1,2,2-Tetrafluoroethyl 2,2,2-Trifluoroethyl Ether","C4H3OF7","406-78-0","C4H3OF7","SG","SG-8521","Fixed","SD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["1,1,2-Trichloro-1,2,2-trifluoroethane","R-113","76-13-1","C2F3CL3","RI","DE-2113-35","Fixed","RI-257","0～5000ppm"]
["1,1,2-Trichloro-1,2,2-trifluoroethane","R-113","76-13-1","C2F3CL3","SG","SG-8513","Fixed","GD-A80V Series","0～2000ppm/0～3000ppm/0～5000ppm/0～10000ppm/0～20000ppm"]
["1,1,2-Trichloro-1,2,2-trifluoroethane","R-113","76-13-1","C2F3CL3","SG","SG-8513","Fixed","GD-D58・GH Series","0～2000ppm/0～3000ppm/0～5000ppm/0～10000ppm/0～20000ppm"]
["1,1,2-Trichloro-1,2,2-trifluoroethane","R-113","76-13-1","C2F3CL3","SG","SG-8513","Fixed","SD-1GH Series","0～2000ppm/0～3000ppm/0～5000ppm/0～10000ppm/0～20000ppm"]
["1,1,2-Trichloro-1,2,2-trifluoroethane","R-113","76-13-1","C2F3CL3","SG","SG-8513","Fixed","SD-D58・GH Series","0～2000ppm/0～3000ppm/0～5000ppm/0～10000ppm/0～20000ppm"]
["1,1-Dichloro-1-fluoroethane","R-141b","1717-00-6","C2H3FCL2","RI","DE-2113-35","Fixed","RI-257","0～10000ppm"]
["1,1-Dichloro-1-fluoroethane","R-141b","1717-00-6","C2H3FCL2","SG","SG-8523","Fixed","GD-A80V Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["1,1-Dichloro-1-fluoroethane","R-141b","1717-00-6","C2H3FCL2","SG","SG-8523","Fixed","GD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["1,1-Dichloro-1-fluoroethane","R-141b","1717-00-6","C2H3FCL2","SG","SG-8523","Fixed","SD-1GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["1,1-Dichloro-1-fluoroethane","R-141b","1717-00-6","C2H3FCL2","SG","SG-8523","Fixed","SD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["1,1-Dichloro-2,2,2-trifluoroethane","R-123","306-83-2","C2HF3CL2","SH","SH-8661","Portable","SP-220(TYPE F)","0～10000ppm"]
["1,1-Dichloro-2,2,2-trifluoroethane","R-123","306-83-2","C2HF3CL2","ES","ESU-23EM","Fixed","GD-70D Series","0～100ppm","PLU-70 required"]
["1,1-Dichloro-2,2,2-trifluoroethane","R-123","306-83-2","C2HF3CL2","ES","ESU-23EM","Fixed","TP-70D","0～100ppm","PLU-70 required"]
["1,1-Dichloro-2,2,2-trifluoroethane","R-123","306-83-2","C2HF3CL2","RI","DE-2113-35","Fixed","RI-257","0～5000ppm"]
["1,1-Difluoroethane","R-152A","75-37-6","C2H4F2","SG","SGU-8511","Fixed","GD-70D Series","0～5000ppm"]
["1,1-Difluoroethane","R-152A","75-37-6","C2H4F2","SG","SGU-8511","Fixed","TP-70D","0～5000ppm"]
["1,1-Difluoroethane","R-152A","75-37-6","C2H4F2","SG","SG-8511","Fixed","GD-A80V Series","0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["1,1-Difluoroethane","R-152A","75-37-6","C2H4F2","SG","SG-8511","Fixed","GD-D58・GH Series","0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["1,1-Difluoroethane","R-152A","75-37-6","C2H4F2","SG","SG-8511","Fixed","SD-1GH Series","0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["1,1-Difluoroethane","R-152A","75-37-6","C2H4F2","SG","SG-8511","Fixed","SD-D58・GH Series","0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["1,1-Difluoroethane","R-152A","75-37-6","C2H4F2","SG","SG-8521","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["1,1-Difluoroethane","R-152A","75-37-6","C2H4F2","SG","SG-8521","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["1,1-Difluoroethane","R-152A","75-37-6","C2H4F2","SG","SG-8521","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["1,1-Difluoroethane","R-152A","75-37-6","C2H4F2","SG","SG-8521","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["1,2,3,4-Tetrahydronaphthalene","C10H12","119-64-2","C10H12","SG","SG-8521","Fixed","GD-A80V Series","★0～1000ppm/★0～2000ppm","★Range easily affected by environmental conditions and other"]
["1,2,3,4-Tetrahydronaphthalene","C10H12","119-64-2","C10H12","SG","SG-8521","Fixed","GD-D58・GH Series","★0～1000ppm/★0～2000ppm","★Range easily affected by environmental conditions and other"]
["1,2,3,4-Tetrahydronaphthalene","C10H12","119-64-2","C10H12","SG","SG-8521","Fixed","SD-1GH Series","★0～1000ppm/★0～2000ppm","★Range easily affected by environmental conditions and other"]
["1,2,3,4-Tetrahydronaphthalene","C10H12","119-64-2","C10H12","SG","SG-8521","Fixed","SD-D58・GH Series","★0～1000ppm/★0～2000ppm","★Range easily affected by environmental conditions and other"]
["1,2,3-Trichloropropane","C3H5CL3","96-18-4","C3H5CL3","SG","SG-8523","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["1,2,3-Trichloropropane","C3H5CL3","96-18-4","C3H5CL3","SG","SG-8523","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["1,2,3-Trichloropropane","C3H5CL3","96-18-4","C3H5CL3","SG","SG-8523","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["1,2,3-Trichloropropane","C3H5CL3","96-18-4","C3H5CL3","SG","SG-8523","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["1,2-Dichloroethane","EDC","107-06-2","C2H4CL2","SH","SH-8662","Portable","SP-220(TYPE SC)","0～10ppm"]
["1,2-Dichloroethane","EDC","107-06-2","C2H4CL2","SG","SGU-8513","Fixed","GD-70D Series","0～500ppm"]
["1,2-Dichloroethane","EDC","107-06-2","C2H4CL2","SG","SGU-8513","Fixed","TP-70D","0～500ppm"]
["1,2-Dichloroethane","EDC","107-06-2","C2H4CL2","RI","DE-3315-1","Fixed","SD-1RI Series","0～100%LEL"]
["1,2-Dichloroethane","EDC","107-06-2","C2H4CL2","SG","SG-8513","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["1,2-Dichloroethane","EDC","107-06-2","C2H4CL2","SG","SG-8513","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["1,2-Dichloroethane","EDC","107-06-2","C2H4CL2","SG","SG-8513","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["1,2-Dichloroethane","EDC","107-06-2","C2H4CL2","SG","SG-8513","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["1,2-Dichloroethane","EDC","107-06-2","C2H4CL2","SG","SG-8523","Fixed","GD-A80V Series","0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["1,2-Dichloroethane","EDC","107-06-2","C2H4CL2","SG","SG-8523","Fixed","GD-D58・GH Series","0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["1,2-Dichloroethane","EDC","107-06-2","C2H4CL2","SG","SG-8523","Fixed","SD-1GH Series","0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["1,2-Dichloroethane","EDC","107-06-2","C2H4CL2","SG","SG-8523","Fixed","SD-D58・GH Series","0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["1,2-Dichloropropane","C3H6CL2","78-87-5","C3H6CL2","SG","SG-8523","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm"]
["1,2-Dichloropropane","C3H6CL2","78-87-5","C3H6CL2","SG","SG-8523","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm"]
["1,2-Dichloropropane","C3H6CL2","78-87-5","C3H6CL2","SG","SG-8523","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm"]
["1,2-Dichloropropane","C3H6CL2","78-87-5","C3H6CL2","SG","SG-8523","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm"]
["1,3-Butadiene","C4H6","106-99-0","C4H6","HW","NC-6215","Portable","GP-1000(HC/CH4)","0～100%LEL"]
["1,3-Butadiene","C4H6","106-99-0","C4H6","HW","NC-6307","Portable","NC-1000(HC/CH4)","0～10000ppm"]
["1,3-Butadiene","C4H6","106-99-0","C4H6","SH","SH-8661","Portable","SP-220(TYPE H2)","0～10000ppm"]
["1,3-Butadiene","C4H6","106-99-0","C4H6","SG","SGU-8521","Fixed","GD-70D Series","0～2000ppm"]
["1,3-Butadiene","C4H6","106-99-0","C4H6","SG","SGU-8521","Fixed","TP-70D","0～2000ppm"]
["1,3-Butadiene","C4H6","106-99-0","C4H6","RI","DE-3315-1","Fixed","SD-1RI Series","0～100%LEL"]
["1,3-Butadiene","C4H6","106-99-0","C4H6","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["1,3-Butadiene","C4H6","106-99-0","C4H6","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["1,3-Butadiene","C4H6","106-99-0","C4H6","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～11000ppm"]
["1,3-Butadiene","C4H6","106-99-0","C4H6","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～11000ppm"]
["1,3-Butadiene","C4H6","106-99-0","C4H6","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～11000ppm"]
["1,3-Butadiene","C4H6","106-99-0","C4H6","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～11000ppm"]
["1,3-Butadiene","C4H6","106-99-0","C4H6","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～11000ppm"]
["1,3-Butadiene","C4H6","106-99-0","C4H6","HW","NC-6250","Fixed","GD-A80 Series","～100%LEL/～11000ppm"]
["1,3-Butadiene","C4H6","106-99-0","C4H6","HW","NC-6250","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～11000ppm"]
["1,3-Butadiene","C4H6","106-99-0","C4H6","SG","SG-8511","Fixed","GD-A80V Series","0～3000ppm/0～5000ppm/0～10000ppm/0～50%LEL/0～100%LEL"]
["1,3-Butadiene","C4H6","106-99-0","C4H6","SG","SG-8511","Fixed","GD-D58・GH Series","0～3000ppm/0～5000ppm/0～10000ppm/0～50%LEL/0～100%LEL"]
["1,3-Butadiene","C4H6","106-99-0","C4H6","SG","SG-8511","Fixed","SD-1GH Series","0～3000ppm/0～5000ppm/0～10000ppm/0～50%LEL/0～100%LEL"]
["1,3-Butadiene","C4H6","106-99-0","C4H6","SG","SG-8511","Fixed","SD-D58・GH Series","0～3000ppm/0～5000ppm/0～10000ppm/0～50%LEL/0～100%LEL"]
["1,3-Butadiene","C4H6","106-99-0","C4H6","SG","SG-8521","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["1,3-Butadiene","C4H6","106-99-0","C4H6","SG","SG-8521","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["1,3-Butadiene","C4H6","106-99-0","C4H6","SG","SG-8521","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["1,3-Butadiene","C4H6","106-99-0","C4H6","SG","SG-8521","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["1,3-Dichloro-1,1,2,2,3-pentafluoropropane","R-225cb","507-55-1","C3HF5CL2","SG","SG-8513","Fixed","GD-A80V Series","0～10000ppm"]
["1,3-Dichloro-1,1,2,2,3-pentafluoropropane","R-225cb","507-55-1","C3HF5CL2","SG","SG-8513","Fixed","GD-D58・GH Series","0～10000ppm"]
["1,3-Dichloro-1,1,2,2,3-pentafluoropropane","R-225cb","507-55-1","C3HF5CL2","SG","SG-8513","Fixed","SD-1GH Series","0～10000ppm"]
["1,3-Dichloro-1,1,2,2,3-pentafluoropropane","R-225cb","507-55-1","C3HF5CL2","SG","SG-8513","Fixed","SD-D58・GH Series","0～10000ppm"]
["1,3-Dimethyl-2-imidazolidinone","DMI","80-73-9","C5H10N2O","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["1,3-Dimethyl-2-imidazolidinone","DMI","80-73-9","C5H10N2O","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["1,3-Dimethyl-2-imidazolidinone","DMI","80-73-9","C5H10N2O","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["1,3-Dimethyl-2-imidazolidinone","DMI","80-73-9","C5H10N2O","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["1,3-Dimethyl-2-imidazolidinone","DMI","80-73-9","C5H10N2O","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["1,3-Dimethyl-2-imidazolidinone","DMI","80-73-9","C5H10N2O","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["1,3-Dimethyl-2-imidazolidinone","DMI","80-73-9","C5H10N2O","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["1,3-Dimethyl-2-imidazolidinone","DMI","80-73-9","C5H10N2O","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["1,3-Dioxolane","C3H6O2","646-46-0","C3H6O2","RI","DE-3315-2","Fixed","SD-1RI Series","0～100%LEL"]
["1,3-Dioxolane","C3H6O2","646-46-0","C3H6O2","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["1,3-Dioxolane","C3H6O2","646-46-0","C3H6O2","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["1,3-Dioxolane","C3H6O2","646-46-0","C3H6O2","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["1,3-Dioxolane","C3H6O2","646-46-0","C3H6O2","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["1,3-Dioxolane","C3H6O2","646-46-0","C3H6O2","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["1,3-Dioxolane","C3H6O2","646-46-0","C3H6O2","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["1,3-Dioxolane","C3H6O2","646-46-0","C3H6O2","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["1,3-Dioxolane","C3H6O2","646-46-0","C3H6O2","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["1,5-Hexadiene","HeXD","592-42-7","C6H10","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","0～100%LEL"]
["1,5-Hexadiene","HeXD","592-42-7","C6H10","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","0～100%LEL"]
["1,5-Hexadiene","HeXD","592-42-7","C6H10","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～20000ppm"]
["1,5-Hexadiene","HeXD","592-42-7","C6H10","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～20000ppm"]
["1,5-Hexadiene","HeXD","592-42-7","C6H10","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～20000ppm"]
["1,5-Hexadiene","HeXD","592-42-7","C6H10","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～20000ppm"]
["1,5-Hexadiene","HeXD","592-42-7","C6H10","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～20000ppm"]
["1,7-Octadiene","C8H14","3710-30-3","C8H14","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["1,7-Octadiene","C8H14","3710-30-3","C8H14","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["1,7-Octadiene","C8H14","3710-30-3","C8H14","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～5000ppm"]
["1,7-Octadiene","C8H14","3710-30-3","C8H14","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～5000ppm"]
["1,7-Octadiene","C8H14","3710-30-3","C8H14","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～5000ppm"]
["1,7-Octadiene","C8H14","3710-30-3","C8H14","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～5000ppm"]
["1,7-Octadiene","C8H14","3710-30-3","C8H14","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～5000ppm"]
["1-Bromopropane","C3H7Br","106-94-5","C3H7Br","SG","SG-8562","Fixed","GD-A80V Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["1-Bromopropane","C3H7Br","106-94-5","C3H7Br","SG","SG-8562","Fixed","GD-D58・GH Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["1-Bromopropane","C3H7Br","106-94-5","C3H7Br","SG","SG-8562","Fixed","SD-1GH Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["1-Bromopropane","C3H7Br","106-94-5","C3H7Br","SG","SG-8562","Fixed","SD-D58・GH Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["1-Butene","C4H8","106-98-9","C4H8","HW","NC-6215","Portable","GP-1000(Specified cal.gas)","0～100%LEL"]
["1-Butene","C4H8","106-98-9","C4H8","RI","DE-3315-1","Fixed","SD-1RI Series","0～100%LEL"]
["1-Butene","C4H8","106-98-9","C4H8","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["1-Butene","C4H8","106-98-9","C4H8","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["1-Butene","C4H8","106-98-9","C4H8","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～16000ppm"]
["1-Butene","C4H8","106-98-9","C4H8","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～16000ppm"]
["1-Butene","C4H8","106-98-9","C4H8","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～16000ppm"]
["1-Butene","C4H8","106-98-9","C4H8","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～16000ppm"]
["1-Butene","C4H8","106-98-9","C4H8","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～16000ppm"]
["1-Butene","C4H8","106-98-9","C4H8","SG","SG-8521","Fixed","GD-A80V Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm"]
["1-Butene","C4H8","106-98-9","C4H8","SG","SG-8521","Fixed","GD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm"]
["1-Butene","C4H8","106-98-9","C4H8","SG","SG-8521","Fixed","SD-1GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm"]
["1-Butene","C4H8","106-98-9","C4H8","SG","SG-8521","Fixed","SD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm"]
["1-Chloro-1,1-difluoroethane","R-142b","75-68-3","C2H3F2CL","SH","SH-8661","Portable","SP-220(TYPE F)","0～1000ppm"]
["1-Chloro-1,1-difluoroethane","R-142b","75-68-3","C2H3F2CL","SG","SG-8513","Fixed","GD-A80V Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["1-Chloro-1,1-difluoroethane","R-142b","75-68-3","C2H3F2CL","SG","SG-8513","Fixed","GD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["1-Chloro-1,1-difluoroethane","R-142b","75-68-3","C2H3F2CL","SG","SG-8513","Fixed","SD-1GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["1-Chloro-1,1-difluoroethane","R-142b","75-68-3","C2H3F2CL","SG","SG-8513","Fixed","SD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["1-Chlorobutane","NBC","109-69-3","C4H9CL","SG","SG-8513","Fixed","GD-A80V Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["1-Chlorobutane","NBC","109-69-3","C4H9CL","SG","SG-8513","Fixed","GD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["1-Chlorobutane","NBC","109-69-3","C4H9CL","SG","SG-8513","Fixed","SD-1GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["1-Chlorobutane","NBC","109-69-3","C4H9CL","SG","SG-8513","Fixed","SD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["1-Chloropropane","NPC","540-54-5","C3H7CL","SG","SG-8523","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["1-Chloropropane","NPC","540-54-5","C3H7CL","SG","SG-8523","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["1-Chloropropane","NPC","540-54-5","C3H7CL","SG","SG-8523","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["1-Chloropropane","NPC","540-54-5","C3H7CL","SG","SG-8523","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["1-Hexanol","HexOH","111-27-3","C6H14O","SG","SG-8521","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["1-Hexanol","HexOH","111-27-3","C6H14O","SG","SG-8521","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["1-Hexanol","HexOH","111-27-3","C6H14O","SG","SG-8521","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["1-Hexanol","HexOH","111-27-3","C6H14O","SG","SG-8521","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["1-Hexene","1-C6H12","592-41-6","C6H12","SG","SGU-8521","Fixed","GD-70D Series","0～1000ppm"]
["1-Hexene","1-C6H12","592-41-6","C6H12","SG","SGU-8521","Fixed","TP-70D","0～1000ppm"]
["1-Hexene","1-C6H12","592-41-6","C6H12","RI","DE-3315-1","Fixed","SD-1RI Series","0～100%LEL"]
["1-Hexene","1-C6H12","592-41-6","C6H12","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["1-Hexene","1-C6H12","592-41-6","C6H12","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["1-Hexene","1-C6H12","592-41-6","C6H12","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～12000ppm"]
["1-Hexene","1-C6H12","592-41-6","C6H12","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～12000ppm"]
["1-Hexene","1-C6H12","592-41-6","C6H12","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～12000ppm"]
["1-Hexene","1-C6H12","592-41-6","C6H12","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～12000ppm"]
["1-Hexene","1-C6H12","592-41-6","C6H12","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～12000ppm"]
["1-Hexene","1-C6H12","592-41-6","C6H12","SG","SG-8521","Fixed","GD-A80V Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["1-Hexene","1-C6H12","592-41-6","C6H12","SG","SG-8521","Fixed","GD-D58・GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["1-Hexene","1-C6H12","592-41-6","C6H12","SG","SG-8521","Fixed","SD-1GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["1-Hexene","1-C6H12","592-41-6","C6H12","SG","SG-8521","Fixed","SD-D58・GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["1-Methylpyrrolidine","C5H11N","120-94-5","C5H11N","SG","SG-8562","Fixed","GD-A80V Series","0～20ppm/0～30ppm/0～50ppm/0～100ppm/0～200ppm"]
["1-Methylpyrrolidine","C5H11N","120-94-5","C5H11N","SG","SG-8562","Fixed","GD-D58・GH Series","0～20ppm/0～30ppm/0～50ppm/0～100ppm/0～200ppm"]
["1-Methylpyrrolidine","C5H11N","120-94-5","C5H11N","SG","SG-8562","Fixed","SD-1GH Series","0～20ppm/0～30ppm/0～50ppm/0～100ppm/0～200ppm"]
["1-Methylpyrrolidine","C5H11N","120-94-5","C5H11N","SG","SG-8562","Fixed","SD-D58・GH Series","0～20ppm/0～30ppm/0～50ppm/0～100ppm/0～200ppm"]
["1-Pentene","1-C5H10","109-67-1","C5H10","HW","NC-6215","Portable","GP-1000(Specified cal.gas)","0～100%LEL"]
["2-(Dimethylamino)ethanol","DMEA","108-01-0","C4H11NO","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～30%LEL/～4000ppm"]
["2-(Dimethylamino)ethanol","DMEA","108-01-0","C4H11NO","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～30%LEL/～4000ppm"]
["2-(Dimethylamino)ethanol","DMEA","108-01-0","C4H11NO","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～30%LEL/～4000ppm"]
["2-(Dimethylamino)ethanol","DMEA","108-01-0","C4H11NO","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～30%LEL/～4000ppm"]
["2-(Dimethylamino)ethanol","DMEA","108-01-0","C4H11NO","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～30%LEL/～4000ppm"]
["2-(Dimethylamino)ethanol","DMEA","108-01-0","C4H11NO","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["2-(Dimethylamino)ethanol","DMEA","108-01-0","C4H11NO","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["2-(Dimethylamino)ethanol","DMEA","108-01-0","C4H11NO","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["2-(Dimethylamino)ethanol","DMEA","108-01-0","C4H11NO","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["2-(Dimethylamino)ethanol","DMEA","108-01-0","C4H11NO","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["2-(Dimethylamino)ethanol","DMEA","108-01-0","C4H11NO","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["2-(Dimethylamino)ethanol","DMEA","108-01-0","C4H11NO","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["2-(Dimethylamino)ethanol","DMEA","108-01-0","C4H11NO","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["2-(Dimethylamino)ethanol","DMEA","108-01-0","C4H11NO","SG","SG-8521","Fixed","GD-A80V Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["2-(Dimethylamino)ethanol","DMEA","108-01-0","C4H11NO","SG","SG-8521","Fixed","GD-D58・GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["2-(Dimethylamino)ethanol","DMEA","108-01-0","C4H11NO","SG","SG-8521","Fixed","SD-1GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["2-(Dimethylamino)ethanol","DMEA","108-01-0","C4H11NO","SG","SG-8521","Fixed","SD-D58・GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["2,2,2-Trifluoroethanol","C2H3OF3","75-89-8","C2H3OF3","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["2,2,2-Trifluoroethanol","C2H3OF3","75-89-8","C2H3OF3","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["2,2,2-Trifluoroethanol","C2H3OF3","75-89-8","C2H3OF3","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～55000ppm"]
["2,2,2-Trifluoroethanol","C2H3OF3","75-89-8","C2H3OF3","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～55000ppm"]
["2,2,2-Trifluoroethanol","C2H3OF3","75-89-8","C2H3OF3","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～55000ppm"]
["2,2,2-Trifluoroethanol","C2H3OF3","75-89-8","C2H3OF3","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～55000ppm"]
["2,2,2-Trifluoroethanol","C2H3OF3","75-89-8","C2H3OF3","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～55000ppm"]
["2,2,2-Trifluoroethanol","C2H3OF3","75-89-8","C2H3OF3","SG","SG-8521","Fixed","GD-A80V Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["2,2,2-Trifluoroethanol","C2H3OF3","75-89-8","C2H3OF3","SG","SG-8521","Fixed","GD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["2,2,2-Trifluoroethanol","C2H3OF3","75-89-8","C2H3OF3","SG","SG-8521","Fixed","SD-1GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["2,2,2-Trifluoroethanol","C2H3OF3","75-89-8","C2H3OF3","SG","SG-8521","Fixed","SD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["2,2-Difluorobutane","C4H8F2","353-81-1","C4H8F2","RI","DE-2113-37","Fixed","RI-257","0～5000ppm"]
["2,2-Dimethylbutane","Neo-Hex","75-83-2","C6H14","SG","SG-8521","Fixed","GD-A80V Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["2,2-Dimethylbutane","Neo-Hex","75-83-2","C6H14","SG","SG-8521","Fixed","GD-D58・GH Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["2,2-Dimethylbutane","Neo-Hex","75-83-2","C6H14","SG","SG-8521","Fixed","SD-1GH Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["2,2-Dimethylbutane","Neo-Hex","75-83-2","C6H14","SG","SG-8521","Fixed","SD-D58・GH Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["2,3,3,3-Tetrafluoroprop-1-ene","CH2C2F4","754-12-1","C3H2F4","SH","SH-8662","Portable","SP-220(TYPE SC)","0～30ppm"]
["2,3,3,3-Tetrafluoroprop-1-ene","CH2C2F4","754-12-1","C3H2F4","SH","SH-8661","Portable","SP-220(TYPE F)","0～2000ppm"]
["2,3,3,3-Tetrafluoroprop-1-ene","CH2C2F4","754-12-1","C3H2F4","SH","SH-8661","Portable","SP-220(TYPE H2)","0～2000ppm"]
["2,3,3,3-Tetrafluoroprop-1-ene","CH2C2F4","754-12-1","C3H2F4","RI","DE-2113-35","Fixed","RI-257","0～5000ppm"]
["2,3,3,3-Tetrafluoroprop-1-ene","CH2C2F4","754-12-1","C3H2F4","SG","SG-8521","Fixed","GD-A80V Series","0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm/0～10000ppm/0～20000ppm"]
["2,3,3,3-Tetrafluoroprop-1-ene","CH2C2F4","754-12-1","C3H2F4","SG","SG-8521","Fixed","GD-D58・GH Series","0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm/0～10000ppm/0～20000ppm"]
["2,3,3,3-Tetrafluoroprop-1-ene","CH2C2F4","754-12-1","C3H2F4","SG","SG-8521","Fixed","SD-1GH Series","0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm/0～10000ppm/0～20000ppm"]
["2,3,3,3-Tetrafluoroprop-1-ene","CH2C2F4","754-12-1","C3H2F4","SG","SG-8521","Fixed","SD-D58・GH Series","0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm/0～10000ppm/0～20000ppm"]
["2,4-Pentanedione","2,4-pent","123-54-6","C5H8O2","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["2,4-Pentanedione","2,4-pent","123-54-6","C5H8O2","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["2,4-Pentanedione","2,4-pent","123-54-6","C5H8O2","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["2,4-Pentanedione","2,4-pent","123-54-6","C5H8O2","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["2,4-Pentanedione","2,4-pent","123-54-6","C5H8O2","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["2,4-Pentanedione","2,4-pent","123-54-6","C5H8O2","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["2,4-Pentanedione","2,4-pent","123-54-6","C5H8O2","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["2,4-Pentanedione","2,4-pent","123-54-6","C5H8O2","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["2,5-Norbornadiene","BCHD","121-46-0","C7H8","SG","SG-8521","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["2,5-Norbornadiene","BCHD","121-46-0","C7H8","SG","SG-8521","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["2,5-Norbornadiene","BCHD","121-46-0","C7H8","SG","SG-8521","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["2,5-Norbornadiene","BCHD","121-46-0","C7H8","SG","SG-8521","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["2-Butanol","2-BuOH","78-92-2","C4H10O","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["2-Butanol","2-BuOH","78-92-2","C4H10O","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["2-Butanol","2-BuOH","78-92-2","C4H10O","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～17000ppm"]
["2-Butanol","2-BuOH","78-92-2","C4H10O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～17000ppm"]
["2-Butanol","2-BuOH","78-92-2","C4H10O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～17000ppm"]
["2-Butanol","2-BuOH","78-92-2","C4H10O","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～17000ppm"]
["2-Butanol","2-BuOH","78-92-2","C4H10O","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～17000ppm"]
["2-Butoxyethanol","C6H14O2","111-76-2","C6H14O2","HW","NC-6211","Fixed","GD-A80 Series","～25%LEL/～2750ppm"]
["2-Butoxyethanol","C6H14O2","111-76-2","C6H14O2","HW","NC-6211","Fixed","GD-D58(TYPE GP) Series","～25%LEL/～2750ppm"]
["2-Butoxyethanol","C6H14O2","111-76-2","C6H14O2","HW","NC-6211","Fixed","GD-D58(TYPE NC) Series","～25%LEL/～2750ppm"]
["2-Butoxyethanol","C6H14O2","111-76-2","C6H14O2","HW","NC-6211","Fixed","SD-1(TYPE NC) Series","～25%LEL/～2750ppm"]
["2-Butoxyethanol","C6H14O2","111-76-2","C6H14O2","HW","NC-6211","Fixed","SD-D58(TYPE NC) Series","～25%LEL/～2750ppm"]
["2-Butoxyethanol","C6H14O2","111-76-2","C6H14O2","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["2-Butoxyethanol","C6H14O2","111-76-2","C6H14O2","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["2-Butoxyethanol","C6H14O2","111-76-2","C6H14O2","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["2-Butoxyethanol","C6H14O2","111-76-2","C6H14O2","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["2-Butoxyethanol","C6H14O2","111-76-2","C6H14O2","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["2-Butoxyethanol","C6H14O2","111-76-2","C6H14O2","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["2-Butoxyethanol","C6H14O2","111-76-2","C6H14O2","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["2-Butoxyethanol","C6H14O2","111-76-2","C6H14O2","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["2-Butoxyethanol","C6H14O2","111-76-2","C6H14O2","SG","SG-8521","Fixed","GD-A80V Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["2-Butoxyethanol","C6H14O2","111-76-2","C6H14O2","SG","SG-8521","Fixed","GD-D58・GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["2-Butoxyethanol","C6H14O2","111-76-2","C6H14O2","SG","SG-8521","Fixed","SD-1GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["2-Butoxyethanol","C6H14O2","111-76-2","C6H14O2","SG","SG-8521","Fixed","SD-D58・GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["2-Butoxyethyl acetate","C8H16O3","112-07-2","C8H16O3","SG","SG-8521","Fixed","GD-A80V Series","0～200ppm"]
["2-Butoxyethyl acetate","C8H16O3","112-07-2","C8H16O3","SG","SG-8521","Fixed","GD-D58・GH Series","0～200ppm"]
["2-Butoxyethyl acetate","C8H16O3","112-07-2","C8H16O3","SG","SG-8521","Fixed","SD-1GH Series","0～200ppm"]
["2-Butoxyethyl acetate","C8H16O3","112-07-2","C8H16O3","SG","SG-8521","Fixed","SD-D58・GH Series","0～200ppm"]
["2-Butyne","2-C4H6","503-17-3","C4H6","SG","SG-8562","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["2-Butyne","2-C4H6","503-17-3","C4H6","SG","SG-8562","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["2-Butyne","2-C4H6","503-17-3","C4H6","SG","SG-8562","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["2-Butyne","2-C4H6","503-17-3","C4H6","SG","SG-8562","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["2-Ethoxyethanol","C4H10O2","110-80-5","C4H10O2","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～85%LEL/～15300ppm"]
["2-Ethoxyethanol","C4H10O2","110-80-5","C4H10O2","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～85%LEL/～15300ppm"]
["2-Ethoxyethanol","C4H10O2","110-80-5","C4H10O2","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～85%LEL/～15300ppm"]
["2-Ethoxyethanol","C4H10O2","110-80-5","C4H10O2","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～85%LEL/～15300ppm"]
["2-Ethoxyethanol","C4H10O2","110-80-5","C4H10O2","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～85%LEL/～15300ppm"]
["2-Ethoxyethanol","C4H10O2","110-80-5","C4H10O2","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["2-Ethoxyethanol","C4H10O2","110-80-5","C4H10O2","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["2-Ethoxyethanol","C4H10O2","110-80-5","C4H10O2","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["2-Ethoxyethanol","C4H10O2","110-80-5","C4H10O2","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["2-Ethoxyethanol","C4H10O2","110-80-5","C4H10O2","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["2-Ethoxyethanol","C4H10O2","110-80-5","C4H10O2","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["2-Ethoxyethanol","C4H10O2","110-80-5","C4H10O2","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["2-Ethoxyethanol","C4H10O2","110-80-5","C4H10O2","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["2-Ethoxyethanol","C4H10O2","110-80-5","C4H10O2","SG","SG-8521","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["2-Ethoxyethanol","C4H10O2","110-80-5","C4H10O2","SG","SG-8521","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["2-Ethoxyethanol","C4H10O2","110-80-5","C4H10O2","SG","SG-8521","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["2-Ethoxyethanol","C4H10O2","110-80-5","C4H10O2","SG","SG-8521","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["2-Ethoxyethyl acetate","C6H12O3","111-15-9","C6H12O3","SG","SGU-8511","Fixed","GD-70D Series","0～3000ppm"]
["2-Ethoxyethyl acetate","C6H12O3","111-15-9","C6H12O3","SG","SGU-8511","Fixed","TP-70D","0～3000ppm"]
["2-Ethoxyethyl acetate","C6H12O3","111-15-9","C6H12O3","HW","NC-6211","Fixed","GD-A80 Series","～50%LEL/～8500ppm"]
["2-Ethoxyethyl acetate","C6H12O3","111-15-9","C6H12O3","HW","NC-6211","Fixed","GD-D58(TYPE GP) Series","～50%LEL/～8500ppm"]
["2-Ethoxyethyl acetate","C6H12O3","111-15-9","C6H12O3","HW","NC-6211","Fixed","GD-D58(TYPE NC) Series","～50%LEL/～8500ppm"]
["2-Ethoxyethyl acetate","C6H12O3","111-15-9","C6H12O3","HW","NC-6211","Fixed","SD-1(TYPE NC) Series","～50%LEL/～8500ppm"]
["2-Ethoxyethyl acetate","C6H12O3","111-15-9","C6H12O3","HW","NC-6211","Fixed","SD-D58(TYPE NC) Series","～50%LEL/～8500ppm"]
["2-Ethoxyethyl acetate","C6H12O3","111-15-9","C6H12O3","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["2-Ethoxyethyl acetate","C6H12O3","111-15-9","C6H12O3","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["2-Ethoxyethyl acetate","C6H12O3","111-15-9","C6H12O3","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["2-Ethoxyethyl acetate","C6H12O3","111-15-9","C6H12O3","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["2-Ethoxyethyl acetate","C6H12O3","111-15-9","C6H12O3","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["2-Ethoxyethyl acetate","C6H12O3","111-15-9","C6H12O3","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["2-Ethoxyethyl acetate","C6H12O3","111-15-9","C6H12O3","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["2-Ethoxyethyl acetate","C6H12O3","111-15-9","C6H12O3","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["2-Ethoxyethyl acetate","C6H12O3","111-15-9","C6H12O3","SG","SG-8511","Fixed","GD-A80V Series","0～1000ppm/0～2000ppm/0～3000ppm"]
["2-Ethoxyethyl acetate","C6H12O3","111-15-9","C6H12O3","SG","SG-8511","Fixed","GD-D58・GH Series","0～1000ppm/0～2000ppm/0～3000ppm"]
["2-Ethoxyethyl acetate","C6H12O3","111-15-9","C6H12O3","SG","SG-8511","Fixed","SD-1GH Series","0～1000ppm/0～2000ppm/0～3000ppm"]
["2-Ethoxyethyl acetate","C6H12O3","111-15-9","C6H12O3","SG","SG-8511","Fixed","SD-D58・GH Series","0～1000ppm/0～2000ppm/0～3000ppm"]
["2-Ethoxyethyl acetate","C6H12O3","111-15-9","C6H12O3","SG","SG-8521","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["2-Ethoxyethyl acetate","C6H12O3","111-15-9","C6H12O3","SG","SG-8521","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["2-Ethoxyethyl acetate","C6H12O3","111-15-9","C6H12O3","SG","SG-8521","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["2-Ethoxyethyl acetate","C6H12O3","111-15-9","C6H12O3","SG","SG-8521","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["2-Ethylhexyl Acrylate Monomer","2-EHA","103-11-7","C11H20O2","SG","SG-8521","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["2-Ethylhexyl Acrylate Monomer","2-EHA","103-11-7","C11H20O2","SG","SG-8521","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["2-Ethylhexyl Acrylate Monomer","2-EHA","103-11-7","C11H20O2","SG","SG-8521","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["2-Ethylhexyl Acrylate Monomer","2-EHA","103-11-7","C11H20O2","SG","SG-8521","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["2-Ethylhexyl Methacrylate","2-EHM","688-84-6","C12H22O2","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["2-Ethylhexyl Methacrylate","2-EHM","688-84-6","C12H22O2","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["2-Ethylhexyl Methacrylate","2-EHM","688-84-6","C12H22O2","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["2-Ethylhexyl Methacrylate","2-EHM","688-84-6","C12H22O2","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["2-Ethylhexyl Methacrylate","2-EHM","688-84-6","C12H22O2","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["2-Ethylhexyl Methacrylate","2-EHM","688-84-6","C12H22O2","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["2-Ethylhexyl Methacrylate","2-EHM","688-84-6","C12H22O2","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["2-Ethylhexyl Methacrylate","2-EHM","688-84-6","C12H22O2","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["2-Fluorobutane","C4H9F","359-01-3","C4H9F","SG","SG-8521","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["2-Fluorobutane","C4H9F","359-01-3","C4H9F","SG","SG-8521","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["2-Fluorobutane","C4H9F","359-01-3","C4H9F","SG","SG-8521","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["2-Fluorobutane","C4H9F","359-01-3","C4H9F","SG","SG-8521","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["2-Hydroxyethyl Methacrylate","C6H10O3","868-77-9","C6H10O3","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["2-Hydroxyethyl Methacrylate","C6H10O3","868-77-9","C6H10O3","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["2-Hydroxyethyl Methacrylate","C6H10O3","868-77-9","C6H10O3","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["2-Hydroxyethyl Methacrylate","C6H10O3","868-77-9","C6H10O3","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["2-Hydroxyethyl Methacrylate","C6H10O3","868-77-9","C6H10O3","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["2-Hydroxyethyl Methacrylate","C6H10O3","868-77-9","C6H10O3","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["2-Hydroxyethyl Methacrylate","C6H10O3","868-77-9","C6H10O3","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["2-Methoxyethanol","C3H8O2","109-86-4","C3H8O2","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["2-Methoxyethanol","C3H8O2","109-86-4","C3H8O2","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["2-Methoxyethanol","C3H8O2","109-86-4","C3H8O2","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～25000ppm"]
["2-Methoxyethanol","C3H8O2","109-86-4","C3H8O2","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～25000ppm"]
["2-Methoxyethanol","C3H8O2","109-86-4","C3H8O2","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～25000ppm"]
["2-Methoxyethanol","C3H8O2","109-86-4","C3H8O2","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～25000ppm"]
["2-Methoxyethanol","C3H8O2","109-86-4","C3H8O2","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～25000ppm"]
["2-Methoxyethanol","C3H8O2","109-86-4","C3H8O2","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["2-Methoxyethanol","C3H8O2","109-86-4","C3H8O2","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["2-Methoxyethanol","C3H8O2","109-86-4","C3H8O2","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["2-Methoxyethanol","C3H8O2","109-86-4","C3H8O2","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["2-Methoxyethanol","C3H8O2","109-86-4","C3H8O2","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["2-Methoxyethanol","C3H8O2","109-86-4","C3H8O2","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["2-Methoxyethanol","C3H8O2","109-86-4","C3H8O2","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["2-Methoxyethanol","C3H8O2","109-86-4","C3H8O2","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["2-Methoxyethanol","C3H8O2","109-86-4","C3H8O2","SG","SG-8521","Fixed","GD-A80V Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["2-Methoxyethanol","C3H8O2","109-86-4","C3H8O2","SG","SG-8521","Fixed","GD-D58・GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["2-Methoxyethanol","C3H8O2","109-86-4","C3H8O2","SG","SG-8521","Fixed","SD-1GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["2-Methoxyethanol","C3H8O2","109-86-4","C3H8O2","SG","SG-8521","Fixed","SD-D58・GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["2-Methylhexane","i-C7H16","591-76-4","C7H16","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["2-Methylhexane","i-C7H16","591-76-4","C7H16","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["2-Methylhexane","i-C7H16","591-76-4","C7H16","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["2-Methylhexane","i-C7H16","591-76-4","C7H16","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["2-Methylhexane","i-C7H16","591-76-4","C7H16","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["2-Methylhexane","i-C7H16","591-76-4","C7H16","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["2-Methylhexane","i-C7H16","591-76-4","C7H16","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["2-Methylhexane","i-C7H16","591-76-4","C7H16","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["2-Norbornene","C7H10","498-66-8","C7H10","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～10000ppm"]
["2-Norbornene","C7H10","498-66-8","C7H10","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～10000ppm"]
["2-Norbornene","C7H10","498-66-8","C7H10","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～10000ppm"]
["2-Norbornene","C7H10","498-66-8","C7H10","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～10000ppm"]
["2-Norbornene","C7H10","498-66-8","C7H10","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～10000ppm"]
["3-Methoxybutyl Acetate","C7H14O3","4435-53-4","C7H14O3","SG","SG-8562","Fixed","GD-A80V Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["3-Methoxybutyl Acetate","C7H14O3","4435-53-4","C7H14O3","SG","SG-8562","Fixed","GD-D58・GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["3-Methoxybutyl Acetate","C7H14O3","4435-53-4","C7H14O3","SG","SG-8562","Fixed","SD-1GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["3-Methoxybutyl Acetate","C7H14O3","4435-53-4","C7H14O3","SG","SG-8562","Fixed","SD-D58・GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["3-Methyl-3-pentanol","3M3POH","77-74-7","C6H14O","SG","SG-8521","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["3-Methyl-3-pentanol","3M3POH","77-74-7","C6H14O","SG","SG-8521","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["3-Methyl-3-pentanol","3M3POH","77-74-7","C6H14O","SG","SG-8521","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["3-Methyl-3-pentanol","3M3POH","77-74-7","C6H14O","SG","SG-8521","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["4-Methoxy-4-methyl-2-pentanone","C7H14O2","107-70-0","C7H14O2","SG","SG-8521","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["4-Methoxy-4-methyl-2-pentanone","C7H14O2","107-70-0","C7H14O2","SG","SG-8521","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["4-Methoxy-4-methyl-2-pentanone","C7H14O2","107-70-0","C7H14O2","SG","SG-8521","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["4-Methoxy-4-methyl-2-pentanone","C7H14O2","107-70-0","C7H14O2","SG","SG-8521","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["4-Methyl-2-pentanol","C6H14O","108-11-2","C6H14O","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["4-Methyl-2-pentanol","C6H14O","108-11-2","C6H14O","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["4-Methyl-2-pentanol","C6H14O","108-11-2","C6H14O","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～10000ppm"]
["4-Methyl-2-pentanol","C6H14O","108-11-2","C6H14O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～10000ppm"]
["4-Methyl-2-pentanol","C6H14O","108-11-2","C6H14O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～10000ppm"]
["4-Methyl-2-pentanol","C6H14O","108-11-2","C6H14O","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～10000ppm"]
["4-Methyl-2-pentanol","C6H14O","108-11-2","C6H14O","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～10000ppm"]
["4-Methyl-2-pentanol","C6H14O","108-11-2","C6H14O","SG","SG-8521","Fixed","GD-A80V Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["4-Methyl-2-pentanol","C6H14O","108-11-2","C6H14O","SG","SG-8521","Fixed","GD-D58・GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["4-Methyl-2-pentanol","C6H14O","108-11-2","C6H14O","SG","SG-8521","Fixed","SD-1GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["4-Methyl-2-pentanol","C6H14O","108-11-2","C6H14O","SG","SG-8521","Fixed","SD-D58・GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["4-Methylmorpholine","C5H11NO","109-02-4","C5H11NO","SG","SG-8521","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["4-Methylmorpholine","C5H11NO","109-02-4","C5H11NO","SG","SG-8521","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["4-Methylmorpholine","C5H11NO","109-02-4","C5H11NO","SG","SG-8521","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["4-Methylmorpholine","C5H11NO","109-02-4","C5H11NO","SG","SG-8521","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["4-Vinylpyridine","C7H7N","100-43-6","C7H7N","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["4-Vinylpyridine","C7H7N","100-43-6","C7H7N","SG","SG-8562","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["4-Vinylpyridine","C7H7N","100-43-6","C7H7N","SG","SG-8562","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["4-Vinylpyridine","C7H7N","100-43-6","C7H7N","SG","SG-8562","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["4-Vinylpyridine","C7H7N","100-43-6","C7H7N","SG","SG-8562","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["Acetic Acid","C2H4O2","64-19-7","C2H4O2","ES","ESM-K233","Portable","SC-8000","0～30ppm"]
["Acetic Acid","C2H4O2","64-19-7","C2H4O2","ES","ESU-K233","Fixed","GD-70D Series","0～30ppm"]
["Acetic Acid","C2H4O2","64-19-7","C2H4O2","ES","ESU-K233","Fixed","TP-70D","0～30ppm"]
["Acetic Acid","C2H4O2","64-19-7","C2H4O2","ES","ESM-K233","Fixed","GD-K88Ai Series","0～30ppm"]
["Acetic Acid","C2H4O2","64-19-7","C2H4O2","ES","ESM-K233","Fixed","GD-K88Di Series","0～30ppm"]
["Acetic Acid","C2H4O2","64-19-7","C2H4O2","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Acetic Acid","C2H4O2","64-19-7","C2H4O2","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Acetic Acid","C2H4O2","64-19-7","C2H4O2","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～40000ppm"]
["Acetic Acid","C2H4O2","64-19-7","C2H4O2","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～40000ppm"]
["Acetic Acid","C2H4O2","64-19-7","C2H4O2","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～40000ppm"]
["Acetic Acid","C2H4O2","64-19-7","C2H4O2","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～40000ppm"]
["Acetic Acid","C2H4O2","64-19-7","C2H4O2","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～40000ppm"]
["Acetic Acid","C2H4O2","64-19-7","C2H4O2","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Acetic Acid","C2H4O2","64-19-7","C2H4O2","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Acetic Acid","C2H4O2","64-19-7","C2H4O2","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Acetic Acid","C2H4O2","64-19-7","C2H4O2","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Acetic Acid","C2H4O2","64-19-7","C2H4O2","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Acetic Acid","C2H4O2","64-19-7","C2H4O2","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Acetic Acid","C2H4O2","64-19-7","C2H4O2","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Acetic Acid","C2H4O2","64-19-7","C2H4O2","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["Acetic Acid","C2H4O2","64-19-7","C2H4O2","SG","SG-8521","Fixed","GD-A80V Series","0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Acetic Acid","C2H4O2","64-19-7","C2H4O2","SG","SG-8521","Fixed","GD-D58・GH Series","0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Acetic Acid","C2H4O2","64-19-7","C2H4O2","SG","SG-8521","Fixed","SD-1GH Series","0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Acetic Acid","C2H4O2","64-19-7","C2H4O2","SG","SG-8521","Fixed","SD-D58・GH Series","0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Acetic Acid","C2H4O2","64-19-7","C2H4O2","SG","SG-8562","Fixed","GD-A80V Series","0～300ppm"]
["Acetic Acid","C2H4O2","64-19-7","C2H4O2","SG","SG-8562","Fixed","GD-D58・GH Series","0～300ppm"]
["Acetic Acid","C2H4O2","64-19-7","C2H4O2","SG","SG-8562","Fixed","SD-1GH Series","0～300ppm"]
["Acetic Acid","C2H4O2","64-19-7","C2H4O2","SG","SG-8562","Fixed","SD-D58・GH Series","0～300ppm"]
["Acetic Acid","C2H4O2","64-19-7","C2H4O2","SG","SG-8562","Fixed","GD-A80V Series","0～300ppm","Standard sensor: SG-8521"]
["Acetic Acid","C2H4O2","64-19-7","C2H4O2","SG","SG-8562","Fixed","GD-D58・GH Series","0～300ppm","Standard sensor: SG-8521"]
["Acetic Acid","C2H4O2","64-19-7","C2H4O2","SG","SG-8562","Fixed","SD-1GH Series","0～300ppm","Standard sensor: SG-8521"]
["Acetic Acid","C2H4O2","64-19-7","C2H4O2","SG","SG-8562","Fixed","SD-D58・GH Series","0～300ppm","Standard sensor: SG-8521"]
["Acetic Aldehyde","ALD","75-07-0","C2H4O","HW","NC-6215","Portable","GP-1000(Specified cal.gas)","0～100%LEL"]
["Acetic Aldehyde","ALD","75-07-0","C2H4O","SG","SGU-8521","Fixed","GD-70D Series","0～100ppm"]
["Acetic Aldehyde","ALD","75-07-0","C2H4O","SG","SGU-8521","Fixed","TP-70D","0～100ppm"]
["Acetic Aldehyde","ALD","75-07-0","C2H4O","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Acetic Aldehyde","ALD","75-07-0","C2H4O","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Acetic Aldehyde","ALD","75-07-0","C2H4O","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL～40000ppm"]
["Acetic Aldehyde","ALD","75-07-0","C2H4O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL～40000ppm"]
["Acetic Aldehyde","ALD","75-07-0","C2H4O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL～40000ppm"]
["Acetic Aldehyde","ALD","75-07-0","C2H4O","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL～40000ppm"]
["Acetic Aldehyde","ALD","75-07-0","C2H4O","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL～40000ppm"]
["Acetic Aldehyde","ALD","75-07-0","C2H4O","SG","SG-8521","Fixed","GD-A80V Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Acetic Aldehyde","ALD","75-07-0","C2H4O","SG","SG-8521","Fixed","GD-D58・GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Acetic Aldehyde","ALD","75-07-0","C2H4O","SG","SG-8521","Fixed","SD-1GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Acetic Aldehyde","ALD","75-07-0","C2H4O","SG","SG-8521","Fixed","SD-D58・GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Acetic anhydride","C4H6O3","108-24-7","C4H6O3","SG","SG-8521","Fixed","GD-A80V Series","0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Acetic anhydride","C4H6O3","108-24-7","C4H6O3","SG","SG-8521","Fixed","GD-D58・GH Series","0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Acetic anhydride","C4H6O3","108-24-7","C4H6O3","SG","SG-8521","Fixed","SD-1GH Series","0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Acetic anhydride","C4H6O3","108-24-7","C4H6O3","SG","SG-8521","Fixed","SD-D58・GH Series","0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Acetone","C3H6O","67-64-1","C3H6O","HW","NC-6215","Portable","GP-1000(HC/CH4)","0～100%LEL"]
["Acetone","C3H6O","67-64-1","C3H6O","HW","NC-6307","Portable","NC-1000(HC/CH4)","0～10000ppm"]
["Acetone","C3H6O","67-64-1","C3H6O","SH","SH-8662","Portable","SP-220(TYPE SC)","0～10ppm"]
["Acetone","C3H6O","67-64-1","C3H6O","SG","SGU-8511","Fixed","GD-70D Series","0～2000ppm"]
["Acetone","C3H6O","67-64-1","C3H6O","SG","SGU-8511","Fixed","TP-70D","0～2000ppm"]
["Acetone","C3H6O","67-64-1","C3H6O","SG","SGU-8521","Fixed","GD-70D Series","0～100ppm"]
["Acetone","C3H6O","67-64-1","C3H6O","SG","SGU-8521","Fixed","TP-70D","0～100ppm"]
["Acetone","C3H6O","67-64-1","C3H6O","HW","NCU-6211","Fixed","GD-70D Series","0～100%LEL","Confirm that GD-70D is non-explosion proof"]
["Acetone","C3H6O","67-64-1","C3H6O","HW","NCU-6211","Fixed","TP-70D","0～100%LEL","Confirm that GD-70D is non-explosion proof"]
["Acetone","C3H6O","67-64-1","C3H6O","RI","DE-3315-1","Fixed","SD-1RI Series","0～100%LEL"]
["Acetone","C3H6O","67-64-1","C3H6O","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Acetone","C3H6O","67-64-1","C3H6O","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Acetone","C3H6O","67-64-1","C3H6O","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～21500ppm"]
["Acetone","C3H6O","67-64-1","C3H6O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～21500ppm"]
["Acetone","C3H6O","67-64-1","C3H6O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～21500ppm"]
["Acetone","C3H6O","67-64-1","C3H6O","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～21500ppm"]
["Acetone","C3H6O","67-64-1","C3H6O","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～21500ppm"]
["Acetone","C3H6O","67-64-1","C3H6O","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Acetone","C3H6O","67-64-1","C3H6O","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Acetone","C3H6O","67-64-1","C3H6O","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Acetone","C3H6O","67-64-1","C3H6O","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Acetone","C3H6O","67-64-1","C3H6O","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Acetone","C3H6O","67-64-1","C3H6O","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Acetone","C3H6O","67-64-1","C3H6O","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Acetone","C3H6O","67-64-1","C3H6O","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["Acetone","C3H6O","67-64-1","C3H6O","SG","SG-8511","Fixed","GD-A80V Series","0～2000ppm/0～3000ppm/0～5000ppm/0～10000ppm"]
["Acetone","C3H6O","67-64-1","C3H6O","SG","SG-8511","Fixed","GD-D58・GH Series","0～2000ppm/0～3000ppm/0～5000ppm/0～10000ppm"]
["Acetone","C3H6O","67-64-1","C3H6O","SG","SG-8511","Fixed","SD-1GH Series","0～2000ppm/0～3000ppm/0～5000ppm/0～10000ppm"]
["Acetone","C3H6O","67-64-1","C3H6O","SG","SG-8511","Fixed","SD-D58・GH Series","0～2000ppm/0～3000ppm/0～5000ppm/0～10000ppm"]
["Acetone","C3H6O","67-64-1","C3H6O","SG","SG-8521","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Acetone","C3H6O","67-64-1","C3H6O","SG","SG-8521","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Acetone","C3H6O","67-64-1","C3H6O","SG","SG-8521","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Acetone","C3H6O","67-64-1","C3H6O","SG","SG-8521","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Acetone cyanohydrin","ACH","75-86-5","C4H7NO","SG","SG-8521","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Acetone cyanohydrin","ACH","75-86-5","C4H7NO","SG","SG-8521","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Acetone cyanohydrin","ACH","75-86-5","C4H7NO","SG","SG-8521","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Acetone cyanohydrin","ACH","75-86-5","C4H7NO","SG","SG-8521","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Acetonitrile","CH3CN","75-05-8","C2H3N","HW","NC-6215","Portable","GP-1000(Specified cal.gas)","0～100%LEL"]
["Acetonitrile","CH3CN","75-05-8","C2H3N","SG","SGU-8521","Fixed","GD-70D Series","0～2000ppm"]
["Acetonitrile","CH3CN","75-05-8","C2H3N","SG","SGU-8521","Fixed","TP-70D","0～2000ppm"]
["Acetonitrile","CH3CN","75-05-8","C2H3N","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Acetonitrile","CH3CN","75-05-8","C2H3N","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Acetonitrile","CH3CN","75-05-8","C2H3N","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～30000ppm"]
["Acetonitrile","CH3CN","75-05-8","C2H3N","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～30000ppm"]
["Acetonitrile","CH3CN","75-05-8","C2H3N","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～30000ppm"]
["Acetonitrile","CH3CN","75-05-8","C2H3N","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～30000ppm"]
["Acetonitrile","CH3CN","75-05-8","C2H3N","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～30000ppm"]
["Acetonitrile","CH3CN","75-05-8","C2H3N","SG","SG-8511","Fixed","GD-A80V Series","0～500ppm/0～1000ppm"]
["Acetonitrile","CH3CN","75-05-8","C2H3N","SG","SG-8511","Fixed","GD-D58・GH Series","0～500ppm/0～1000ppm"]
["Acetonitrile","CH3CN","75-05-8","C2H3N","SG","SG-8511","Fixed","SD-1GH Series","0～500ppm/0～1000ppm"]
["Acetonitrile","CH3CN","75-05-8","C2H3N","SG","SG-8511","Fixed","SD-D58・GH Series","0～500ppm/0～1000ppm"]
["Acetonitrile","CH3CN","75-05-8","C2H3N","SG","SG-8521","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Acetonitrile","CH3CN","75-05-8","C2H3N","SG","SG-8521","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Acetonitrile","CH3CN","75-05-8","C2H3N","SG","SG-8521","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Acetonitrile","CH3CN","75-05-8","C2H3N","SG","SG-8521","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Acetylene","C2H2","74-86-2","C2H2","HW","NC-6215","Portable","GX-8000","0～100%LEL"]
["Acetylene","C2H2","74-86-2","C2H2","HW","NC-6215","Portable","GX-8000(TYPE LEL)","0～100%LEL"]
["Acetylene","C2H2","74-86-2","C2H2","HW","NC-6215","Portable","GP-1000(HC/CH4)","0～100%LEL"]
["Acetylene","C2H2","74-86-2","C2H2","HW","NC-6307","Portable","NC-1000(HC/CH4)","0～10000ppm"]
["Acetylene","C2H2","74-86-2","C2H2","SH","SH-8661","Portable","SP-220(TYPE H2)","0～10000ppm"]
["Acetylene","C2H2","74-86-2","C2H2","SG","SGU-8521","Fixed","GD-70D Series","0～2000ppm"]
["Acetylene","C2H2","74-86-2","C2H2","SG","SGU-8521","Fixed","TP-70D","0～2000ppm"]
["Acetylene","C2H2","74-86-2","C2H2","SG","SGU-8521","Fixed","GD-70D Series","0～5000ppm"]
["Acetylene","C2H2","74-86-2","C2H2","SG","SGU-8521","Fixed","TP-70D","0～5000ppm"]
["Acetylene","C2H2","74-86-2","C2H2","HW","NCU-6211","Fixed","GD-70D Series","0～100%LEL","Confirm that GD-70D is non-explosion proof"]
["Acetylene","C2H2","74-86-2","C2H2","HW","NCU-6211","Fixed","TP-70D","0～100%LEL","Confirm that GD-70D is non-explosion proof"]
["Acetylene","C2H2","74-86-2","C2H2","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Acetylene","C2H2","74-86-2","C2H2","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～15000ppm"]
["Acetylene","C2H2","74-86-2","C2H2","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～15000ppm"]
["Acetylene","C2H2","74-86-2","C2H2","HW","HW-6213/NC-6213","Fixed","GD-A80 Series","0～100%LEL/0～15000ppm"]
["Acetylene","C2H2","74-86-2","C2H2","HW","HW-6215","Fixed","GD-A80 Series","0～100%LEL"]
["Acetylene","C2H2","74-86-2","C2H2","HW","HW-6239","Fixed","GD-A80-70 Series","0～100%LEL"]
["Acetylene","C2H2","74-86-2","C2H2","HW","HW-6239","Fixed","SD-1(TYPE GP) Series","0～100%LEL"]
["Acetylene","C2H2","74-86-2","C2H2","HW","HW-6239/NC-6239","Fixed","GD-A80 Series","0～100%LEL/0～15000ppm"]
["Acetylene","C2H2","74-86-2","C2H2","HW","HW-6239/NC-6239","Fixed","SD-1(TYPE NC) Series","0～100%LEL/0～15000ppm"]
["Acetylene","C2H2","74-86-2","C2H2","HW","NC-6240A","Fixed","GD-A80 Series","0～100%LEL/0～15000ppm"]
["Acetylene","C2H2","74-86-2","C2H2","HW","NC-6240A","Fixed","SD-1(TYPE NC) Series","0～100%LEL/0～15000ppm"]
["Acetylene","C2H2","74-86-2","C2H2","HW","NC-6245","Fixed","GD-A80 Series","0～100%LEL"]
["Acetylene","C2H2","74-86-2","C2H2","HW","NC-6245","Fixed","SD-1(TYPE NC) Series","0～100%LEL"]
["Acetylene","C2H2","74-86-2","C2H2","HW","NC-6250","Fixed","GD-A80 Series","0～100%LEL/0～15000ppm"]
["Acetylene","C2H2","74-86-2","C2H2","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Acetylene","C2H2","74-86-2","C2H2","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Acetylene","C2H2","74-86-2","C2H2","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Acetylene","C2H2","74-86-2","C2H2","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Acetylene","C2H2","74-86-2","C2H2","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Acetylene","C2H2","74-86-2","C2H2","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Acetylene","C2H2","74-86-2","C2H2","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Acetylene","C2H2","74-86-2","C2H2","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["Acetylene","C2H2","74-86-2","C2H2","SG","SG-8521","Fixed","GD-A80V Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Acetylene","C2H2","74-86-2","C2H2","SG","SG-8521","Fixed","SD-1GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Acrolein","C3H4O","107-02-8","C3H4O","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Acrolein","C3H4O","107-02-8","C3H4O","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Acrolein","C3H4O","107-02-8","C3H4O","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～28000ppm"]
["Acrolein","C3H4O","107-02-8","C3H4O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～28000ppm"]
["Acrolein","C3H4O","107-02-8","C3H4O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～28000ppm"]
["Acrolein","C3H4O","107-02-8","C3H4O","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～28000ppm"]
["Acrolein","C3H4O","107-02-8","C3H4O","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～28000ppm"]
["Acrolein","C3H4O","107-02-8","C3H4O","SG","SG-8521","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["Acrolein","C3H4O","107-02-8","C3H4O","SG","SG-8521","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["Acrolein","C3H4O","107-02-8","C3H4O","SG","SG-8521","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["Acrolein","C3H4O","107-02-8","C3H4O","SG","SG-8521","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["Acrylic acid","C3H4O2","79-10-7","C3H4O2","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Acrylic acid","C3H4O2","79-10-7","C3H4O2","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Acrylic acid","C3H4O2","79-10-7","C3H4O2","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～30000ppm"]
["Acrylic acid","C3H4O2","79-10-7","C3H4O2","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～30000ppm"]
["Acrylic acid","C3H4O2","79-10-7","C3H4O2","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～30000ppm"]
["Acrylic acid","C3H4O2","79-10-7","C3H4O2","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～30000ppm"]
["Acrylic acid","C3H4O2","79-10-7","C3H4O2","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～30000ppm"]
["Acrylic acid","C3H4O2","79-10-7","C3H4O2","SG","SG-8521","Fixed","GD-A80V Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Acrylic acid","C3H4O2","79-10-7","C3H4O2","SG","SG-8521","Fixed","GD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Acrylic acid","C3H4O2","79-10-7","C3H4O2","SG","SG-8521","Fixed","SD-1GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Acrylic acid","C3H4O2","79-10-7","C3H4O2","SG","SG-8521","Fixed","SD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Acrylonitrile","C3H3N","107-13-1","C3H3N","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Acrylonitrile","C3H3N","107-13-1","C3H3N","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Acrylonitrile","C3H3N","107-13-1","C3H3N","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～28000ppm"]
["Acrylonitrile","C3H3N","107-13-1","C3H3N","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～28000ppm"]
["Acrylonitrile","C3H3N","107-13-1","C3H3N","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～28000ppm"]
["Acrylonitrile","C3H3N","107-13-1","C3H3N","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～28000ppm"]
["Acrylonitrile","C3H3N","107-13-1","C3H3N","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～28000ppm"]
["Acrylonitrile","C3H3N","107-13-1","C3H3N","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Acrylonitrile","C3H3N","107-13-1","C3H3N","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Acrylonitrile","C3H3N","107-13-1","C3H3N","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Acrylonitrile","C3H3N","107-13-1","C3H3N","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Acrylonitrile","C3H3N","107-13-1","C3H3N","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Acrylonitrile","C3H3N","107-13-1","C3H3N","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Acrylonitrile","C3H3N","107-13-1","C3H3N","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Acrylonitrile","C3H3N","107-13-1","C3H3N","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["Acrylonitrile","C3H3N","107-13-1","C3H3N","SG","SG-8511","Fixed","GD-A80V Series","★0～2000ppm/★0～3000ppm/★0～5000ppm/0～10000ppm","★Range easily affected by environmental conditions and other"]
["Acrylonitrile","C3H3N","107-13-1","C3H3N","SG","SG-8511","Fixed","GD-D58・GH Series","★0～2000ppm/★0～3000ppm/★0～5000ppm/0～10000ppm","★Range easily affected by environmental conditions and other"]
["Acrylonitrile","C3H3N","107-13-1","C3H3N","SG","SG-8511","Fixed","SD-1GH Series","★0～2000ppm/★0～3000ppm/★0～5000ppm/0～10000ppm","★Range easily affected by environmental conditions and other"]
["Acrylonitrile","C3H3N","107-13-1","C3H3N","SG","SG-8511","Fixed","SD-D58・GH Series","★0～2000ppm/★0～3000ppm/★0～5000ppm/0～10000ppm","★Range easily affected by environmental conditions and other"]
["Acrylonitrile","C3H3N","107-13-1","C3H3N","SG","SG-8521","Fixed","GD-A80V Series","★0～100ppm/★0～150ppm/★0～200ppm/★0～300ppm/0～500ppm/0～1000ppm/0～2000ppm","★Range easily affected by environmental conditions and other"]
["Acrylonitrile","C3H3N","107-13-1","C3H3N","SG","SG-8521","Fixed","GD-D58・GH Series","★0～100ppm/★0～150ppm/★0～200ppm/★0～300ppm/0～500ppm/0～1000ppm/0～2000ppm","★Range easily affected by environmental conditions and other"]
["Acrylonitrile","C3H3N","107-13-1","C3H3N","SG","SG-8521","Fixed","SD-1GH Series","★0～100ppm/★0～150ppm/★0～200ppm/★0～300ppm/0～500ppm/0～1000ppm/0～2000ppm","★Range easily affected by environmental conditions and other"]
["Acrylonitrile","C3H3N","107-13-1","C3H3N","SG","SG-8521","Fixed","SD-D58・GH Series","★0～100ppm/★0～150ppm/★0～200ppm/★0～300ppm/0～500ppm/0～1000ppm/0～2000ppm","★Range easily affected by environmental conditions and other"]
["Aｌlyl chloride","C3H5CL","107-05-1","C3H5CL","SG","SG-8523","Fixed","GD-A80V Series","0～20ppm/0～30ppm/0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["Aｌlyl chloride","C3H5CL","107-05-1","C3H5CL","SG","SG-8523","Fixed","GD-D58・GH Series","0～20ppm/0～30ppm/0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["Aｌlyl chloride","C3H5CL","107-05-1","C3H5CL","SG","SG-8523","Fixed","SD-1GH Series","0～20ppm/0～30ppm/0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["Aｌlyl chloride","C3H5CL","107-05-1","C3H5CL","SG","SG-8523","Fixed","SD-D58・GH Series","0～20ppm/0～30ppm/0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["Allyl glycidyl ether","AGE","106-92-3","C6H10O2","SG","SG-8521","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Allyl glycidyl ether","AGE","106-92-3","C6H10O2","SG","SG-8521","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Allyl glycidyl ether","AGE","106-92-3","C6H10O2","SG","SG-8521","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Allyl glycidyl ether","AGE","106-92-3","C6H10O2","SG","SG-8521","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Allyl Methacrylate","AMA","96-05-9","C7H10O2","SG","SG-8521","Fixed","GD-A80V Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm"]
["Allyl Methacrylate","AMA","96-05-9","C7H10O2","SG","SG-8521","Fixed","GD-D58・GH Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm"]
["Allyl Methacrylate","AMA","96-05-9","C7H10O2","SG","SG-8521","Fixed","SD-1GH Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm"]
["Allyl Methacrylate","AMA","96-05-9","C7H10O2","SG","SG-8521","Fixed","SD-D58・GH Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm"]
["Allylamine","C3H7N","107-11-9","C3H7N","SG","SG-8562","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Allylamine","C3H7N","107-11-9","C3H7N","SG","SG-8562","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Allylamine","C3H7N","107-11-9","C3H7N","SG","SG-8562","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Allylamine","C3H7N","107-11-9","C3H7N","SG","SG-8562","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Ammonia","NH3","7664-41-7","NH3","SH","SH-8662","Portable","SP-220(TYPE SC)","0～10ppm"]
["Ammonia","NH3","7664-41-7","NH3","ES","ESS-B332","Portable","GX-6000","0～400ppm"]
["Ammonia","NH3","7664-41-7","NH3","ES","ESM-01R-D","Portable","SC-01","0～75ppm"]
["Ammonia","NH3","7664-41-7","NH3","ES","ESM-23R","Portable","SC-8000","0～75ppm"]
["Ammonia","NH3","7664-41-7","NH3","ES","ESU-23R","Fixed","GD-70D Series","0～75ppm"]
["Ammonia","NH3","7664-41-7","NH3","ES","ESU-23R","Fixed","TP-70D","0～75ppm"]
["Ammonia","NH3","7664-41-7","NH3","ES","ESU-23R-A","Fixed","GD-70D Series","0～150ppm"]
["Ammonia","NH3","7664-41-7","NH3","ES","ESU-23R-A","Fixed","TP-70D","0～150ppm"]
["Ammonia","NH3","7664-41-7","NH3","ES","ESU-23RH","Fixed","GD-70D Series","0～75ppm","Sensor for high humidity /Range： higher than 70%RH"]
["Ammonia","NH3","7664-41-7","NH3","ES","ESU-23RH","Fixed","TP-70D","0～75ppm","Sensor for high humidity /Range： higher than 70%RH"]
["Ammonia","NH3","7664-41-7","NH3","ES","ESU-23RL","Fixed","GD-70D Series","0～75ppm","Sensor for low humidity /Range： 3～70%RH"]
["Ammonia","NH3","7664-41-7","NH3","ES","ESU-23RL","Fixed","TP-70D","0～75ppm","Sensor for low humidity /Range： 3～70%RH"]
["Ammonia","NH3","7664-41-7","NH3","ES","ESU-23RVM","Fixed","GD-70D Series","0～10ppm","For low concentration measurement (NH3)"]
["Ammonia","NH3","7664-41-7","NH3","ES","ESU-23RVM","Fixed","TP-70D","0～10ppm","For low concentration measurement (NH3)"]
["Ammonia","NH3","7664-41-7","NH3","ES","ESM-23R","Fixed","GD-K88Ai Series","0～75ppm"]
["Ammonia","NH3","7664-41-7","NH3","ES","ESM-23R","Fixed","GD-K88Di Series","0～75ppm"]
["Ammonia","NH3","7664-41-7","NH3","ES","ESM-23RH","Fixed","GD-K88Ai Series","0～75ppm"]
["Ammonia","NH3","7664-41-7","NH3","ES","ESM-23RH","Fixed","GD-K88Di Series","0～75ppm"]
["Ammonia","NH3","7664-41-7","NH3","ES","ESM-23RL","Fixed","GD-K88Ai Series","0～75ppm"]
["Ammonia","NH3","7664-41-7","NH3","ES","ESM-23RL","Fixed","GD-K88Di Series","0～75ppm"]
["Ammonia","NH3","7664-41-7","NH3","ES","ESM-23R-A","Fixed","GD-K88Ai Series","0～150ppm"]
["Ammonia","NH3","7664-41-7","NH3","ES","ESM-23R-A","Fixed","GD-K88Di Series","0～150ppm"]
["Ammonia","NH3","7664-41-7","NH3","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Ammonia","NH3","7664-41-7","NH3","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Ammonia","NH3","7664-41-7","NH3","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL～150000ppm"]
["Ammonia","NH3","7664-41-7","NH3","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL～150000ppm"]
["Ammonia","NH3","7664-41-7","NH3","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL～150000ppm"]
["Ammonia","NH3","7664-41-7","NH3","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL～150000ppm"]
["Ammonia","NH3","7664-41-7","NH3","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL～150000ppm"]
["Ammonia","NH3","7664-41-7","NH3","SG","SG-8511","Fixed","GD-A80V Series","0～3000ppm/0～5000ppm/0～10000ppm"]
["Ammonia","NH3","7664-41-7","NH3","SG","SG-8511","Fixed","GD-D58・GH Series","0～3000ppm/0～5000ppm/0～10000ppm"]
["Ammonia","NH3","7664-41-7","NH3","SG","SG-8511","Fixed","SD-1GH Series","0～3000ppm/0～5000ppm/0～10000ppm"]
["Ammonia","NH3","7664-41-7","NH3","SG","SG-8511","Fixed","SD-D58・GH Series","0～3000ppm/0～5000ppm/0～10000ppm"]
["Ammonia","NH3","7664-41-7","NH3","SG","SG-8562","Fixed","GD-A80V Series","★0～75ppm/★0～100ppm/★0～150ppm/★0～200ppm/★0～300ppm/0～400ppm/0～500ppm/0～1000ppm","★Range easily affected by environmental conditions and other"]
["Ammonia","NH3","7664-41-7","NH3","SG","SG-8562","Fixed","GD-D58・GH Series","★0～75ppm/★0～100ppm/★0～150ppm/★0～200ppm/★0～300ppm/0～400ppm/0～500ppm/0～1000ppm","★Range easily affected by environmental conditions and other"]
["Ammonia","NH3","7664-41-7","NH3","SG","SG-8562","Fixed","SD-1GH Series","★0～75ppm/★0～100ppm/★0～150ppm/★0～200ppm/★0～300ppm/0～400ppm/0～500ppm/0～1000ppm","★Range easily affected by environmental conditions and other"]
["Ammonia","NH3","7664-41-7","NH3","SG","SG-8562","Fixed","SD-D58・GH Series","★0～75ppm/★0～100ppm/★0～150ppm/★0～200ppm/★0～300ppm/0～400ppm/0～500ppm/0～1000ppm","★Range easily affected by environmental conditions and other"]
["Aniline","C6H5NH2","62-53-3","C6H7N","SG","SG-8562","Fixed","GD-A80V Series","0～200ppm/0～300ppm"]
["Aniline","C6H5NH2","62-53-3","C6H7N","SG","SG-8562","Fixed","GD-D58・GH Series","0～200ppm/0～300ppm"]
["Aniline","C6H5NH2","62-53-3","C6H7N","SG","SG-8562","Fixed","SD-1GH Series","0～200ppm/0～300ppm"]
["Aniline","C6H5NH2","62-53-3","C6H7N","SG","SG-8562","Fixed","SD-D58・GH Series","0～200ppm/0～300ppm"]
["Anisole","ANISOLE","100-66-3","C7H8O","HW","NC-6211","Fixed","GD-A80 Series","～100%LEL/～3000ppm"]
["Anisole","ANISOLE","100-66-3","C7H8O","HW","NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～3000ppm"]
["Anisole","ANISOLE","100-66-3","C7H8O","HW","NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～3000ppm"]
["Anisole","ANISOLE","100-66-3","C7H8O","HW","NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～3000ppm"]
["Anisole","ANISOLE","100-66-3","C7H8O","HW","NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～3000ppm"]
["Anisole","ANISOLE","100-66-3","C7H8O","SG","SG-8521","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Anisole","ANISOLE","100-66-3","C7H8O","SG","SG-8521","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Anisole","ANISOLE","100-66-3","C7H8O","SG","SG-8521","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Anisole","ANISOLE","100-66-3","C7H8O","SG","SG-8521","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Argon","Ar","7440-37-1","Ar","TE","TE-7515W","Portable","NP-1000(CH4)","0～100vol%"]
["Arsine","AsH3","7784-42-1","AsH3","SH","SH-8662","Portable","SP-220(TYPE SC)","0～0.2ppm"]
["Arsine","AsH3","7784-42-1","AsH3","ES","ESM-23AHS-N","Portable","SC-8000","0～0.2ppm"]
["Arsine","AsH3","7784-42-1","AsH3","ES","ESM-23AH","Portable","SC-8000","0～1ppm"]
["Arsine","AsH3","7784-42-1","AsH3","ES","ESM-23AP","Portable","SC-8000","0～0.2ppm"]
["Arsine","AsH3","7784-42-1","AsH3","ES","ESU-23AHS","Fixed","GD-70D Series","0～0.2ppm"]
["Arsine","AsH3","7784-42-1","AsH3","ES","ESU-23AHS","Fixed","TP-70D","0～0.2ppm"]
["Arsine","AsH3","7784-42-1","AsH3","ES","ESU-23AHS-N","Fixed","GD-70D Series","0～0.2ppm","NOx Updated against interference gas"]
["Arsine","AsH3","7784-42-1","AsH3","ES","ESU-23AHS-N","Fixed","TP-70D","0～0.2ppm","NOx Updated against interference gas"]
["Arsine","AsH3","7784-42-1","AsH3","ES","ESU-23AP","Fixed","GD-70D Series","0～0.2ppm"]
["Arsine","AsH3","7784-42-1","AsH3","ES","ESU-23AP","Fixed","TP-70D","0～0.2ppm"]
["Arsine","AsH3","7784-42-1","AsH3","ES","ESU-C23F","Fixed","GD-70D Series","0～0.2ppm"]
["Arsine","AsH3","7784-42-1","AsH3","ES","ESU-C23F","Fixed","TP-70D","0～0.2ppm"]
["Arsine","AsH3","7784-42-1","AsH3","ES","ESU-C23F-S","Fixed","GD-70D Series","0～50ppb","Capable to set alarm point 10ppb/With CF-8364TP（for dehumidification）"]
["Arsine","AsH3","7784-42-1","AsH3","ES","ESU-C23F-S","Fixed","TP-70D","0～50ppb","Capable to set alarm point 10ppb/With CF-8364TP（for dehumidification）"]
["Arsine","AsH3","7784-42-1","AsH3","ES","ESM-23AH","Fixed","GD-K88Ai Series","0～1ppm"]
["Arsine","AsH3","7784-42-1","AsH3","ES","ESM-23AH","Fixed","GD-K88Di Series","0～1ppm"]
["Arsine","AsH3","7784-42-1","AsH3","ES","ESM-23AHS","Fixed","GD-K88Ai Series","0～0.2ppm"]
["Arsine","AsH3","7784-42-1","AsH3","ES","ESM-23AHS","Fixed","GD-K88Di Series","0～0.2ppm"]
["Arsine","AsH3","7784-42-1","AsH3","ES","ESM-23AHS-N","Fixed","GD-K88Ai Series","0～0.2ppm"]
["Arsine","AsH3","7784-42-1","AsH3","ES","ESM-23AHS-N","Fixed","GD-K88Di Series","0～0.2ppm"]
["Arsine","AsH3","7784-42-1","AsH3","ES","ESM-23AP","Fixed","GD-K88Ai Series","0～0.2ppm"]
["Arsine","AsH3","7784-42-1","AsH3","ES","ESM-23AP","Fixed","GD-K88Di Series","0～0.2ppm"]
["Arsine","AsH3","7784-42-1","AsH3","ES","ESM-23AY","Fixed","GD-K88Ai Series","0～0.2ppm"]
["Arsine","AsH3","7784-42-1","AsH3","ES","ESM-23AY","Fixed","GD-K88Di Series","0～0.2ppm"]
["Benzene","C6H6","71-43-2","C6H6","HW","NC-6215","Portable","GP-1000(HC/CH4)","0～100%LEL"]
["Benzene","C6H6","71-43-2","C6H6","HW","NC-6307","Portable","NC-1000(HC/CH4)","0～10000ppm"]
["Benzene","C6H6","71-43-2","C6H6","SH","SH-8662","Portable","SP-220(TYPE SC)","0～10ppm"]
["Benzene","C6H6","71-43-2","C6H6","RI","DE-3315-1","Fixed","SD-1RI Series","0～100%LEL"]
["Benzene","C6H6","71-43-2","C6H6","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Benzene","C6H6","71-43-2","C6H6","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Benzene","C6H6","71-43-2","C6H6","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～12000ppm"]
["Benzene","C6H6","71-43-2","C6H6","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～12000ppm"]
["Benzene","C6H6","71-43-2","C6H6","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～12000ppm"]
["Benzene","C6H6","71-43-2","C6H6","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～12000ppm"]
["Benzene","C6H6","71-43-2","C6H6","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～12000ppm"]
["Benzene","C6H6","71-43-2","C6H6","HW","NC-6240A","Fixed","GD-A80 Series","0～100%LEL/0～12000ppm"]
["Benzene","C6H6","71-43-2","C6H6","HW","NC-6240A","Fixed","GD-D58(TYPE NC) Series","0～100%LEL/0～12000ppm"]
["Benzene","C6H6","71-43-2","C6H6","HW","NC-6240A","Fixed","SD-1(TYPE NC) Series","0～100%LEL/0～12000ppm"]
["Benzene","C6H6","71-43-2","C6H6","HW","NC-6240A","Fixed","SD-D58(TYPE NC) Series","0～100%LEL/0～12000ppm"]
["Benzene","C6H6","71-43-2","C6H6","HW","NC-6245","Fixed","GD-A80 Series","0～100%LEL"]
["Benzene","C6H6","71-43-2","C6H6","HW","NC-6245","Fixed","GD-D58(TYPE NC) Series","0～100%LEL"]
["Benzene","C6H6","71-43-2","C6H6","HW","NC-6245","Fixed","SD-1(TYPE NC) Series","0～100%LEL"]
["Benzene","C6H6","71-43-2","C6H6","HW","NC-6245","Fixed","SD-D58(TYPE NC) Series","0～100%LEL"]
["Benzene","C6H6","71-43-2","C6H6","SG","SG-8521","Fixed","GD-A80V Series","0～30ppm/0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Benzene","C6H6","71-43-2","C6H6","SG","SG-8521","Fixed","GD-D58・GH Series","0～30ppm/0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Benzene","C6H6","71-43-2","C6H6","SG","SG-8521","Fixed","SD-1GH Series","0～30ppm/0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Benzene","C6H6","71-43-2","C6H6","SG","SG-8521","Fixed","SD-D58・GH Series","0～30ppm/0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Benzene","C6H6","71-43-2","C6H6","SG","SG-8521","Fixed","GD-A80V Series","0～75ppm/0～150ppm"]
["Benzene","C6H6","71-43-2","C6H6","SG","SG-8521","Fixed","GD-D58・GH Series","0～75ppm/0～150ppm"]
["Benzene","C6H6","71-43-2","C6H6","SG","SG-8521","Fixed","SD-1GH Series","0～75ppm/0～150ppm"]
["Benzene","C6H6","71-43-2","C6H6","SG","SG-8521","Fixed","SD-D58・GH Series","0～75ppm/0～150ppm"]
["Benzyl Alcohol","Benz-ol","100-51-6","C7H8O","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Benzyl Alcohol","Benz-ol","100-51-6","C7H8O","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Benzyl Alcohol","Benz-ol","100-51-6","C7H8O","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Benzyl Alcohol","Benz-ol","100-51-6","C7H8O","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Benzyl Alcohol","Benz-ol","100-51-6","C7H8O","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Benzyl Alcohol","Benz-ol","100-51-6","C7H8O","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Benzyl Alcohol","Benz-ol","100-51-6","C7H8O","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Bis(tert-butylamino)silane","BTBAS","186598-40-3","C8H22N2Si","ES","ESM-23RVM","Portable","SC-8000","0～15ppm"]
["Bis(tert-butylamino)silane","BTBAS","186598-40-3","C8H22N2Si","ES","ESU-23RV","Fixed","GD-70D Series","0～15ppm"]
["Bis(tert-butylamino)silane","BTBAS","186598-40-3","C8H22N2Si","ES","ESU-23RV","Fixed","TP-70D","0～15ppm"]
["Bis(tert-butylamino)silane","BTBAS","186598-40-3","C8H22N2Si","ES","ESU-23RVM","Fixed","GD-70D Series","0～15ppm","Updated against electrolyte reduction"]
["Bis(tert-butylamino)silane","BTBAS","186598-40-3","C8H22N2Si","ES","ESU-23RVM","Fixed","TP-70D","0～15ppm","Updated against electrolyte reduction"]
["Bis(tert-butylamino)silane","BTBAS","186598-40-3","C8H22N2Si","ES","ESM-23RV","Fixed","GD-K88Ai Series","0～15ppm"]
["Bis(tert-butylamino)silane","BTBAS","186598-40-3","C8H22N2Si","ES","ESM-23RV","Fixed","GD-K88Di Series","0～15ppm"]
["Bis(tert-butylamino)silane","BTBAS","186598-40-3","C8H22N2Si","ES","ESM-23RVM","Fixed","GD-K88Ai Series","0～15ppm","Updated against electrolyte reduction"]
["Bis(tert-butylamino)silane","BTBAS","186598-40-3","C8H22N2Si","ES","ESM-23RVM","Fixed","GD-K88Di Series","0～15ppm","Updated against electrolyte reduction"]
["Bromine","Br2","7726-95-6","Br2","ES","ESM-K233","Portable","SC-8000","0～1ppm"]
["Bromine","Br2","7726-95-6","Br2","ES","ESU-K233","Fixed","GD-70D Series","0～1ppm"]
["Bromine","Br2","7726-95-6","Br2","ES","ESU-K233","Fixed","TP-70D","0～1ppm"]
["Bromine","Br2","7726-95-6","Br2","ES","ESM-K233","Fixed","GD-K88Ai Series","0～1ppm"]
["Bromine","Br2","7726-95-6","Br2","ES","ESM-K233","Fixed","GD-K88Di Series","0～1ppm"]
["Butyl Methacrylate","n-BMA","97-88-1","C8H14O2","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～50%LEL/～10000ppm"]
["Butyl Methacrylate","n-BMA","97-88-1","C8H14O2","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～50%LEL/～10000ppm"]
["Butyl Methacrylate","n-BMA","97-88-1","C8H14O2","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～50%LEL/～10000ppm"]
["Butyl Methacrylate","n-BMA","97-88-1","C8H14O2","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～50%LEL/～10000ppm"]
["Butyl Methacrylate","n-BMA","97-88-1","C8H14O2","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～50%LEL/～10000ppm"]
["Butyl Methacrylate","n-BMA","97-88-1","C8H14O2","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Butyl Methacrylate","n-BMA","97-88-1","C8H14O2","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Butyl Methacrylate","n-BMA","97-88-1","C8H14O2","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Butyl Methacrylate","n-BMA","97-88-1","C8H14O2","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Butyl Methacrylate","n-BMA","97-88-1","C8H14O2","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Butyl Methacrylate","n-BMA","97-88-1","C8H14O2","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Butyl Methacrylate","n-BMA","97-88-1","C8H14O2","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Butyl Methacrylate","n-BMA","97-88-1","C8H14O2","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["C2 olefin","C2-OLEF","-","C4H3F5","SG","SG-8562","Fixed","GD-A80V Series","0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["C2 olefin","C2-OLEF","-","C4H3F5","SG","SG-8562","Fixed","GD-D58・GH Series","0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["C2 olefin","C2-OLEF","-","C4H3F5","SG","SG-8562","Fixed","SD-1GH Series","0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["C2 olefin","C2-OLEF","-","C4H3F5","SG","SG-8562","Fixed","SD-D58・GH Series","0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Carbon Dioxide","CO2","124-38-9","CO2","RI","DE-3123-5","Portable","RX-8500","0～20vol%"]
["Carbon Dioxide","CO2","124-38-9","CO2","RI","DES-3311-1","Portable","GX-6000","0～10vol%"]
["Carbon Dioxide","CO2","124-38-9","CO2","RI","DES-3311-4","Portable","GX-6000","0～10000ppm"]
["Carbon Dioxide","CO2","124-38-9","CO2","RI","DE-2113-44","Fixed","RI-557","0～2vol%"]
["Carbon Dioxide","CO2","124-38-9","CO2","RI","DE-2113-41","Fixed","RI-557","0～5vol%"]
["Carbon Dioxide","CO2","124-38-9","CO2","RI","DE-2113-47","Fixed","RI-557","0～10vol%"]
["Carbon Dioxide","CO2","124-38-9","CO2","RI","DE-2113-46","Fixed","RI-557","0～20vol%"]
["Carbon Dioxide","CO2","124-38-9","CO2","RI","DE-2113-46","Fixed","RI-557","0～50vol%"]
["Carbon Dioxide","CO2","124-38-9","CO2","RI","DE-2113-45","Fixed","RI-557","0～100vol%"]
["Carbon Dioxide","CO2","124-38-9","CO2","RI","DE-3315-3","Fixed","SD-1RI Series","0～10000ppm"]
["Carbon disulfide","CS2","75-15-0","CS2","SH","SH-8662","Portable","SP-220(TYPE FUM)","0～0.1ppm"]
["Carbon disulfide","CS2","75-15-0","CS2","SG","SG-8513","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["Carbon disulfide","CS2","75-15-0","CS2","SG","SG-8513","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["Carbon disulfide","CS2","75-15-0","CS2","SG","SG-8513","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["Carbon disulfide","CS2","75-15-0","CS2","SG","SG-8513","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["Carbon disulfide","CS2","75-15-0","CS2","SG","SG-8523","Fixed","GD-A80V Series","0～50ppm"]
["Carbon disulfide","CS2","75-15-0","CS2","SG","SG-8523","Fixed","GD-D58・GH Series","0～50ppm"]
["Carbon disulfide","CS2","75-15-0","CS2","SG","SG-8523","Fixed","SD-1GH Series","0～50ppm"]
["Carbon disulfide","CS2","75-15-0","CS2","SG","SG-8523","Fixed","SD-D58・GH Series","0～50ppm"]
["Carbon Monoxide","CO","630-08-0","CO","ES","ES-A3CP","Portable","CX-5","0～1000ppm"]
["Carbon Monoxide","CO","630-08-0","CO","ES","ES-1821","Portable","GX-2009","0～150ppm"]
["Carbon Monoxide","CO","630-08-0","CO","ES","ES-1821","Portable","GX-2012","0～150ppm"]
["Carbon Monoxide","CO","630-08-0","CO","ES","ES-1821","Portable","GX-2012GT","0～150ppm"]
["Carbon Monoxide","CO","630-08-0","CO","ES","ES-1821","Portable","GX-6000","0～150ppm"]
["Carbon Monoxide","CO","630-08-0","CO","ES","ES-1821","Portable","CO-03","0～150ppm"]
["Carbon Monoxide","CO","630-08-0","CO","ES","ES-031","Portable","GX-8000","0～150ppm"]
["Carbon Monoxide","CO","630-08-0","CO","ES","ES-031M","Portable","RX-8500","0～1000ppm"]
["Carbon Monoxide","CO","630-08-0","CO","SH","SH-8662","Portable","SP-220(TYPE SC)","0～30ppm"]
["Carbon Monoxide","CO","630-08-0","CO","ES","ESM-011","Portable","SC-01","0～75ppm"]
["Carbon Monoxide","CO","630-08-0","CO","ES","ESM-23","Portable","SC-8000","0～75ppm"]
["Carbon Monoxide","CO","630-08-0","CO","ES","ESM-23","Portable","SC-8000","0～150ppm"]
["Carbon Monoxide","CO","630-08-0","CO","ES","ESM-23","Portable","SC-8000","0～300ppm"]
["Carbon Monoxide","CO","630-08-0","CO","ES","ESU-23","Fixed","GD-70D Series","0～75ppm"]
["Carbon Monoxide","CO","630-08-0","CO","ES","ESU-23","Fixed","TP-70D","0～75ppm"]
["Carbon Monoxide","CO","630-08-0","CO","ES","ESU-23","Fixed","GD-70D Series","0～150ppm"]
["Carbon Monoxide","CO","630-08-0","CO","ES","ESU-23","Fixed","TP-70D","0～150ppm"]
["Carbon Monoxide","CO","630-08-0","CO","ES","ESU-23","Fixed","GD-70D Series","0～300ppm"]
["Carbon Monoxide","CO","630-08-0","CO","ES","ESU-23","Fixed","TP-70D","0～300ppm"]
["Carbon Monoxide","CO","630-08-0","CO","ES","ESU-231","Fixed","GD-70D Series","0～75ppm"]
["Carbon Monoxide","CO","630-08-0","CO","ES","ESU-231","Fixed","TP-70D","0～75ppm"]
["Carbon Monoxide","CO","630-08-0","CO","ES","ESU-231","Fixed","GD-70D Series","0～150ppm"]
["Carbon Monoxide","CO","630-08-0","CO","ES","ESU-231","Fixed","TP-70D","0～150ppm"]
["Carbon Monoxide","CO","630-08-0","CO","ES","ESU-231","Fixed","GD-70D Series","0～300ppm"]
["Carbon Monoxide","CO","630-08-0","CO","ES","ESU-231","Fixed","TP-70D","0～300ppm"]
["Carbon Monoxide","CO","630-08-0","CO","ES","ES-831","Fixed","SD-1EC Series","0～75ppm/0～150ppm/0～200ppm/0～250ppm/0～300ppm"]
["Carbon Monoxide","CO","630-08-0","CO","ES","ES-831","Fixed","SDWL-1EC Series","0～75ppm/0～150ppm/0～200ppm/0～250ppm/0～300ppm"]
["Carbon Monoxide","CO","630-08-0","CO","RI","DE-2113-53","Fixed","RI-557","0～5vol%"]
["Carbon Monoxide","CO","630-08-0","CO","RI","DE-2113-54","Fixed","RI-557","0～10vol%"]
["Carbon Monoxide","CO","630-08-0","CO","RI","DE-2113-59","Fixed","RI-557","0～20vol%"]
["Carbon Monoxide","CO","630-08-0","CO","RI","DE-2113-57","Fixed","RI-557","0～50vol%"]
["Carbon Monoxide","CO","630-08-0","CO","RI","DE-2113-63","Fixed","RI-557","0～100vol%"]
["Carbon Monoxide","CO","630-08-0","CO","ES","ESM-23","Fixed","GD-K88Ai Series","0～300ppm"]
["Carbon Monoxide","CO","630-08-0","CO","ES","ESM-23","Fixed","GD-K88Di Series","0～300ppm"]
["Carbon Monoxide","CO","630-08-0","CO","ES","ESM-23","Fixed","GD-K88Ai Series","0～150ppm"]
["Carbon Monoxide","CO","630-08-0","CO","ES","ESM-23","Fixed","GD-K88Di Series","0～150ppm"]
["Carbon Monoxide","CO","630-08-0","CO","ES","ESM-23","Fixed","GD-K88Ai Series","0～75ppm"]
["Carbon Monoxide","CO","630-08-0","CO","ES","ESM-23","Fixed","GD-K88Di Series","0～75ppm"]
["Carbon Monoxide","CO","630-08-0","CO","ES","ESM-231","Fixed","GD-K88Ai Series","0～300ppm"]
["Carbon Monoxide","CO","630-08-0","CO","ES","ESM-231","Fixed","GD-K88Di Series","0～300ppm"]
["Carbon Monoxide","CO","630-08-0","CO","ES","ESM-231","Fixed","GD-K88Ai Series","0～150ppm"]
["Carbon Monoxide","CO","630-08-0","CO","ES","ESM-231","Fixed","GD-K88Di Series","0～150ppm"]
["Carbon Monoxide","CO","630-08-0","CO","ES","ESM-231","Fixed","GD-K88Ai Series","0～75ppm"]
["Carbon Monoxide","CO","630-08-0","CO","ES","ESM-231","Fixed","GD-K88Di Series","0～75ppm"]
["Carbon Monoxide","CO","630-08-0","CO","ES","ESM-23M","Fixed","GD-K88Ai Series","0～1000ppm"]
["Carbon Monoxide","CO","630-08-0","CO","ES","ESM-23M","Fixed","GD-K88Di Series","0～1000ppm"]
["Carbon Monoxide","CO","630-08-0","CO","ES","ESM-23N","Fixed","GD-K88Ai Series","0～500ppm"]
["Carbon Monoxide","CO","630-08-0","CO","ES","ESM-23N","Fixed","GD-K88Di Series","0～500ppm"]
["Carbon Monoxide","CO","630-08-0","CO","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Carbon Monoxide","CO","630-08-0","CO","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Carbon Monoxide","CO","630-08-0","CO","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～125000ppm"]
["Carbon Monoxide","CO","630-08-0","CO","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～125000ppm"]
["Carbon Monoxide","CO","630-08-0","CO","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～125000ppm"]
["Carbon Monoxide","CO","630-08-0","CO","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～125000ppm"]
["Carbon Monoxide","CO","630-08-0","CO","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～125000ppm"]
["Carbon Monoxide","CO","630-08-0","CO","HW","HW-6239","Fixed","GD-A80-70 Series","0～100%LEL"]
["Carbon Monoxide","CO","630-08-0","CO","HW","HW-6239","Fixed","SD-1(TYPE GP) Series","0～100%LEL"]
["Carbon Monoxide","CO","630-08-0","CO","HW","HW-6239","Fixed","SD-D58(TYPE GP) Series","0～100%LEL"]
["Carbon Monoxide","CO","630-08-0","CO","HW","HW-6239/NC-6239","Fixed","GD-A80 Series","0～100%LEL/0～125000ppm"]
["Carbon Monoxide","CO","630-08-0","CO","HW","HW-6239/NC-6239","Fixed","GD-D58(TYPE GP) Series","0～100%LEL/0～125000ppm"]
["Carbon Monoxide","CO","630-08-0","CO","HW","HW-6239/NC-6239","Fixed","GD-D58(TYPE NC) Series","0～100%LEL/0～125000ppm"]
["Carbon Monoxide","CO","630-08-0","CO","HW","HW-6239/NC-6239","Fixed","SD-1(TYPE NC) Series","0～100%LEL/0～125000ppm"]
["Carbon Monoxide","CO","630-08-0","CO","HW","HW-6239/NC-6239","Fixed","SD-D58(TYPE NC) Series","0～100%LEL/0～125000ppm"]
["Carbon Monoxide","CO","630-08-0","CO","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Carbon Monoxide","CO","630-08-0","CO","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Carbon Monoxide","CO","630-08-0","CO","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Carbon Monoxide","CO","630-08-0","CO","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Carbon Monoxide","CO","630-08-0","CO","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Carbon Monoxide","CO","630-08-0","CO","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Carbon Monoxide","CO","630-08-0","CO","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Carbon Monoxide","CO","630-08-0","CO","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["Carbon Monoxide","CO","630-08-0","CO","SG","SG-8521","Fixed","GD-A80V Series","★0～150ppm/★0～200ppm/★0～300ppm/★0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm/0～10000ppm","★Range easily affected by environmental conditions and other"]
["Carbon Monoxide","CO","630-08-0","CO","SG","SG-8521","Fixed","GD-D58・GH Series","★0～150ppm/★0～200ppm/★0～300ppm/★0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm/0～10000ppm","★Range easily affected by environmental conditions and other"]
["Carbon Monoxide","CO","630-08-0","CO","SG","SG-8521","Fixed","SD-1GH Series","★0～150ppm/★0～200ppm/★0～300ppm/★0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm/0～10000ppm","★Range easily affected by environmental conditions and other"]
["Carbon Monoxide","CO","630-08-0","CO","SG","SG-8521","Fixed","SD-D58・GH Series","★0～150ppm/★0～200ppm/★0～300ppm/★0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm/0～10000ppm","★Range easily affected by environmental conditions and other"]
["Carbon Monoxide","CO","630-08-0","CO","SG","SG-8751","Fixed","GD-A44V","0～75ppm/0～100ppm/0～150ppm/0～200ppm"]
["Carbon tetrachloride","CCL4","56-23-5","CCL4","SG","SG-8513","Fixed","GD-A80V Series","0～500ppm/0～1000ppm/0～2000ppm"]
["Carbon tetrachloride","CCL4","56-23-5","CCL4","SG","SG-8513","Fixed","GD-D58・GH Series","0～500ppm/0～1000ppm/0～2000ppm"]
["Carbon tetrachloride","CCL4","56-23-5","CCL4","SG","SG-8513","Fixed","SD-1GH Series","0～500ppm/0～1000ppm/0～2000ppm"]
["Carbon tetrachloride","CCL4","56-23-5","CCL4","SG","SG-8513","Fixed","SD-D58・GH Series","0～500ppm/0～1000ppm/0～2000ppm"]
["Carbontetrafluoride","FC-14","75-73-0","CF4","RI","DE-2113-37","Fixed","RI-257","0～10000ppm"]
["Carbonyl fluoride","COF2","353-50-4","COF2","ES","ESU-K253","Fixed","GD-70D Series","0～6ppm"]
["Carbonyl fluoride","COF2","353-50-4","COF2","ES","ESU-K253","Fixed","TP-70D","0～6ppm"]
["Carbonyl fluoride","COF2","353-50-4","COF2","ES","ESU-K253L","Fixed","GD-70D Series","0～6ppm","Sensor for low humidity/Range: ～62%RH"]
["Carbonyl fluoride","COF2","353-50-4","COF2","ES","ESU-K253L","Fixed","TP-70D","0～6ppm","Sensor for low humidity/Range: ～62%RH"]
["Carbonyl sulfide","COS","463-58-1","COS","ES","ESU-237iF","Fixed","TP-70DGⅡ Series","0～15ppm","Only for TP-70DGⅡ"]
["Carbonyl sulfide","COS","463-58-1","COS","ES","ESU-238","Fixed","GD-70D+PLU Series","0～90ppm","PLU-70 required/Standard alarm point： 30ppm, 60ppm/Capable to set alarm point 25ppm under 20～30℃ environment"]
["Carbonyl sulfide","COS","463-58-1","COS","ES","ESU-238","Fixed","GD-70DG","0～90ppm","PLU-70 required/Standard alarm point： 30ppm, 60ppm/Capable to set alarm point 25ppm under 20～30℃ environment"]
["Carbonyl sulfide","COS","463-58-1","COS","ES","ESU-238","Fixed","TP-70DG","0～90ppm","PLU-70 required/Standard alarm point： 30ppm, 60ppm/Capable to set alarm point 25ppm under 20～30℃ environment"]
["Carbonyl sulfide","COS","463-58-1","COS","SG","SGU-8562","Fixed","GD-70D Series","0～2000ppm"]
["Carbonyl sulfide","COS","463-58-1","COS","SG","SGU-8562","Fixed","TP-70D","0～2000ppm"]
["Carbonyl sulfide","COS","463-58-1","COS","SG","SGU-8562","Fixed","GD-70D Series","0～5000ppm"]
["Carbonyl sulfide","COS","463-58-1","COS","SG","SGU-8562","Fixed","TP-70D","0～5000ppm"]
["Carbonyl sulfide","COS","463-58-1","COS","SG","SG-8521","Fixed","GD-A80V Series","★0～100ppm","★Range easily affected by environmental conditions and other"]
["Carbonyl sulfide","COS","463-58-1","COS","SG","SG-8521","Fixed","GD-D58・GH Series","★0～100ppm","★Range easily affected by environmental conditions and other"]
["Carbonyl sulfide","COS","463-58-1","COS","SG","SG-8521","Fixed","SD-1GH Series","★0～100ppm","★Range easily affected by environmental conditions and other"]
["Carbonyl sulfide","COS","463-58-1","COS","SG","SG-8521","Fixed","SD-D58・GH Series","★0～100ppm","★Range easily affected by environmental conditions and other"]
["Carbonyl sulfide","COS","463-58-1","COS","SG","SG-8562","Fixed","GD-A80V Series","0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Carbonyl sulfide","COS","463-58-1","COS","SG","SG-8562","Fixed","GD-D58・GH Series","0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Carbonyl sulfide","COS","463-58-1","COS","SG","SG-8562","Fixed","SD-1GH Series","0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Carbonyl sulfide","COS","463-58-1","COS","SG","SG-8562","Fixed","SD-D58・GH Series","0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESS-B335","Portable","GX-6000","0～10ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESM-K01-D","Portable","SC-01","0～3ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESM-K233","Portable","SC-8000","0～1.5ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESM-K233","Portable","SC-8000","0～3ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESM-K235","Portable","SC-8000","0～1.5ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESM-K235","Portable","SC-8000","0～3ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESU-K233","Fixed","GD-70D Series","0～1.5ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESU-K233","Fixed","TP-70D","0～1.5ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESU-K233","Fixed","GD-70D Series","0～3ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESU-K233","Fixed","TP-70D","0～3ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESU-K233L","Fixed","GD-70D Series","0～1.5ppm","Sensor for low humidity/Range： 20～62%RH"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESU-K233L","Fixed","TP-70D","0～1.5ppm","Sensor for low humidity/Range： 20～62%RH"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESU-K233L","Fixed","GD-70D Series","0～3ppm","Sensor for low humidity/Range： 20～62%RH"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESU-K233L","Fixed","TP-70D","0～3ppm","Sensor for low humidity/Range： 20～62%RH"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESU-K235","Fixed","GD-70D Series","0～1.5ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESU-K235","Fixed","TP-70D","0～1.5ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESU-K235","Fixed","GD-70D Series","0～3ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESU-K235","Fixed","TP-70D","0～3ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESU-K235L","Fixed","GD-70D Series","0～1.5ppm","Sensor for low humidity/Range： 20～65%RH"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESU-K235L","Fixed","TP-70D","0～1.5ppm","Sensor for low humidity/Range： 20～65%RH"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESU-K235L","Fixed","GD-70D Series","0～3ppm","Sensor for low humidity/Range： 20～65%RH"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESU-K235L","Fixed","TP-70D","0～3ppm","Sensor for low humidity/Range： 20～65%RH"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESU-K235","Fixed","GD-70D Series","0～10ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESU-K235","Fixed","TP-70D","0～10ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESU-K235L","Fixed","GD-70D Series","0～10ppm","Sensor for low humidity/Range： 20～65%RH"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESU-K235L","Fixed","TP-70D","0～10ppm","Sensor for low humidity/Range： 20～65%RH"]
["Chlorine","CL2","7782-50-5","CL2","ES","ES-B435","Fixed","SDWL-1EC Series","0～1.5ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESM-K233","Fixed","GD-K88Ai Series","0～15ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESM-K233","Fixed","GD-K88Di Series","0～15ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESM-K233","Fixed","GD-K88Ai Series","0～3ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESM-K233","Fixed","GD-K88Di Series","0～3ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESM-K235","Fixed","GD-K88Ai Series","0～1.5ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESM-K235","Fixed","GD-K88Di Series","0～1.5ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESM-K235","Fixed","GD-K88Ai Series","0～3ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESM-K235","Fixed","GD-K88Di Series","0～3ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESM-K239","Fixed","GD-K88Ai Series","0～1.5ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESM-K239","Fixed","GD-K88Di Series","0～1.5ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESM-K239","Fixed","GD-K88Ai Series","0～3ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESM-K239","Fixed","GD-K88Di Series","0～3ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESM-K239B","Fixed","GD-K88Ai Series","0～1.5ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESM-K239B","Fixed","GD-K88Di Series","0～1.5ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESM-K239B","Fixed","GD-K88Ai Series","0～3ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESM-K239B","Fixed","GD-K88Di Series","0～3ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESM-K233C","Fixed","GD-K88Ai Series","0～1.5ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESM-K233C","Fixed","GD-K88Di Series","0～1.5ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESM-K233C","Fixed","GD-K88Ai Series","0～3ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESM-K233C","Fixed","GD-K88Di Series","0～3ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESM-K233SE","Fixed","GD-K88Ai Series","0～1.5ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESM-K233SE","Fixed","GD-K88Di Series","0～1.5ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESM-K233SE","Fixed","GD-K88Ai Series","0～3ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESM-K233SE","Fixed","GD-K88Di Series","0～3ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESM-K239C","Fixed","GD-K88Ai Series","0～1.5ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESM-K239C","Fixed","GD-K88Di Series","0～1.5ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESM-K239C","Fixed","GD-K88Ai Series","0～3ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESM-K239C","Fixed","GD-K88Di Series","0～3ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESM-K233L","Fixed","GD-K88Ai Series","0～1.5ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESM-K233L","Fixed","GD-K88Di Series","0～1.5ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESM-K233L","Fixed","GD-K88Ai Series","0～3ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESM-K233L","Fixed","GD-K88Di Series","0～3ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESM-K235L","Fixed","GD-K88Ai Series","0～1.5ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESM-K235L","Fixed","GD-K88Di Series","0～1.5ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESM-K235L","Fixed","GD-K88Ai Series","0～3ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESM-K235L","Fixed","GD-K88Di Series","0～3ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESM-K239L","Fixed","GD-K88Ai Series","0～1.5ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESM-K239L","Fixed","GD-K88Di Series","0～1.5ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESM-K239L","Fixed","GD-K88Ai Series","0～3ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESM-K239L","Fixed","GD-K88Di Series","0～3ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESM-K235","Fixed","GD-K88Ai Series","0～10ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESM-K235","Fixed","GD-K88Di Series","0～10ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESM-K235L","Fixed","GD-K88Ai Series","0～10ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESM-K235L","Fixed","GD-K88Di Series","0～10ppm"]
["Chlorine Trifluoride","CLF3","7790-91-2","CLF3","ES","ESM-K233C(A)","Portable","SC-8000","0～1ppm","Acid interference"]
["Chlorine Trifluoride","CLF3","7790-91-2","CLF3","ES","ESM-K233C-S(A)","Portable","SC-8000","0～0.6ppm","Acid interference"]
["Chlorine Trifluoride","CLF3","7790-91-2","CLF3","ES","ESM-K233C-S(C)","Portable","SC-8000","0～0.6ppm","Non acid interference"]
["Chlorine Trifluoride","CLF3","7790-91-2","CLF3","ES","ESU-K233C(A)","Fixed","GD-70D Series","0～1ppm","Acid interference"]
["Chlorine Trifluoride","CLF3","7790-91-2","CLF3","ES","ESU-K233C(A)","Fixed","TP-70D","0～1ppm","Acid interference"]
["Chlorine Trifluoride","CLF3","7790-91-2","CLF3","ES","ESU-K233C(C)","Fixed","GD-70D Series","0～1ppm","Non acid interference"]
["Chlorine Trifluoride","CLF3","7790-91-2","CLF3","ES","ESU-K233C(C)","Fixed","TP-70D","0～1ppm","Non acid interference"]
["Chlorine Trifluoride","CLF3","7790-91-2","CLF3","ES","ESU-K233C-S(A)","Fixed","GD-70D Series","0～0.6ppm","Acid interference"]
["Chlorine Trifluoride","CLF3","7790-91-2","CLF3","ES","ESU-K233C-S(A)","Fixed","TP-70D","0～0.6ppm","Acid interference"]
["Chlorine Trifluoride","CLF3","7790-91-2","CLF3","ES","ESU-K233C-S(C)","Fixed","GD-70D Series","0～0.6ppm","Non acid interference"]
["Chlorine Trifluoride","CLF3","7790-91-2","CLF3","ES","ESU-K233C-S(C)","Fixed","TP-70D","0～0.6ppm","Non acid interference"]
["Chlorine Trifluoride","CLF3","7790-91-2","CLF3","ES","ESU-K233CL-S(A)","Fixed","GD-70D Series","0～0.6ppm","Acid interference/Sensor for low humidity/Range： 20～62%RH"]
["Chlorine Trifluoride","CLF3","7790-91-2","CLF3","ES","ESU-K233CL-S(A)","Fixed","TP-70D","0～0.6ppm","Acid interference/Sensor for low humidity/Range： 20～62%RH"]
["Chlorine Trifluoride","CLF3","7790-91-2","CLF3","ES","ESU-K233CL-S(C)","Fixed","GD-70D Series","0～0.6ppm","Non acid interference/Sensor for low humidity/Range： 20～62%Rh"]
["Chlorine Trifluoride","CLF3","7790-91-2","CLF3","ES","ESU-K233CL-S(C)","Fixed","TP-70D","0～0.6ppm","Non acid interference/Sensor for low humidity/Range： 20～62%Rh"]
["Chlorine Trifluoride","CLF3","7790-91-2","CLF3","ES","ESU-K236","Fixed","GD-70D Series","0～0.3ppm","Acid interference"]
["Chlorine Trifluoride","CLF3","7790-91-2","CLF3","ES","ESU-K236","Fixed","TP-70D","0～0.3ppm","Acid interference"]
["Chlorine Trifluoride","CLF3","7790-91-2","CLF3","ES","ESU-K236L","Fixed","GD-70D Series","0～0.3ppm","Acid interference/Sensor for low humidity/Range： 20～65%RH"]
["Chlorine Trifluoride","CLF3","7790-91-2","CLF3","ES","ESU-K236L","Fixed","TP-70D","0～0.3ppm","Acid interference/Sensor for low humidity/Range： 20～65%RH"]
["Chlorine Trifluoride","CLF3","7790-91-2","CLF3","ES","ESM-K233C(A)","Fixed","GD-K88Ai Series","0～1ppm","Acid interference"]
["Chlorine Trifluoride","CLF3","7790-91-2","CLF3","ES","ESM-K233C(A)","Fixed","GD-K88Di Series","0～1ppm","Acid interference"]
["Chlorine Trifluoride","CLF3","7790-91-2","CLF3","ES","ESM-K233C(C)","Fixed","GD-K88Ai Series","0～1ppm","Non acid interference"]
["Chlorine Trifluoride","CLF3","7790-91-2","CLF3","ES","ESM-K233C(C)","Fixed","GD-K88Di Series","0～1ppm","Non acid interference"]
["Chlorine Trifluoride","CLF3","7790-91-2","CLF3","ES","ESM-K233C-S(A)","Fixed","GD-K88Ai Series","0～0.6ppm","Acid interference"]
["Chlorine Trifluoride","CLF3","7790-91-2","CLF3","ES","ESM-K233C-S(A)","Fixed","GD-K88Di Series","0～0.6ppm","Acid interference"]
["Chlorine Trifluoride","CLF3","7790-91-2","CLF3","ES","ESM-K233C-S(C)","Fixed","GD-K88Ai Series","0～0.6ppm","Non acid interference"]
["Chlorine Trifluoride","CLF3","7790-91-2","CLF3","ES","ESM-K233C-S(C)","Fixed","GD-K88Di Series","0～0.6ppm","Non acid interference"]
["Chlorine Trifluoride","CLF3","7790-91-2","CLF3","ES","ESM-K236","Fixed","GD-K88Ai Series","0～0.3ppm","Acid interference"]
["Chlorine Trifluoride","CLF3","7790-91-2","CLF3","ES","ESM-K236","Fixed","GD-K88Di Series","0～0.3ppm","Acid interference"]
["Chlorine Trifluoride","CLF3","7790-91-2","CLF3","ES","ESM-K233CL(A)","Fixed","GD-K88Ai Series","0～1ppm","Acid interference/Sensor for low humidity/Range： 20～62%RH"]
["Chlorine Trifluoride","CLF3","7790-91-2","CLF3","ES","ESM-K233CL(A)","Fixed","GD-K88Di Series","0～1ppm","Acid interference/Sensor for low humidity/Range： 20～62%RH"]
["Chlorine Trifluoride","CLF3","7790-91-2","CLF3","ES","ESM-K233CL(C)","Fixed","GD-K88Ai Series","0～1ppm","Non acid interference/Sensor for low humidity/Range： 20～62%Rh"]
["Chlorine Trifluoride","CLF3","7790-91-2","CLF3","ES","ESM-K233CL(C)","Fixed","GD-K88Di Series","0～1ppm","Non acid interference/Sensor for low humidity/Range： 20～62%Rh"]
["Chlorine Trifluoride","CLF3","7790-91-2","CLF3","ES","ESM-K233CL-S(A)","Fixed","GD-K88Ai Series","0～0.6ppm","Acid interference/Sensor for low humidity/Range： 20～62%RH"]
["Chlorine Trifluoride","CLF3","7790-91-2","CLF3","ES","ESM-K233CL-S(A)","Fixed","GD-K88Di Series","0～0.6ppm","Acid interference/Sensor for low humidity/Range： 20～62%RH"]
["Chlorine Trifluoride","CLF3","7790-91-2","CLF3","ES","ESM-K233CL-S(C)","Fixed","GD-K88Ai Series","0～0.6ppm","Non acid interference/Sensor for low humidity/Range： 20～62%Rh"]
["Chlorine Trifluoride","CLF3","7790-91-2","CLF3","ES","ESM-K233CL-S(C)","Fixed","GD-K88Di Series","0～0.6ppm","Non acid interference/Sensor for low humidity/Range： 20～62%Rh"]
["Chlorine Trifluoride","CLF3","7790-91-2","CLF3","ES","ESM-K236L","Fixed","GD-K88Ai Series","0～0.3ppm","Acid interference/Sensor for low humidity/Range： 20～62%RH"]
["Chlorine Trifluoride","CLF3","7790-91-2","CLF3","ES","ESM-K236L","Fixed","GD-K88Di Series","0～0.3ppm","Acid interference/Sensor for low humidity/Range： 20～62%RH"]
["Chlorobenzene","C6H5CL","108-90-7","C6H5CL","SG","SG-8513","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Chlorobenzene","C6H5CL","108-90-7","C6H5CL","SG","SG-8513","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Chlorobenzene","C6H5CL","108-90-7","C6H5CL","SG","SG-8513","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Chlorobenzene","C6H5CL","108-90-7","C6H5CL","SG","SG-8513","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Chlorobromomethane","BCM","74-97-5","CH2CLBr","SG","SG-8523","Fixed","GD-A80V Series","0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Chlorobromomethane","BCM","74-97-5","CH2CLBr","SG","SG-8523","Fixed","GD-D58・GH Series","0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Chlorobromomethane","BCM","74-97-5","CH2CLBr","SG","SG-8523","Fixed","SD-1GH Series","0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Chlorobromomethane","BCM","74-97-5","CH2CLBr","SG","SG-8523","Fixed","SD-D58・GH Series","0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Chlorodifluoromethane","R-22","75-45-6","CHF2CL","SH","SH-8662","Portable","SP-220(TYPE SC)","0～50ppm"]
["Chlorodifluoromethane","R-22","75-45-6","CHF2CL","SH","SH-8661","Portable","SP-220(TYPE F)","0～10000ppm"]
["Chlorodifluoromethane","R-22","75-45-6","CHF2CL","SH","SH-8661","Portable","SP-220(TYPE H2)","0～10000ppm"]
["Chlorodifluoromethane","R-22","75-45-6","CHF2CL","RI","DE-2113-35","Fixed","RI-257","0～5000ppm"]
["Chlorodifluoromethane","R-22","75-45-6","CHF2CL","SG","SG-8513","Fixed","GD-A80V Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Chlorodifluoromethane","R-22","75-45-6","CHF2CL","SG","SG-8513","Fixed","GD-D58・GH Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Chlorodifluoromethane","R-22","75-45-6","CHF2CL","SG","SG-8513","Fixed","SD-1GH Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Chlorodifluoromethane","R-22","75-45-6","CHF2CL","SG","SG-8513","Fixed","SD-D58・GH Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Chloroform","CHCL3","67-66-3","CHCL3","SG","SG-8513","Fixed","GD-A80V Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Chloroform","CHCL3","67-66-3","CHCL3","SG","SG-8513","Fixed","GD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Chloroform","CHCL3","67-66-3","CHCL3","SG","SG-8513","Fixed","SD-1GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Chloroform","CHCL3","67-66-3","CHCL3","SG","SG-8513","Fixed","SD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Chloromethyl methyl ether","CMME","107-30-2","C2H5OCL","SG","SG-8523","Fixed","GD-A80V Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["Chloromethyl methyl ether","CMME","107-30-2","C2H5OCL","SG","SG-8523","Fixed","GD-D58・GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["Chloromethyl methyl ether","CMME","107-30-2","C2H5OCL","SG","SG-8523","Fixed","SD-1GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["Chloromethyl methyl ether","CMME","107-30-2","C2H5OCL","SG","SG-8523","Fixed","SD-D58・GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["Chlorotrifluoroethylene","CTFE","79-38-9","C2F3CL","SG","SGU-8513","Fixed","GD-70D Series","0～5000ppm"]
["Chlorotrifluoroethylene","CTFE","79-38-9","C2F3CL","SG","SGU-8513","Fixed","TP-70D","0～5000ppm"]
["Chlorotrifluoroethylene","CTFE","79-38-9","C2F3CL","SG","SG-8513","Fixed","GD-A80V Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Chlorotrifluoroethylene","CTFE","79-38-9","C2F3CL","SG","SG-8513","Fixed","GD-D58・GH Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Chlorotrifluoroethylene","CTFE","79-38-9","C2F3CL","SG","SG-8513","Fixed","SD-1GH Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Chlorotrifluoroethylene","CTFE","79-38-9","C2F3CL","SG","SG-8513","Fixed","SD-D58・GH Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Cresol","C7H8O","1319-77-3,95-48-7(-o),108-39-4(-m),106-44-5(-p)","C7H8O","SG","SG-8521","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Cresol","C7H8O","1319-77-3,95-48-7(-o),108-39-4(-m),106-44-5(-p)","C7H8O","SG","SG-8521","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Cresol","C7H8O","1319-77-3,95-48-7(-o),108-39-4(-m),106-44-5(-p)","C7H8O","SG","SG-8521","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Cresol","C7H8O","1319-77-3,95-48-7(-o),108-39-4(-m),106-44-5(-p)","C7H8O","SG","SG-8521","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Cumene","Cumene","98-82-8","C9H12","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Cumene","Cumene","98-82-8","C9H12","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Cumene","Cumene","98-82-8","C9H12","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～9000ppm"]
["Cumene","Cumene","98-82-8","C9H12","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～9000ppm"]
["Cumene","Cumene","98-82-8","C9H12","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～9000ppm"]
["Cumene","Cumene","98-82-8","C9H12","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～9000ppm"]
["Cumene","Cumene","98-82-8","C9H12","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～9000ppm"]
["Cumene","Cumene","98-82-8","C9H12","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Cumene","Cumene","98-82-8","C9H12","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Cumene","Cumene","98-82-8","C9H12","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Cumene","Cumene","98-82-8","C9H12","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Cumene","Cumene","98-82-8","C9H12","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Cumene","Cumene","98-82-8","C9H12","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Cumene","Cumene","98-82-8","C9H12","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Cumene","Cumene","98-82-8","C9H12","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["Cumene","Cumene","98-82-8","C9H12","SG","SG-8521","Fixed","GD-A80V Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Cumene","Cumene","98-82-8","C9H12","SG","SG-8521","Fixed","GD-D58・GH Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Cumene","Cumene","98-82-8","C9H12","SG","SG-8521","Fixed","SD-1GH Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Cumene","Cumene","98-82-8","C9H12","SG","SG-8521","Fixed","SD-D58・GH Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Cyclohexane","C6H12","110-82-7","C6H12","SG","SGU-8521","Fixed","GD-70D Series","0～2000ppm"]
["Cyclohexane","C6H12","110-82-7","C6H12","SG","SGU-8521","Fixed","TP-70D","0～2000ppm"]
["Cyclohexane","C6H12","110-82-7","C6H12","RI","DE-3315-2","Fixed","SD-1RI Series","0～100%LEL"]
["Cyclohexane","C6H12","110-82-7","C6H12","RI","DE-3315-2","Fixed","SD-1RI Series","0～5000ppm"]
["Cyclohexane","C6H12","110-82-7","C6H12","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Cyclohexane","C6H12","110-82-7","C6H12","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Cyclohexane","C6H12","110-82-7","C6H12","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～13000ppm"]
["Cyclohexane","C6H12","110-82-7","C6H12","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～13000ppm"]
["Cyclohexane","C6H12","110-82-7","C6H12","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～13000ppm"]
["Cyclohexane","C6H12","110-82-7","C6H12","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～13000ppm"]
["Cyclohexane","C6H12","110-82-7","C6H12","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～13000ppm"]
["Cyclohexane","C6H12","110-82-7","C6H12","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Cyclohexane","C6H12","110-82-7","C6H12","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Cyclohexane","C6H12","110-82-7","C6H12","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Cyclohexane","C6H12","110-82-7","C6H12","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Cyclohexane","C6H12","110-82-7","C6H12","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Cyclohexane","C6H12","110-82-7","C6H12","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Cyclohexane","C6H12","110-82-7","C6H12","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Cyclohexane","C6H12","110-82-7","C6H12","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["Cyclohexane","C6H12","110-82-7","C6H12","SG","SG-8521","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Cyclohexane","C6H12","110-82-7","C6H12","SG","SG-8521","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Cyclohexane","C6H12","110-82-7","C6H12","SG","SG-8521","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Cyclohexane","C6H12","110-82-7","C6H12","SG","SG-8521","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Cyclohexanol","C6H12O","108-93-0","C6H12O","HW","NC-6211","Fixed","GD-A80 Series","～25%LEL/～3000ppm"]
["Cyclohexanol","C6H12O","108-93-0","C6H12O","HW","NC-6211","Fixed","GD-D58(TYPE GP) Series","～25%LEL/～3000ppm"]
["Cyclohexanol","C6H12O","108-93-0","C6H12O","HW","NC-6211","Fixed","GD-D58(TYPE NC) Series","～25%LEL/～3000ppm"]
["Cyclohexanol","C6H12O","108-93-0","C6H12O","HW","NC-6211","Fixed","SD-1(TYPE NC) Series","～25%LEL/～3000ppm"]
["Cyclohexanol","C6H12O","108-93-0","C6H12O","HW","NC-6211","Fixed","SD-D58(TYPE NC) Series","～25%LEL/～3000ppm"]
["Cyclohexanol","C6H12O","108-93-0","C6H12O","SG","SG-8521","Fixed","GD-A80V Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Cyclohexanol","C6H12O","108-93-0","C6H12O","SG","SG-8521","Fixed","GD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Cyclohexanol","C6H12O","108-93-0","C6H12O","SG","SG-8521","Fixed","SD-1GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Cyclohexanol","C6H12O","108-93-0","C6H12O","SG","SG-8521","Fixed","SD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Cyclohexanone","C6H10O","108-94-1","C6H10O","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Cyclohexanone","C6H10O","108-94-1","C6H10O","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Cyclohexanone","C6H10O","108-94-1","C6H10O","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～11000ppm"]
["Cyclohexanone","C6H10O","108-94-1","C6H10O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～11000ppm"]
["Cyclohexanone","C6H10O","108-94-1","C6H10O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～11000ppm"]
["Cyclohexanone","C6H10O","108-94-1","C6H10O","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～11000ppm"]
["Cyclohexanone","C6H10O","108-94-1","C6H10O","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～11000ppm"]
["Cyclohexanone","C6H10O","108-94-1","C6H10O","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Cyclohexanone","C6H10O","108-94-1","C6H10O","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Cyclohexanone","C6H10O","108-94-1","C6H10O","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Cyclohexanone","C6H10O","108-94-1","C6H10O","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Cyclohexanone","C6H10O","108-94-1","C6H10O","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Cyclohexanone","C6H10O","108-94-1","C6H10O","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Cyclohexanone","C6H10O","108-94-1","C6H10O","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Cyclohexanone","C6H10O","108-94-1","C6H10O","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["Cyclohexanone","C6H10O","108-94-1","C6H10O","SG","SG-8521","Fixed","GD-A80V Series","0～50ppm/0～100ppm/0～200ppm/0～250ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Cyclohexanone","C6H10O","108-94-1","C6H10O","SG","SG-8521","Fixed","GD-D58・GH Series","0～50ppm/0～100ppm/0～200ppm/0～250ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Cyclohexanone","C6H10O","108-94-1","C6H10O","SG","SG-8521","Fixed","SD-1GH Series","0～50ppm/0～100ppm/0～200ppm/0～250ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Cyclohexanone","C6H10O","108-94-1","C6H10O","SG","SG-8521","Fixed","SD-D58・GH Series","0～50ppm/0～100ppm/0～200ppm/0～250ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Cyclohexene","C6H10","110-83-8","C6H10","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Cyclohexene","C6H10","110-83-8","C6H10","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Cyclohexene","C6H10","110-83-8","C6H10","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～12000ppm"]
["Cyclohexene","C6H10","110-83-8","C6H10","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～12000ppm"]
["Cyclohexene","C6H10","110-83-8","C6H10","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～12000ppm"]
["Cyclohexene","C6H10","110-83-8","C6H10","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～12000ppm"]
["Cyclohexene","C6H10","110-83-8","C6H10","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～12000ppm"]
["Cyclohexene","C6H10","110-83-8","C6H10","SG","SG-8521","Fixed","GD-A80V Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm"]
["Cyclohexene","C6H10","110-83-8","C6H10","SG","SG-8521","Fixed","GD-D58・GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm"]
["Cyclohexene","C6H10","110-83-8","C6H10","SG","SG-8521","Fixed","SD-1GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm"]
["Cyclohexene","C6H10","110-83-8","C6H10","SG","SG-8521","Fixed","SD-D58・GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm"]
["Cyclopentane","C5H10","287-92-3","C5H10","HW","NC-6215","Portable","GP-1000(HC/CH4)","0～100%LEL"]
["Cyclopentane","C5H10","287-92-3","C5H10","HW","NC-6307","Portable","NC-1000(HC/CH4)","0～10000ppm"]
["Cyclopentane","C5H10","287-92-3","C5H10","SH","SH-8661","Portable","SP-220(TYPE H2)","0～10000ppm"]
["Cyclopentane","C5H10","287-92-3","C5H10","RI","DE-2113-55","Fixed","RI-557","0～2000ppm"]
["Cyclopentane","C5H10","287-92-3","C5H10","RI","DE-3315-2","Fixed","SD-1RI Series","0～100%LEL"]
["Cyclopentane","C5H10","287-92-3","C5H10","RI","DE-3315-2","Fixed","SD-1RI Series","0～5000ppm"]
["Cyclopentane","C5H10","287-92-3","C5H10","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Cyclopentane","C5H10","287-92-3","C5H10","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Cyclopentane","C5H10","287-92-3","C5H10","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～14000ppm"]
["Cyclopentane","C5H10","287-92-3","C5H10","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～14000ppm"]
["Cyclopentane","C5H10","287-92-3","C5H10","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～14000ppm"]
["Cyclopentane","C5H10","287-92-3","C5H10","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～14000ppm"]
["Cyclopentane","C5H10","287-92-3","C5H10","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～14000ppm"]
["Cyclopentane","C5H10","287-92-3","C5H10","SG","SG-8521","Fixed","GD-A80V Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Cyclopentane","C5H10","287-92-3","C5H10","SG","SG-8521","Fixed","GD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Cyclopentane","C5H10","287-92-3","C5H10","SG","SG-8521","Fixed","SD-1GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Cyclopentane","C5H10","287-92-3","C5H10","SG","SG-8521","Fixed","SD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Cyclopentanone","C5H8O","120-92-3","C5H8O","SG","SGU-8521","Fixed","GD-70D Series","0～1000ppm"]
["Cyclopentanone","C5H8O","120-92-3","C5H8O","SG","SGU-8521","Fixed","TP-70D","0～1000ppm"]
["Cyclopentanone","C5H8O","120-92-3","C5H8O","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Cyclopentanone","C5H8O","120-92-3","C5H8O","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Cyclopentanone","C5H8O","120-92-3","C5H8O","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～14000ppm"]
["Cyclopentanone","C5H8O","120-92-3","C5H8O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～14000ppm"]
["Cyclopentanone","C5H8O","120-92-3","C5H8O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～14000ppm"]
["Cyclopentanone","C5H8O","120-92-3","C5H8O","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～14000ppm"]
["Cyclopentanone","C5H8O","120-92-3","C5H8O","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～14000ppm"]
["Cyclopentanone","C5H8O","120-92-3","C5H8O","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Cyclopentanone","C5H8O","120-92-3","C5H8O","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Cyclopentanone","C5H8O","120-92-3","C5H8O","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Cyclopentanone","C5H8O","120-92-3","C5H8O","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Cyclopentanone","C5H8O","120-92-3","C5H8O","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Cyclopentanone","C5H8O","120-92-3","C5H8O","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Cyclopentanone","C5H8O","120-92-3","C5H8O","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Cyclopentanone","C5H8O","120-92-3","C5H8O","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["Cyclopentanone","C5H8O","120-92-3","C5H8O","SG","SG-8521","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Cyclopentanone","C5H8O","120-92-3","C5H8O","SG","SG-8521","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Cyclopentanone","C5H8O","120-92-3","C5H8O","SG","SG-8521","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Cyclopentanone","C5H8O","120-92-3","C5H8O","SG","SG-8521","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Cyclopentene","c-C5H8","142-29-0","C5H8","SG","SG-8562","Fixed","GD-A80V Series","0～20ppm/0～30ppm/0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Cyclopentene","c-C5H8","142-29-0","C5H8","SG","SG-8562","Fixed","GD-D58・GH Series","0～20ppm/0～30ppm/0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Cyclopentene","c-C5H8","142-29-0","C5H8","SG","SG-8562","Fixed","SD-1GH Series","0～20ppm/0～30ppm/0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Cyclopentene","c-C5H8","142-29-0","C5H8","SG","SG-8562","Fixed","SD-D58・GH Series","0～20ppm/0～30ppm/0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Decahydronaphthalene","C10H18","91-17-8","C10H18","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Decahydronaphthalene","C10H18","91-17-8","C10H18","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Decahydronaphthalene","C10H18","91-17-8","C10H18","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Decahydronaphthalene","C10H18","91-17-8","C10H18","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Decahydronaphthalene","C10H18","91-17-8","C10H18","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Decahydronaphthalene","C10H18","91-17-8","C10H18","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Decahydronaphthalene","C10H18","91-17-8","C10H18","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Decahydronaphthalene","C10H18","91-17-8","C10H18","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["Decahydronaphthalene","C10H18","91-17-8","C10H18","SG","SG-8521","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Decahydronaphthalene","C10H18","91-17-8","C10H18","SG","SG-8521","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Decahydronaphthalene","C10H18","91-17-8","C10H18","SG","SG-8521","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Decahydronaphthalene","C10H18","91-17-8","C10H18","SG","SG-8521","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Deuterium","D2","7782-39-0","-","SG","SGU-8541","Fixed","GD-70D Series","0～2000ppm"]
["Deuterium","D2","7782-39-0","-","SG","SGU-8541","Fixed","TP-70D","0～2000ppm"]
["Deuterium","D2","7782-39-0","-","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Deuterium","D2","7782-39-0","-","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Deuterium","D2","7782-39-0","-","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～50000ppm"]
["Deuterium","D2","7782-39-0","-","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～50000ppm"]
["Deuterium","D2","7782-39-0","-","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～50000ppm"]
["Deuterium","D2","7782-39-0","-","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～50000ppm"]
["Deuterium","D2","7782-39-0","-","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～50000ppm"]
["Deuterium","D2","7782-39-0","-","SG","SG-8541","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Deuterium","D2","7782-39-0","-","SG","SG-8541","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Deuterium","D2","7782-39-0","-","SG","SG-8541","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Deuterium","D2","7782-39-0","-","SG","SG-8541","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Di(2-ethylhexyl)phthalate","DOP","117-81-7","C24H38O4","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Di(2-ethylhexyl)phthalate","DOP","117-81-7","C24H38O4","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Di(2-ethylhexyl)phthalate","DOP","117-81-7","C24H38O4","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Diborane","B2H6","19287-45-7","B2H6","SH","SH-8662","Portable","SP-220(TYPE SC)","0～0.1ppm"]
["Diborane","B2H6","19287-45-7","B2H6","ES","ESM-23AY","Portable","SC-8000","0～0.3ppm"]
["Diborane","B2H6","19287-45-7","B2H6","ES","ESM-23AYA","Portable","SC-8000","0～0.3ppm"]
["Diborane","B2H6","19287-45-7","B2H6","ES","ESU-23AY","Fixed","GD-70D Series","0～0.3ppm"]
["Diborane","B2H6","19287-45-7","B2H6","ES","ESU-23AY","Fixed","TP-70D","0～0.3ppm"]
["Diborane","B2H6","19287-45-7","B2H6","ES","ESM-23AYA","Fixed","GD-K88Ai Series","0～0.3ppm"]
["Diborane","B2H6","19287-45-7","B2H6","ES","ESM-23AYA","Fixed","GD-K88Di Series","0～0.3ppm"]
["Diborane","B2H6","19287-45-7","B2H6","ES","ESM-23AY-SA","Fixed","GD-K88Ai Series","0～0.3ppm"]
["Diborane","B2H6","19287-45-7","B2H6","ES","ESM-23AY-SA","Fixed","GD-K88Di Series","0～0.3ppm"]
["Dibromomethane","CH2Br2","74-95-3","CH2Br2","SG","SG-8511","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Dibromomethane","CH2Br2","74-95-3","CH2Br2","SG","SG-8511","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Dibromomethane","CH2Br2","74-95-3","CH2Br2","SG","SG-8511","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Dibromomethane","CH2Br2","74-95-3","CH2Br2","SG","SG-8511","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Dibromomethane","CH2Br2","74-95-3","CH2Br2","SG","SG-8521","Fixed","GD-A80V Series","0～2000ppm/0～3000ppm/0～5000ppm"]
["Dibromomethane","CH2Br2","74-95-3","CH2Br2","SG","SG-8521","Fixed","GD-D58・GH Series","0～2000ppm/0～3000ppm/0～5000ppm"]
["Dibromomethane","CH2Br2","74-95-3","CH2Br2","SG","SG-8521","Fixed","SD-1GH Series","0～2000ppm/0～3000ppm/0～5000ppm"]
["Dibromomethane","CH2Br2","74-95-3","CH2Br2","SG","SG-8521","Fixed","SD-D58・GH Series","0～2000ppm/0～3000ppm/0～5000ppm"]
["Dibutyl ether","DBuE","142-96-1","C8H18O","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Dibutyl ether","DBuE","142-96-1","C8H18O","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Dibutyl ether","DBuE","142-96-1","C8H18O","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～15000ppm"]
["Dibutyl ether","DBuE","142-96-1","C8H18O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～15000ppm"]
["Dibutyl ether","DBuE","142-96-1","C8H18O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～15000ppm"]
["Dibutyl ether","DBuE","142-96-1","C8H18O","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～15000ppm"]
["Dibutyl ether","DBuE","142-96-1","C8H18O","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～15000ppm"]
["Dibutyl ether","DBuE","142-96-1","C8H18O","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Dibutyl ether","DBuE","142-96-1","C8H18O","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Dibutyl ether","DBuE","142-96-1","C8H18O","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Dibutyl ether","DBuE","142-96-1","C8H18O","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Dibutyl ether","DBuE","142-96-1","C8H18O","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Dibutyl ether","DBuE","142-96-1","C8H18O","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Dibutyl ether","DBuE","142-96-1","C8H18O","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Dibutyl ether","DBuE","142-96-1","C8H18O","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["Dibutyl ether","DBuE","142-96-1","C8H18O","SG","SG-8511","Fixed","GD-A80V Series","0～2000ppm/0～3000ppm/0～5000ppm"]
["Dibutyl ether","DBuE","142-96-1","C8H18O","SG","SG-8511","Fixed","GD-D58・GH Series","0～2000ppm/0～3000ppm/0～5000ppm"]
["Dibutyl ether","DBuE","142-96-1","C8H18O","SG","SG-8511","Fixed","SD-1GH Series","0～2000ppm/0～3000ppm/0～5000ppm"]
["Dibutyl ether","DBuE","142-96-1","C8H18O","SG","SG-8511","Fixed","SD-D58・GH Series","0～2000ppm/0～3000ppm/0～5000ppm"]
["Dibutyl ether","DBuE","142-96-1","C8H18O","SG","SG-8521","Fixed","GD-A80V Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Dibutyl ether","DBuE","142-96-1","C8H18O","SG","SG-8521","Fixed","GD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Dibutyl ether","DBuE","142-96-1","C8H18O","SG","SG-8521","Fixed","SD-1GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Dibutyl ether","DBuE","142-96-1","C8H18O","SG","SG-8521","Fixed","SD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Dichlorobenzene","C6H4CL2","106-46-7(-p),95-50-1(-o)","C6H4CL2","SG","SG-8523","Fixed","GD-A80V Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Dichlorobenzene","C6H4CL2","106-46-7(-p),95-50-1(-o)","C6H4CL2","SG","SG-8523","Fixed","GD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Dichlorobenzene","C6H4CL2","106-46-7(-p),95-50-1(-o)","C6H4CL2","SG","SG-8523","Fixed","SD-1GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Dichlorobenzene","C6H4CL2","106-46-7(-p),95-50-1(-o)","C6H4CL2","SG","SG-8523","Fixed","SD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Dichlorodifluoromethane","R-12","75-71-8","CF2CL2","SG","SG-8513","Fixed","GD-A80V Series","0～10000ppm"]
["Dichlorodifluoromethane","R-12","75-71-8","CF2CL2","SG","SG-8513","Fixed","GD-D58・GH Series","0～10000ppm"]
["Dichlorodifluoromethane","R-12","75-71-8","CF2CL2","SG","SG-8513","Fixed","SD-1GH Series","0～10000ppm"]
["Dichlorodifluoromethane","R-12","75-71-8","CF2CL2","SG","SG-8513","Fixed","SD-D58・GH Series","0～10000ppm"]
["Dichlorofluoromethane","R-21","75-43-4","CHFCL2","SG","SG-8513","Fixed","GD-A80V Series","0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Dichlorofluoromethane","R-21","75-43-4","CHFCL2","SG","SG-8513","Fixed","GD-D58・GH Series","0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Dichlorofluoromethane","R-21","75-43-4","CHFCL2","SG","SG-8513","Fixed","SD-1GH Series","0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Dichlorofluoromethane","R-21","75-43-4","CHFCL2","SG","SG-8513","Fixed","SD-D58・GH Series","0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Dichloromethane","CH2CL2","75-09-2","CH2CL2","SG","SGU-8523","Fixed","GD-70D Series","0～2000ppm"]
["Dichloromethane","CH2CL2","75-09-2","CH2CL2","SG","SGU-8523","Fixed","TP-70D","0～2000ppm"]
["Dichloromethane","CH2CL2","75-09-2","CH2CL2","RI","DE-3315-1","Fixed","SD-1RI Series","0～100%LEL"]
["Dichloromethane","CH2CL2","75-09-2","CH2CL2","SG","SG-8523","Fixed","GD-A80V Series","0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Dichloromethane","CH2CL2","75-09-2","CH2CL2","SG","SG-8523","Fixed","GD-D58・GH Series","0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Dichloromethane","CH2CL2","75-09-2","CH2CL2","SG","SG-8523","Fixed","SD-1GH Series","0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Dichloromethane","CH2CL2","75-09-2","CH2CL2","SG","SG-8523","Fixed","SD-D58・GH Series","0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Dichlorotetrafluoroethane","R-114","76-14-2","C2F4CL2","RI","DE-2113-35","Fixed","RI-257","0～5000ppm"]
["Dichlorotetrafluoroethane","R-114","76-14-2","C2F4CL2","SG","SG-8513","Fixed","GD-A80V Series","0～10000ppm"]
["Dichlorotetrafluoroethane","R-114","76-14-2","C2F4CL2","SG","SG-8513","Fixed","GD-D58・GH Series","0～10000ppm"]
["Dichlorotetrafluoroethane","R-114","76-14-2","C2F4CL2","SG","SG-8513","Fixed","SD-1GH Series","0～10000ppm"]
["Dichlorotetrafluoroethane","R-114","76-14-2","C2F4CL2","SG","SG-8513","Fixed","SD-D58・GH Series","0～10000ppm"]
["Dichlorotoluene","C7H6CL2","95-73-8,19398-61-9,118-69-4,32768-54-0","C7H6CL2","SG","SG-8511","Fixed","GD-A80V Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Dichlorotoluene","C7H6CL2","95-73-8,19398-61-9,118-69-4,32768-54-0","C7H6CL2","SG","SG-8511","Fixed","GD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Dichlorotoluene","C7H6CL2","95-73-8,19398-61-9,118-69-4,32768-54-0","C7H6CL2","SG","SG-8511","Fixed","SD-1GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Dichlorotoluene","C7H6CL2","95-73-8,19398-61-9,118-69-4,32768-54-0","C7H6CL2","SG","SG-8511","Fixed","SD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Dicyclopentadiene","DCPD","77-73-6","C10H12","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Dicyclopentadiene","DCPD","77-73-6","C10H12","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Dicyclopentadiene","DCPD","77-73-6","C10H12","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～10000ppm"]
["Dicyclopentadiene","DCPD","77-73-6","C10H12","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～10000ppm"]
["Dicyclopentadiene","DCPD","77-73-6","C10H12","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～10000ppm"]
["Dicyclopentadiene","DCPD","77-73-6","C10H12","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～10000ppm"]
["Dicyclopentadiene","DCPD","77-73-6","C10H12","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～10000ppm"]
["Dicyclopentadiene","DCPD","77-73-6","C10H12","SG","SG-8521","Fixed","GD-A80V Series","0～500ppm/0～1000ppm/0～2000ppm"]
["Dicyclopentadiene","DCPD","77-73-6","C10H12","SG","SG-8521","Fixed","GD-D58・GH Series","0～500ppm/0～1000ppm/0～2000ppm"]
["Dicyclopentadiene","DCPD","77-73-6","C10H12","SG","SG-8521","Fixed","SD-1GH Series","0～500ppm/0～1000ppm/0～2000ppm"]
["Dicyclopentadiene","DCPD","77-73-6","C10H12","SG","SG-8521","Fixed","SD-D58・GH Series","0～500ppm/0～1000ppm/0～2000ppm"]
["Diethoxymethylsilane","DEMS","2031-62-1","C5H14O2Si","SS","SSU-1925","Fixed","GD-70D+PLU Series","0‐15ppm","PLU-70 required"]
["Diethoxymethylsilane","DEMS","2031-62-1","C5H14O2Si","SS","SSU-1925","Fixed","GD-70DG","0‐15ppm","PLU-70 required"]
["Diethyl carbonate","C5H10O3","105-58-8","C5H10O3","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Diethyl carbonate","C5H10O3","105-58-8","C5H10O3","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Diethyl carbonate","C5H10O3","105-58-8","C5H10O3","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～14000ppm"]
["Diethyl carbonate","C5H10O3","105-58-8","C5H10O3","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～14000ppm"]
["Diethyl carbonate","C5H10O3","105-58-8","C5H10O3","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～14000ppm"]
["Diethyl carbonate","C5H10O3","105-58-8","C5H10O3","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～14000ppm"]
["Diethyl carbonate","C5H10O3","105-58-8","C5H10O3","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～14000ppm"]
["Diethyl carbonate","C5H10O3","105-58-8","C5H10O3","SG","SG-8521","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm"]
["Diethyl carbonate","C5H10O3","105-58-8","C5H10O3","SG","SG-8521","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm"]
["Diethyl carbonate","C5H10O3","105-58-8","C5H10O3","SG","SG-8521","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm"]
["Diethyl carbonate","C5H10O3","105-58-8","C5H10O3","SG","SG-8521","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm"]
["Diethyl ketone","DEK","96-22-0","C5H10O","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Diethyl ketone","DEK","96-22-0","C5H10O","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Diethyl ketone","DEK","96-22-0","C5H10O","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～16000ppm"]
["Diethyl ketone","DEK","96-22-0","C5H10O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～16000ppm"]
["Diethyl ketone","DEK","96-22-0","C5H10O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～16000ppm"]
["Diethyl ketone","DEK","96-22-0","C5H10O","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～16000ppm"]
["Diethyl ketone","DEK","96-22-0","C5H10O","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～16000ppm"]
["Diethylamine","DEA","109-89-7","C4H11N","ES","ESU-23RV-EX","Fixed","GD-70D Series","0.2～15ppm","Export limited：unable to measure under 0.2ppm"]
["Diethylamine","DEA","109-89-7","C4H11N","ES","ESU-23RV-EX","Fixed","TP-70D","0.2～15ppm","Export limited：unable to measure under 0.2ppm"]
["Diethylamine","DEA","109-89-7","C4H11N","ES","ESU-23RVM-EX","Fixed","GD-70D Series","0.2～15ppm","Export limited：unable to measure under 0.2ppm"]
["Diethylamine","DEA","109-89-7","C4H11N","ES","ESU-23RVM-EX","Fixed","TP-70D","0.2～15ppm","Export limited：unable to measure under 0.2ppm"]
["Diethylamine","DEA","109-89-7","C4H11N","ES","ESM-23RV","Fixed","GD-K88Ai Series","0～15ppm"]
["Diethylamine","DEA","109-89-7","C4H11N","ES","ESM-23RV","Fixed","GD-K88Di Series","0～15ppm"]
["Diethylamine","DEA","109-89-7","C4H11N","ES","ESM-23RVM","Fixed","GD-K88Ai Series","0.2～15ppm","Export limited：unable to measure under 0.2ppm"]
["Diethylamine","DEA","109-89-7","C4H11N","ES","ESM-23RVM","Fixed","GD-K88Di Series","0.2～15ppm","Export limited：unable to measure under 0.2ppm"]
["Diethylbenzene","C10H14","25340-17-4","C10H14","SG","SG-8521","Fixed","GD-A80V Series","0～30ppm/0～50ppm/0～100ppm/0～200ppm"]
["Diethylbenzene","C10H14","25340-17-4","C10H14","SG","SG-8521","Fixed","GD-D58・GH Series","0～30ppm/0～50ppm/0～100ppm/0～200ppm"]
["Diethylbenzene","C10H14","25340-17-4","C10H14","SG","SG-8521","Fixed","SD-1GH Series","0～30ppm/0～50ppm/0～100ppm/0～200ppm"]
["Diethylbenzene","C10H14","25340-17-4","C10H14","SG","SG-8521","Fixed","SD-D58・GH Series","0～30ppm/0～50ppm/0～100ppm/0～200ppm"]
["Diethylene Glycol","C4H10O3","111-46-4","C4H10O3","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Diethylene Glycol","C4H10O3","111-46-4","C4H10O3","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Diethylene Glycol","C4H10O3","111-46-4","C4H10O3","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Diethylene Glycol","C4H10O3","111-46-4","C4H10O3","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Diethylene Glycol","C4H10O3","111-46-4","C4H10O3","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Diethylene Glycol","C4H10O3","111-46-4","C4H10O3","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Diethylene Glycol","C4H10O3","111-46-4","C4H10O3","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Diethylene Glycol","C4H10O3","111-46-4","C4H10O3","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Diethylene Glycol","C4H10O3","111-46-4","C4H10O3","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Diethylene Glycol","C4H10O3","111-46-4","C4H10O3","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Diethylene Glycol Dimethyl Ether","C6H14O3","111-96-6","C6H14O3","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Diethylene Glycol Dimethyl Ether","C6H14O3","111-96-6","C6H14O3","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Diethylene Glycol Dimethyl Ether","C6H14O3","111-96-6","C6H14O3","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Diethylene Glycol Dimethyl Ether","C6H14O3","111-96-6","C6H14O3","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Diethylene Glycol Dimethyl Ether","C6H14O3","111-96-6","C6H14O3","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Diethylene Glycol Dimethyl Ether","C6H14O3","111-96-6","C6H14O3","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Diethylene Glycol Dimethyl Ether","C6H14O3","111-96-6","C6H14O3","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Diethylene Glycol Dimethyl Ether","C6H14O3","111-96-6","C6H14O3","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["Diethylene Glycol Dimethyl Ether","C6H14O3","111-96-6","C6H14O3","SG","SG-8521","Fixed","GD-A80V Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Diethylene Glycol Dimethyl Ether","C6H14O3","111-96-6","C6H14O3","SG","SG-8521","Fixed","GD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Diethylene Glycol Dimethyl Ether","C6H14O3","111-96-6","C6H14O3","SG","SG-8521","Fixed","SD-1GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Diethylene Glycol Dimethyl Ether","C6H14O3","111-96-6","C6H14O3","SG","SG-8521","Fixed","SD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Diethylene Glycol Ethyl Methyl Ether","C7H16O3","1002-67-1","C7H16O3","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Diethylene Glycol Ethyl Methyl Ether","C7H16O3","1002-67-1","C7H16O3","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Diethylene Glycol Ethyl Methyl Ether","C7H16O3","1002-67-1","C7H16O3","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Diethylene Glycol Ethyl Methyl Ether","C7H16O3","1002-67-1","C7H16O3","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Diethylene Glycol Ethyl Methyl Ether","C7H16O3","1002-67-1","C7H16O3","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Diethylene Glycol Ethyl Methyl Ether","C7H16O3","1002-67-1","C7H16O3","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Diethylene Glycol Ethyl Methyl Ether","C7H16O3","1002-67-1","C7H16O3","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Diethylene Glycol Ethyl Methyl Ether","C7H16O3","1002-67-1","C7H16O3","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["Diethylene Glycol Ethyl Methyl Ether","C7H16O3","1002-67-1","C7H16O3","SG","SG-8521","Fixed","GD-A80V Series","0～200ppm/0～300ppm/0～500ppm"]
["Diethylene Glycol Ethyl Methyl Ether","C7H16O3","1002-67-1","C7H16O3","SG","SG-8521","Fixed","GD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm"]
["Diethylene Glycol Ethyl Methyl Ether","C7H16O3","1002-67-1","C7H16O3","SG","SG-8521","Fixed","SD-1GH Series","0～200ppm/0～300ppm/0～500ppm"]
["Diethylene Glycol Ethyl Methyl Ether","C7H16O3","1002-67-1","C7H16O3","SG","SG-8521","Fixed","SD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm"]
["Diethylene Glycol Monoethyl Ether","DEGEE","111-90-0","C6H14O3","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Diethylene Glycol Monoethyl Ether","DEGEE","111-90-0","C6H14O3","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Diethylene Glycol Monoethyl Ether","DEGEE","111-90-0","C6H14O3","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Diethylene Glycol Monoethyl Ether","DEGEE","111-90-0","C6H14O3","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Diethylene Glycol Monoethyl Ether","DEGEE","111-90-0","C6H14O3","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Diethylene Glycol Monoethyl Ether","DEGEE","111-90-0","C6H14O3","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Diethylene Glycol Monoethyl Ether","DEGEE","111-90-0","C6H14O3","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Diethylene Glycol Monoethyl Ether","DEGEE","111-90-0","C6H14O3","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["Difluorodibromomethane","CF2Br2","75-61-6","CF2Br2","SG","SG-8562","Fixed","GD-A80V Series","0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Difluorodibromomethane","CF2Br2","75-61-6","CF2Br2","SG","SG-8562","Fixed","GD-D58・GH Series","0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Difluorodibromomethane","CF2Br2","75-61-6","CF2Br2","SG","SG-8562","Fixed","SD-1GH Series","0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Difluorodibromomethane","CF2Br2","75-61-6","CF2Br2","SG","SG-8562","Fixed","SD-D58・GH Series","0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Difluoromethane","R-32","75-10-5","CH2F2","SH","SH-8662","Portable","SP-220(TYPE SC)","0～50ppm"]
["Difluoromethane","R-32","75-10-5","CH2F2","SH","SH-8661","Portable","SP-220(TYPE F)","0～10000ppm"]
["Difluoromethane","R-32","75-10-5","CH2F2","ES","ESU-K233","Fixed","GD-70D Series","0～60ppm","PLU-70 required/Response(T62.5)150sec，10～30℃"]
["Difluoromethane","R-32","75-10-5","CH2F2","ES","ESU-K233","Fixed","TP-70D","0～60ppm","PLU-70 required/Response(T62.5)150sec，10～30℃"]
["Difluoromethane","R-32","75-10-5","CH2F2","SG","SGU-8521","Fixed","GD-70D Series","0～2000ppm"]
["Difluoromethane","R-32","75-10-5","CH2F2","SG","SGU-8521","Fixed","TP-70D","0～2000ppm"]
["Difluoromethane","R-32","75-10-5","CH2F2","SG","SGU-8521","Fixed","GD-70D Series","0～5000ppm"]
["Difluoromethane","R-32","75-10-5","CH2F2","SG","SGU-8521","Fixed","TP-70D","0～5000ppm"]
["Difluoromethane","R-32","75-10-5","CH2F2","SG","SGU-8521","Fixed","GD-70D Series","0～9000ppm"]
["Difluoromethane","R-32","75-10-5","CH2F2","SG","SGU-8521","Fixed","TP-70D","0～9000ppm"]
["Difluoromethane","R-32","75-10-5","CH2F2","SG","SGU-8582","Fixed","GD-70D Series","0～2000ppm"]
["Difluoromethane","R-32","75-10-5","CH2F2","SG","SGU-8582","Fixed","TP-70D","0～2000ppm"]
["Difluoromethane","R-32","75-10-5","CH2F2","SG","SGU-8582","Fixed","GD-70D Series","0～10000ppm"]
["Difluoromethane","R-32","75-10-5","CH2F2","SG","SGU-8582","Fixed","TP-70D","0～10000ppm"]
["Difluoromethane","R-32","75-10-5","CH2F2","RI","DE-2113-35","Fixed","RI-257","0～10000ppm"]
["Difluoromethane","R-32","75-10-5","CH2F2","SG","SG-8521","Fixed","GD-A80V Series","0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm/0～9000ppm/0～10000ppm"]
["Difluoromethane","R-32","75-10-5","CH2F2","SG","SG-8521","Fixed","GD-D58・GH Series","0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm/0～9000ppm/0～10000ppm"]
["Difluoromethane","R-32","75-10-5","CH2F2","SG","SG-8521","Fixed","SD-1GH Series","0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm/0～9000ppm/0～10000ppm"]
["Difluoromethane","R-32","75-10-5","CH2F2","SG","SG-8521","Fixed","SD-D58・GH Series","0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm/0～9000ppm/0～10000ppm"]
["Difluoromethane","R-32","75-10-5","CH2F2","SG","SG-8582","Fixed","GD-A80V Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm/0～10000ppm"]
["Difluoromethane","R-32","75-10-5","CH2F2","SG","SG-8582","Fixed","GD-D58・GH Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm/0～10000ppm"]
["Difluoromethane","R-32","75-10-5","CH2F2","SG","SG-8582","Fixed","SD-1GH Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm/0～10000ppm"]
["Difluoromethane","R-32","75-10-5","CH2F2","SG","SG-8582","Fixed","SD-D58・GH Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm/0～10000ppm"]
["Diisobutyl ketone","C9H18O","108-83-8","C9H18O","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Diisobutyl ketone","C9H18O","108-83-8","C9H18O","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Diisobutyl ketone","C9H18O","108-83-8","C9H18O","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Diisobutyl ketone","C9H18O","108-83-8","C9H18O","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Diisobutyl ketone","C9H18O","108-83-8","C9H18O","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Diisobutyl ketone","C9H18O","108-83-8","C9H18O","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Diisobutyl ketone","C9H18O","108-83-8","C9H18O","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Diisobutyl ketone","C9H18O","108-83-8","C9H18O","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["Dimethoxydimethylsilane","DMDMOS","1112-39-6","C4H12O2Si","SS","SSU-1925","Fixed","GD-70D+PLU Series","0‐15ppm","PLU-70 required"]
["Dimethoxydimethylsilane","DMDMOS","1112-39-6","C4H12O2Si","SS","SSU-1925","Fixed","GD-70DG","0‐15ppm","PLU-70 required"]
["Dimethyl carbonate","C3H6O3","616-38-6","C3H6O3","RI","DE-3315-2","Fixed","SD-1RI Series","0～100%LEL"]
["Dimethyl carbonate","C3H6O3","616-38-6","C3H6O3","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Dimethyl carbonate","C3H6O3","616-38-6","C3H6O3","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Dimethyl carbonate","C3H6O3","616-38-6","C3H6O3","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～42000ppm"]
["Dimethyl carbonate","C3H6O3","616-38-6","C3H6O3","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～42000ppm"]
["Dimethyl carbonate","C3H6O3","616-38-6","C3H6O3","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～42000ppm"]
["Dimethyl carbonate","C3H6O3","616-38-6","C3H6O3","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～42000ppm"]
["Dimethyl carbonate","C3H6O3","616-38-6","C3H6O3","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～42000ppm"]
["Dimethyl carbonate","C3H6O3","616-38-6","C3H6O3","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Dimethyl carbonate","C3H6O3","616-38-6","C3H6O3","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Dimethyl carbonate","C3H6O3","616-38-6","C3H6O3","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Dimethyl carbonate","C3H6O3","616-38-6","C3H6O3","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Dimethyl carbonate","C3H6O3","616-38-6","C3H6O3","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Dimethyl carbonate","C3H6O3","616-38-6","C3H6O3","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Dimethyl carbonate","C3H6O3","616-38-6","C3H6O3","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Dimethyl carbonate","C3H6O3","616-38-6","C3H6O3","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["Dimethyl carbonate","C3H6O3","616-38-6","C3H6O3","SG","SG-8521","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Dimethyl carbonate","C3H6O3","616-38-6","C3H6O3","SG","SG-8521","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Dimethyl carbonate","C3H6O3","616-38-6","C3H6O3","SG","SG-8521","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Dimethyl carbonate","C3H6O3","616-38-6","C3H6O3","SG","SG-8521","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Dimethyl ether","DME","115-10-6","C2H6O","HW","NC-6215","Portable","GP-1000(HC/CH4)","0～100%LEL"]
["Dimethyl ether","DME","115-10-6","C2H6O","HW","NC-6307","Portable","NC-1000(HC/CH4)","0～10000ppm"]
["Dimethyl ether","DME","115-10-6","C2H6O","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Dimethyl ether","DME","115-10-6","C2H6O","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Dimethyl ether","DME","115-10-6","C2H6O","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～30000ppm"]
["Dimethyl ether","DME","115-10-6","C2H6O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～30000ppm"]
["Dimethyl ether","DME","115-10-6","C2H6O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～30000ppm"]
["Dimethyl ether","DME","115-10-6","C2H6O","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～30000ppm"]
["Dimethyl ether","DME","115-10-6","C2H6O","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～30000ppm"]
["Dimethyl ether","DME","115-10-6","C2H6O","SG","SG-8521","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Dimethyl ether","DME","115-10-6","C2H6O","SG","SG-8521","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Dimethyl ether","DME","115-10-6","C2H6O","SG","SG-8521","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Dimethyl ether","DME","115-10-6","C2H6O","SG","SG-8521","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Dimethyl sulfate","C2H6O4S","77-78-1","C2H6O4S","SG","SG-8562","Fixed","GD-A80V Series","0～200ppm/0～300ppm/0～500ppm"]
["Dimethyl sulfate","C2H6O4S","77-78-1","C2H6O4S","SG","SG-8562","Fixed","GD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm"]
["Dimethyl sulfate","C2H6O4S","77-78-1","C2H6O4S","SG","SG-8562","Fixed","SD-1GH Series","0～200ppm/0～300ppm/0～500ppm"]
["Dimethyl sulfate","C2H6O4S","77-78-1","C2H6O4S","SG","SG-8562","Fixed","SD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm"]
["Dimethyl sulfoxide","DMSO","67-68-5","C2H6OS","SG","SG-8521","Fixed","GD-A80V Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Dimethyl sulfoxide","DMSO","67-68-5","C2H6OS","SG","SG-8521","Fixed","GD-D58・GH Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Dimethyl sulfoxide","DMSO","67-68-5","C2H6OS","SG","SG-8521","Fixed","SD-1GH Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Dimethyl sulfoxide","DMSO","67-68-5","C2H6OS","SG","SG-8521","Fixed","SD-D58・GH Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Dimethylamine","DMA","124-40-3","C2H7N","ES","ESM-23RVM","Portable","SC-8000","0.2～15ppm"]
["Dimethylamine","DMA","124-40-3","C2H7N","ES","ESU-23RV-EX","Fixed","GD-70D Series","0.9～15ppm","Export limited：unable to measure under 6%FS"]
["Dimethylamine","DMA","124-40-3","C2H7N","ES","ESU-23RV-EX","Fixed","TP-70D","0.9～15ppm","Export limited：unable to measure under 6%FS"]
["Dimethylamine","DMA","124-40-3","C2H7N","ES","ESU-23RVM-EX","Fixed","GD-70D Series","0.9～15ppm","Updated against electrolyte reduction/Export limited：unable to measure under 6%FS"]
["Dimethylamine","DMA","124-40-3","C2H7N","ES","ESU-23RVM-EX","Fixed","TP-70D","0.9～15ppm","Updated against electrolyte reduction/Export limited：unable to measure under 6%FS"]
["Dimethylamine","DMA","124-40-3","C2H7N","ES","ESM-23RV","Fixed","GD-K88Ai Series","0～15ppm"]
["Dimethylamine","DMA","124-40-3","C2H7N","ES","ESM-23RV","Fixed","GD-K88Di Series","0～15ppm"]
["Dimethylamine","DMA","124-40-3","C2H7N","ES","ESM-23RVM","Fixed","GD-K88Ai Series","0.9～15ppm","Updated against electrolyte reduction/Export limited：unable to measure under 6%FS"]
["Dimethylamine","DMA","124-40-3","C2H7N","ES","ESM-23RVM","Fixed","GD-K88Di Series","0.9～15ppm","Updated against electrolyte reduction/Export limited：unable to measure under 6%FS"]
["Dimethylamine","DMA","124-40-3","C2H7N","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Dimethylamine","DMA","124-40-3","C2H7N","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Dimethylamine","DMA","124-40-3","C2H7N","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～28000ppm"]
["Dimethylamine","DMA","124-40-3","C2H7N","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～28000ppm"]
["Dimethylamine","DMA","124-40-3","C2H7N","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～28000ppm"]
["Dimethylamine","DMA","124-40-3","C2H7N","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～28000ppm"]
["Dimethylamine","DMA","124-40-3","C2H7N","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～28000ppm"]
["Dimethylamine","DMA","124-40-3","C2H7N","SG","SG-8521","Fixed","GD-A80V Series","0～30ppm/0～50ppm/0～100ppm/0～200ppm/0～300ppm"]
["Dimethylamine","DMA","124-40-3","C2H7N","SG","SG-8521","Fixed","GD-D58・GH Series","0～30ppm/0～50ppm/0～100ppm/0～200ppm/0～300ppm"]
["Dimethylamine","DMA","124-40-3","C2H7N","SG","SG-8521","Fixed","SD-1GH Series","0～30ppm/0～50ppm/0～100ppm/0～200ppm/0～300ppm"]
["Dimethylamine","DMA","124-40-3","C2H7N","SG","SG-8521","Fixed","SD-D58・GH Series","0～30ppm/0～50ppm/0～100ppm/0～200ppm/0～300ppm"]
["Dimethylamine","DMA","124-40-3","C2H7N","SG","SG-8562","Fixed","GD-A80V Series","0～30ppm/0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm","Standard sensor: SG-8521"]
["Dimethylamine","DMA","124-40-3","C2H7N","SG","SG-8562","Fixed","GD-D58・GH Series","0～30ppm/0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm","Standard sensor: SG-8521"]
["Dimethylamine","DMA","124-40-3","C2H7N","SG","SG-8562","Fixed","SD-1GH Series","0～30ppm/0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm","Standard sensor: SG-8521"]
["Dimethylamine","DMA","124-40-3","C2H7N","SG","SG-8562","Fixed","SD-D58・GH Series","0～30ppm/0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm","Standard sensor: SG-8521"]
["Dimethylaminopropylamine","DMAPA","109-55-7","C5H14N2","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Dimethylaminopropylamine","DMAPA","109-55-7","C5H14N2","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Dimethylaminopropylamine","DMAPA","109-55-7","C5H14N2","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～23000ppm"]
["Dimethylaminopropylamine","DMAPA","109-55-7","C5H14N2","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～23000ppm"]
["Dimethylaminopropylamine","DMAPA","109-55-7","C5H14N2","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～23000ppm"]
["Dimethylaminopropylamine","DMAPA","109-55-7","C5H14N2","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～23000ppm"]
["Dimethylaminopropylamine","DMAPA","109-55-7","C5H14N2","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～23000ppm"]
["Dimethylformamide","DMF","68-12-2","C3H7NO","SG","SGU-8563","Fixed","GD-70D Series","0～50ppm"]
["Dimethylformamide","DMF","68-12-2","C3H7NO","SG","SGU-8563","Fixed","TP-70D","0～50ppm"]
["Dimethylformamide","DMF","68-12-2","C3H7NO","HW","NC-6211","Fixed","GD-A80 Series","～50%LEL/～9000ppm"]
["Dimethylformamide","DMF","68-12-2","C3H7NO","HW","NC-6211","Fixed","GD-D58(TYPE GP) Series","～50%LEL/～9000ppm"]
["Dimethylformamide","DMF","68-12-2","C3H7NO","HW","NC-6211","Fixed","GD-D58(TYPE NC) Series","～50%LEL/～9000ppm"]
["Dimethylformamide","DMF","68-12-2","C3H7NO","HW","NC-6211","Fixed","SD-1(TYPE NC) Series","～50%LEL/～9000ppm"]
["Dimethylformamide","DMF","68-12-2","C3H7NO","HW","NC-6211","Fixed","SD-D58(TYPE NC) Series","～50%LEL/～9000ppm"]
["Dimethylformamide","DMF","68-12-2","C3H7NO","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Dimethylformamide","DMF","68-12-2","C3H7NO","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Dimethylformamide","DMF","68-12-2","C3H7NO","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Dimethylformamide","DMF","68-12-2","C3H7NO","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Dimethylformamide","DMF","68-12-2","C3H7NO","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Dimethylformamide","DMF","68-12-2","C3H7NO","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Dimethylformamide","DMF","68-12-2","C3H7NO","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Dimethylformamide","DMF","68-12-2","C3H7NO","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["Dimethylformamide","DMF","68-12-2","C3H7NO","SG","SG-8521","Fixed","GD-A80V Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm","Standard sensor: SG-8563"]
["Dimethylformamide","DMF","68-12-2","C3H7NO","SG","SG-8521","Fixed","GD-D58・GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm","Standard sensor: SG-8563"]
["Dimethylformamide","DMF","68-12-2","C3H7NO","SG","SG-8521","Fixed","SD-1GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm","Standard sensor: SG-8563"]
["Dimethylformamide","DMF","68-12-2","C3H7NO","SG","SG-8521","Fixed","SD-D58・GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm","Standard sensor: SG-8563"]
["Dimethylformamide","DMF","68-12-2","C3H7NO","SG","SG-8563","Fixed","GD-A80V Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Dimethylformamide","DMF","68-12-2","C3H7NO","SG","SG-8563","Fixed","GD-D58・GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Dimethylformamide","DMF","68-12-2","C3H7NO","SG","SG-8563","Fixed","SD-1GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Dimethylformamide","DMF","68-12-2","C3H7NO","SG","SG-8563","Fixed","SD-D58・GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Dioxane","C4H8O2","123-91-1","C4H8O2","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Dioxane","C4H8O2","123-91-1","C4H8O2","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Dioxane","C4H8O2","123-91-1","C4H8O2","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～19000ppm"]
["Dioxane","C4H8O2","123-91-1","C4H8O2","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～19000ppm"]
["Dioxane","C4H8O2","123-91-1","C4H8O2","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～19000ppm"]
["Dioxane","C4H8O2","123-91-1","C4H8O2","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～19000ppm"]
["Dioxane","C4H8O2","123-91-1","C4H8O2","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～19000ppm"]
["Dioxane","C4H8O2","123-91-1","C4H8O2","SG","SG-8511","Fixed","GD-A80V Series","0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Dioxane","C4H8O2","123-91-1","C4H8O2","SG","SG-8511","Fixed","GD-D58・GH Series","0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Dioxane","C4H8O2","123-91-1","C4H8O2","SG","SG-8511","Fixed","SD-1GH Series","0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Dioxane","C4H8O2","123-91-1","C4H8O2","SG","SG-8511","Fixed","SD-D58・GH Series","0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Dioxane","C4H8O2","123-91-1","C4H8O2","SG","SG-8521","Fixed","GD-A80V Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["Dioxane","C4H8O2","123-91-1","C4H8O2","SG","SG-8521","Fixed","GD-D58・GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["Dioxane","C4H8O2","123-91-1","C4H8O2","SG","SG-8521","Fixed","SD-1GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["Dioxane","C4H8O2","123-91-1","C4H8O2","SG","SG-8521","Fixed","SD-D58・GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["Disilane","Si2H6","1590-87-0","Si2H6","ES","ESM-23DH","Portable","SC-8000","0～15ppm"]
["Disilane","Si2H6","1590-87-0","Si2H6","ES","ESU-23AH","Fixed","GD-70D Series","0～15ppm"]
["Disilane","Si2H6","1590-87-0","Si2H6","ES","ESU-23AH","Fixed","TP-70D","0～15ppm"]
["Disilane","Si2H6","1590-87-0","Si2H6","ES","ESU-23DH","Fixed","GD-70D Series","0～15ppm"]
["Disilane","Si2H6","1590-87-0","Si2H6","ES","ESU-23DH","Fixed","TP-70D","0～15ppm"]
["Disilane","Si2H6","1590-87-0","Si2H6","ES","ESM-23AH","Fixed","GD-K88Ai Series","0～15ppm"]
["Disilane","Si2H6","1590-87-0","Si2H6","ES","ESM-23AH","Fixed","GD-K88Di Series","0～15ppm"]
["Disilane","Si2H6","1590-87-0","Si2H6","ES","ESM-23DH","Fixed","GD-K88Ai Series","0～15ppm"]
["Disilane","Si2H6","1590-87-0","Si2H6","ES","ESM-23DH","Fixed","GD-K88Di Series","0～15ppm"]
["Divinyl benzene","DVB","1321-74-0","C10H10","SG","SG-8521","Fixed","GD-A80V Series","0～300ppm/0～500ppm/0～1000ppm"]
["Divinyl benzene","DVB","1321-74-0","C10H10","SG","SG-8521","Fixed","GD-D58・GH Series","0～300ppm/0～500ppm/0～1000ppm"]
["Divinyl benzene","DVB","1321-74-0","C10H10","SG","SG-8521","Fixed","SD-1GH Series","0～300ppm/0～500ppm/0～1000ppm"]
["Divinyl benzene","DVB","1321-74-0","C10H10","SG","SG-8521","Fixed","SD-D58・GH Series","0～300ppm/0～500ppm/0～1000ppm"]
["Dodecane","C12H26","112-40-3","C12H26","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Dodecane","C12H26","112-40-3","C12H26","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Dodecane","C12H26","112-40-3","C12H26","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Dodecane","C12H26","112-40-3","C12H26","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Dodecane","C12H26","112-40-3","C12H26","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Dodecane","C12H26","112-40-3","C12H26","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Dodecane","C12H26","112-40-3","C12H26","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Dodecane","C12H26","112-40-3","C12H26","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["Dodecane","C12H26","112-40-3","C12H26","SG","SG-8521","Fixed","GD-A80V Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm"]
["Dodecane","C12H26","112-40-3","C12H26","SG","SG-8521","Fixed","GD-D58・GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm"]
["Dodecane","C12H26","112-40-3","C12H26","SG","SG-8521","Fixed","SD-1GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm"]
["Dodecane","C12H26","112-40-3","C12H26","SG","SG-8521","Fixed","SD-D58・GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm"]
["Epichlorohydrin","C3H5OCL","106-89-8","C3H5OCL","SG","SG-8523","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm"]
["Epichlorohydrin","C3H5OCL","106-89-8","C3H5OCL","SG","SG-8523","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm"]
["Epichlorohydrin","C3H5OCL","106-89-8","C3H5OCL","SG","SG-8523","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm"]
["Epichlorohydrin","C3H5OCL","106-89-8","C3H5OCL","SG","SG-8523","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm"]
["Ethane","C2H6","74-84-0","C2H6","HW","NC-6215","Portable","GP-1000(CH4)","0～100%LEL"]
["Ethane","C2H6","74-84-0","C2H6","HW","NC-6307","Portable","NC-1000(CH4)","0～10000ppm"]
["Ethane","C2H6","74-84-0","C2H6","SH","SH-8661","Portable","SP-220(TYPE H2)","0～10000ppm"]
["Ethane","C2H6","74-84-0","C2H6","SG","SGU-8521","Fixed","GD-70D Series","0～2000ppm"]
["Ethane","C2H6","74-84-0","C2H6","SG","SGU-8521","Fixed","TP-70D","0～2000ppm"]
["Ethane","C2H6","74-84-0","C2H6","HW","NCU-6211","Fixed","GD-70D Series","0～100%LEL","Confirm that GD-70D is non-explosion proof"]
["Ethane","C2H6","74-84-0","C2H6","HW","NCU-6211","Fixed","TP-70D","0～100%LEL","Confirm that GD-70D is non-explosion proof"]
["Ethane","C2H6","74-84-0","C2H6","RI","DE-3315-2","Fixed","SD-1RI Series","0～100%LEL"]
["Ethane","C2H6","74-84-0","C2H6","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Ethane","C2H6","74-84-0","C2H6","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Ethane","C2H6","74-84-0","C2H6","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～30000ppm"]
["Ethane","C2H6","74-84-0","C2H6","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～30000ppm"]
["Ethane","C2H6","74-84-0","C2H6","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～30000ppm"]
["Ethane","C2H6","74-84-0","C2H6","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～30000ppm"]
["Ethane","C2H6","74-84-0","C2H6","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～30000ppm"]
["Ethane","C2H6","74-84-0","C2H6","HW","HW-6239","Fixed","GD-A80-70 Series","0～100%LEL"]
["Ethane","C2H6","74-84-0","C2H6","HW","HW-6239","Fixed","SD-1(TYPE GP) Series","0～100%LEL"]
["Ethane","C2H6","74-84-0","C2H6","HW","HW-6239","Fixed","SD-D58(TYPE GP) Series","0～100%LEL"]
["Ethane","C2H6","74-84-0","C2H6","HW","HW-6239/NC-6239","Fixed","GD-A80 Series","0～100%LEL/0～30000ppm"]
["Ethane","C2H6","74-84-0","C2H6","HW","HW-6239/NC-6239","Fixed","GD-D58(TYPE GP) Series","0～100%LEL/0～30000ppm"]
["Ethane","C2H6","74-84-0","C2H6","HW","HW-6239/NC-6239","Fixed","GD-D58(TYPE NC) Series","0～100%LEL/0～30000ppm"]
["Ethane","C2H6","74-84-0","C2H6","HW","HW-6239/NC-6239","Fixed","SD-1(TYPE NC) Series","0～100%LEL/0～30000ppm"]
["Ethane","C2H6","74-84-0","C2H6","HW","HW-6239/NC-6239","Fixed","SD-D58(TYPE NC) Series","0～100%LEL/0～30000ppm"]
["Ethane","C2H6","74-84-0","C2H6","SG","SG-8521","Fixed","GD-A80V Series","0～1000ppm/0～2000ppm/0～2500ppm/0～3000ppm/0～5000ppm/0～10000ppm"]
["Ethane","C2H6","74-84-0","C2H6","SG","SG-8521","Fixed","GD-D58・GH Series","0～1000ppm/0～2000ppm/0～2500ppm/0～3000ppm/0～5000ppm/0～10000ppm"]
["Ethane","C2H6","74-84-0","C2H6","SG","SG-8521","Fixed","SD-1GH Series","0～1000ppm/0～2000ppm/0～2500ppm/0～3000ppm/0～5000ppm/0～10000ppm"]
["Ethane","C2H6","74-84-0","C2H6","SG","SG-8521","Fixed","SD-D58・GH Series","0～1000ppm/0～2000ppm/0～2500ppm/0～3000ppm/0～5000ppm/0～10000ppm"]
["Ethane","C2H6","74-84-0","C2H6","SG","SG-8582","Fixed","GD-A80V Series","0～500ppm/0～1000ppm/0～2000ppm"]
["Ethane","C2H6","74-84-0","C2H6","SG","SG-8582","Fixed","GD-D58・GH Series","0～500ppm/0～1000ppm/0～2000ppm"]
["Ethane","C2H6","74-84-0","C2H6","SG","SG-8582","Fixed","SD-1GH Series","0～500ppm/0～1000ppm/0～2000ppm"]
["Ethane","C2H6","74-84-0","C2H6","SG","SG-8582","Fixed","SD-D58・GH Series","0～500ppm/0～1000ppm/0～2000ppm"]
["Ethanol","C2H5OH","64-17-5","C2H6O","HW","NC-6215","Portable","GP-1000(HC/CH4)","0～100%LEL"]
["Ethanol","C2H5OH","64-17-5","C2H6O","HW","NC-6307","Portable","NC-1000(HC/CH4)","0～10000ppm"]
["Ethanol","C2H5OH","64-17-5","C2H6O","SH","SH-8662","Portable","SP-220(TYPE SC)","0～10ppm"]
["Ethanol","C2H5OH","64-17-5","C2H6O","SG","SGU-8521","Fixed","GD-70D Series","0～2000ppm"]
["Ethanol","C2H5OH","64-17-5","C2H6O","SG","SGU-8521","Fixed","TP-70D","0～2000ppm"]
["Ethanol","C2H5OH","64-17-5","C2H6O","HW","NCU-6211","Fixed","GD-70D Series","0～100%LEL","Confirm that GD-70D is non-explosion proof"]
["Ethanol","C2H5OH","64-17-5","C2H6O","HW","NCU-6211","Fixed","TP-70D","0～100%LEL","Confirm that GD-70D is non-explosion proof"]
["Ethanol","C2H5OH","64-17-5","C2H6O","RI","DE-3315-2","Fixed","SD-1RI Series","0～100%LEL"]
["Ethanol","C2H5OH","64-17-5","C2H6O","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Ethanol","C2H5OH","64-17-5","C2H6O","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Ethanol","C2H5OH","64-17-5","C2H6O","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～330000ppm"]
["Ethanol","C2H5OH","64-17-5","C2H6O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～330000ppm"]
["Ethanol","C2H5OH","64-17-5","C2H6O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～330000ppm"]
["Ethanol","C2H5OH","64-17-5","C2H6O","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～330000ppm"]
["Ethanol","C2H5OH","64-17-5","C2H6O","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～330000ppm"]
["Ethanol","C2H5OH","64-17-5","C2H6O","HW","HW-6213/NC-6213","Fixed","GD-A80 Series","0～100%LEL/0～33000ppm"]
["Ethanol","C2H5OH","64-17-5","C2H6O","HW","HW-6213/NC-6213","Fixed","GD-D58(TYPE GP) Series","0～100%LEL/0～33000ppm"]
["Ethanol","C2H5OH","64-17-5","C2H6O","HW","HW-6213/NC-6213","Fixed","GD-D58(TYPE NC) Series","0～100%LEL/0～33000ppm"]
["Ethanol","C2H5OH","64-17-5","C2H6O","HW","NC-6250","Fixed","GD-A80 Series","0～100%LEL/0～33000ppm"]
["Ethanol","C2H5OH","64-17-5","C2H6O","HW","NC-6250","Fixed","GD-D58(TYPE NC) Series","0～100%LEL/0～33000ppm"]
["Ethanol","C2H5OH","64-17-5","C2H6O","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Ethanol","C2H5OH","64-17-5","C2H6O","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Ethanol","C2H5OH","64-17-5","C2H6O","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Ethanol","C2H5OH","64-17-5","C2H6O","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Ethanol","C2H5OH","64-17-5","C2H6O","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Ethanol","C2H5OH","64-17-5","C2H6O","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Ethanol","C2H5OH","64-17-5","C2H6O","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Ethanol","C2H5OH","64-17-5","C2H6O","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["Ethanol","C2H5OH","64-17-5","C2H6O","SG","SG-8521","Fixed","GD-A80V Series","★0～30ppm/★0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/◆0～3000ppm","★Range easily affected by environmental conditions and other, ◆Accuracy near the F.S. concentration range is likely to deteriorate"]
["Ethanol","C2H5OH","64-17-5","C2H6O","SG","SG-8521","Fixed","GD-D58・GH Series","★0～30ppm/★0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/◆0～3000ppm","★Range easily affected by environmental conditions and other, ◆Accuracy near the F.S. concentration range is likely to deteriorate"]
["Ethanol","C2H5OH","64-17-5","C2H6O","SG","SG-8521","Fixed","SD-1GH Series","★0～30ppm/★0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/◆0～3000ppm","★Range easily affected by environmental conditions and other, ◆Accuracy near the F.S. concentration range is likely to deteriorate"]
["Ethanol","C2H5OH","64-17-5","C2H6O","SG","SG-8521","Fixed","SD-D58・GH Series","★0～30ppm/★0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/◆0～3000ppm","★Range easily affected by environmental conditions and other, ◆Accuracy near the F.S. concentration range is likely to deteriorate"]
["Ethanol","C2H5OH","64-17-5","C2H6O","SG","SG-8565","Fixed","GD-A80V Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～4000ppm/0～5000ppm"]
["Ethanol","C2H5OH","64-17-5","C2H6O","SG","SG-8565","Fixed","GD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～4000ppm/0～5000ppm"]
["Ethanol","C2H5OH","64-17-5","C2H6O","SG","SG-8565","Fixed","SD-1GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～4000ppm/0～5000ppm"]
["Ethanol","C2H5OH","64-17-5","C2H6O","SG","SG-8565","Fixed","SD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～4000ppm/0～5000ppm"]
["Ethanolamine","C2H7NO","141-43-5","C2H7NO","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Ethanolamine","C2H7NO","141-43-5","C2H7NO","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Ethanolamine","C2H7NO","141-43-5","C2H7NO","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Ethanolamine","C2H7NO","141-43-5","C2H7NO","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Ethanolamine","C2H7NO","141-43-5","C2H7NO","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Ethanolamine","C2H7NO","141-43-5","C2H7NO","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Ethanolamine","C2H7NO","141-43-5","C2H7NO","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Ethanolamine","C2H7NO","141-43-5","C2H7NO","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["Ethanolamine","C2H7NO","141-43-5","C2H7NO","SG","SG-8562","Fixed","GD-A80V Series","0～100ppm/0～200ppm"]
["Ethanolamine","C2H7NO","141-43-5","C2H7NO","SG","SG-8562","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm"]
["Ethanolamine","C2H7NO","141-43-5","C2H7NO","SG","SG-8562","Fixed","SD-1GH Series","0～100ppm/0～200ppm"]
["Ethanolamine","C2H7NO","141-43-5","C2H7NO","SG","SG-8562","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm"]
["Ethyl 3-Ethoxypropionate","EtEP","763-69-9","C7H14O3","SG","SG-8521","Fixed","GD-A80V Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Ethyl 3-Ethoxypropionate","EtEP","763-69-9","C7H14O3","SG","SG-8521","Fixed","GD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Ethyl 3-Ethoxypropionate","EtEP","763-69-9","C7H14O3","SG","SG-8521","Fixed","SD-1GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Ethyl 3-Ethoxypropionate","EtEP","763-69-9","C7H14O3","SG","SG-8521","Fixed","SD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Ethyl Acetate","EtAc","141-78-6","C4H8O2","HW","NC-6215","Portable","GP-1000(HC/CH4)","0～100%LEL"]
["Ethyl Acetate","EtAc","141-78-6","C4H8O2","HW","NC-6307","Portable","NC-1000(HC/CH4)","0～10000ppm"]
["Ethyl Acetate","EtAc","141-78-6","C4H8O2","SG","SGU-8511","Fixed","GD-70D Series","0～2000ppm"]
["Ethyl Acetate","EtAc","141-78-6","C4H8O2","SG","SGU-8511","Fixed","TP-70D","0～2000ppm"]
["Ethyl Acetate","EtAc","141-78-6","C4H8O2","RI","DE-3315-2","Fixed","SD-1RI Series","0～100%LEL"]
["Ethyl Acetate","EtAc","141-78-6","C4H8O2","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Ethyl Acetate","EtAc","141-78-6","C4H8O2","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Ethyl Acetate","EtAc","141-78-6","C4H8O2","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～21000ppm"]
["Ethyl Acetate","EtAc","141-78-6","C4H8O2","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～21000ppm"]
["Ethyl Acetate","EtAc","141-78-6","C4H8O2","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～21000ppm"]
["Ethyl Acetate","EtAc","141-78-6","C4H8O2","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～21000ppm"]
["Ethyl Acetate","EtAc","141-78-6","C4H8O2","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～21000ppm"]
["Ethyl Acetate","EtAc","141-78-6","C4H8O2","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Ethyl Acetate","EtAc","141-78-6","C4H8O2","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Ethyl Acetate","EtAc","141-78-6","C4H8O2","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Ethyl Acetate","EtAc","141-78-6","C4H8O2","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Ethyl Acetate","EtAc","141-78-6","C4H8O2","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Ethyl Acetate","EtAc","141-78-6","C4H8O2","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Ethyl Acetate","EtAc","141-78-6","C4H8O2","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Ethyl Acetate","EtAc","141-78-6","C4H8O2","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["Ethyl Acetate","EtAc","141-78-6","C4H8O2","SG","SG-8511","Fixed","GD-A80V Series","0～2000ppm/0～3000ppm/0～5000ppm"]
["Ethyl Acetate","EtAc","141-78-6","C4H8O2","SG","SG-8511","Fixed","GD-D58・GH Series","0～2000ppm/0～3000ppm/0～5000ppm"]
["Ethyl Acetate","EtAc","141-78-6","C4H8O2","SG","SG-8511","Fixed","SD-1GH Series","0～2000ppm/0～3000ppm/0～5000ppm"]
["Ethyl Acetate","EtAc","141-78-6","C4H8O2","SG","SG-8511","Fixed","SD-D58・GH Series","0～2000ppm/0～3000ppm/0～5000ppm"]
["Ethyl Acetate","EtAc","141-78-6","C4H8O2","SG","SG-8521","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Ethyl Acetate","EtAc","141-78-6","C4H8O2","SG","SG-8521","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Ethyl Acetate","EtAc","141-78-6","C4H8O2","SG","SG-8521","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Ethyl Acetate","EtAc","141-78-6","C4H8O2","SG","SG-8521","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Ethyl acrylate","C5H8O2","140-88-5","C5H8O2","HW","NC-6215","Portable","GP-1000(Specified cal.gas)","0～100%LEL"]
["Ethyl acrylate","C5H8O2","140-88-5","C5H8O2","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Ethyl acrylate","C5H8O2","140-88-5","C5H8O2","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Ethyl acrylate","C5H8O2","140-88-5","C5H8O2","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～14000ppm"]
["Ethyl acrylate","C5H8O2","140-88-5","C5H8O2","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～14000ppm"]
["Ethyl acrylate","C5H8O2","140-88-5","C5H8O2","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～14000ppm"]
["Ethyl acrylate","C5H8O2","140-88-5","C5H8O2","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～14000ppm"]
["Ethyl acrylate","C5H8O2","140-88-5","C5H8O2","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～14000ppm"]
["Ethyl acrylate","C5H8O2","140-88-5","C5H8O2","SG","SG-8521","Fixed","GD-A80V Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Ethyl acrylate","C5H8O2","140-88-5","C5H8O2","SG","SG-8521","Fixed","GD-D58・GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Ethyl acrylate","C5H8O2","140-88-5","C5H8O2","SG","SG-8521","Fixed","SD-1GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Ethyl acrylate","C5H8O2","140-88-5","C5H8O2","SG","SG-8521","Fixed","SD-D58・GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Ethyl benzene","EtBenz","100-41-4","C8H10","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Ethyl benzene","EtBenz","100-41-4","C8H10","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Ethyl benzene","EtBenz","100-41-4","C8H10","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～10000ppm"]
["Ethyl benzene","EtBenz","100-41-4","C8H10","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～10000ppm"]
["Ethyl benzene","EtBenz","100-41-4","C8H10","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～10000ppm"]
["Ethyl benzene","EtBenz","100-41-4","C8H10","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～10000ppm"]
["Ethyl benzene","EtBenz","100-41-4","C8H10","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～10000ppm"]
["Ethyl benzene","EtBenz","100-41-4","C8H10","SG","SG-8521","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Ethyl benzene","EtBenz","100-41-4","C8H10","SG","SG-8521","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Ethyl benzene","EtBenz","100-41-4","C8H10","SG","SG-8521","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Ethyl benzene","EtBenz","100-41-4","C8H10","SG","SG-8521","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Ethyl chloride","C2H5CL","75-00-3","C2H5CL","SG","SG-8523","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm"]
["Ethyl chloride","C2H5CL","75-00-3","C2H5CL","SG","SG-8523","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm"]
["Ethyl chloride","C2H5CL","75-00-3","C2H5CL","SG","SG-8523","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm"]
["Ethyl chloride","C2H5CL","75-00-3","C2H5CL","SG","SG-8523","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm"]
["Ethyl ether","C4H10O","60-29-7","C4H10O","HW","NC-6215","Portable","GP-1000(Specified cal.gas)","0～100%LEL"]
["Ethyl ether","C4H10O","60-29-7","C4H10O","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Ethyl ether","C4H10O","60-29-7","C4H10O","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Ethyl ether","C4H10O","60-29-7","C4H10O","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～17000ppm"]
["Ethyl ether","C4H10O","60-29-7","C4H10O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～17000ppm"]
["Ethyl ether","C4H10O","60-29-7","C4H10O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～17000ppm"]
["Ethyl ether","C4H10O","60-29-7","C4H10O","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～17000ppm"]
["Ethyl ether","C4H10O","60-29-7","C4H10O","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～17000ppm"]
["Ethyl ether","C4H10O","60-29-7","C4H10O","SG","SG-8521","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Ethyl ether","C4H10O","60-29-7","C4H10O","SG","SG-8521","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Ethyl ether","C4H10O","60-29-7","C4H10O","SG","SG-8521","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Ethyl ether","C4H10O","60-29-7","C4H10O","SG","SG-8521","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Ethyl lactate","LAE","97-64-3","C5H10O3","SG","SGU-8521","Fixed","GD-70D Series","0～5000ppm"]
["Ethyl lactate","LAE","97-64-3","C5H10O3","SG","SGU-8521","Fixed","TP-70D","0～5000ppm"]
["Ethyl lactate","LAE","97-64-3","C5H10O3","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Ethyl lactate","LAE","97-64-3","C5H10O3","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Ethyl lactate","LAE","97-64-3","C5H10O3","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Ethyl lactate","LAE","97-64-3","C5H10O3","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Ethyl lactate","LAE","97-64-3","C5H10O3","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Ethyl lactate","LAE","97-64-3","C5H10O3","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Ethyl lactate","LAE","97-64-3","C5H10O3","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Ethyl lactate","LAE","97-64-3","C5H10O3","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["Ethyl lactate","LAE","97-64-3","C5H10O3","SG","SG-8521","Fixed","GD-A80V Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Ethyl lactate","LAE","97-64-3","C5H10O3","SG","SG-8521","Fixed","GD-D58・GH Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Ethyl lactate","LAE","97-64-3","C5H10O3","SG","SG-8521","Fixed","SD-1GH Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Ethyl lactate","LAE","97-64-3","C5H10O3","SG","SG-8521","Fixed","SD-D58・GH Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Ethyl mercaptan","C2H5SH","75-08-1","C2H6S","SG","SG-8562","Fixed","GD-A80V Series","0～30ppm/0～50ppm/0～100ppm"]
["Ethyl mercaptan","C2H5SH","75-08-1","C2H6S","SG","SG-8562","Fixed","GD-D58・GH Series","0～30ppm/0～50ppm/0～100ppm"]
["Ethyl mercaptan","C2H5SH","75-08-1","C2H6S","SG","SG-8562","Fixed","SD-1GH Series","0～30ppm/0～50ppm/0～100ppm"]
["Ethyl mercaptan","C2H5SH","75-08-1","C2H6S","SG","SG-8562","Fixed","SD-D58・GH Series","0～30ppm/0～50ppm/0～100ppm"]
["Ethyl Methyl Carbonate","EMC","623-53-0","C4H8O3","RI","DE-3315-1","Fixed","SD-1RI Series","0～100%LEL"]
["Ethyl Methyl Carbonate","EMC","623-53-0","C4H8O3","SG","SG-8521","Fixed","GD-A80V Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Ethyl Methyl Carbonate","EMC","623-53-0","C4H8O3","SG","SG-8521","Fixed","GD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Ethyl Methyl Carbonate","EMC","623-53-0","C4H8O3","SG","SG-8521","Fixed","SD-1GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Ethyl Methyl Carbonate","EMC","623-53-0","C4H8O3","SG","SG-8521","Fixed","SD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Ethyｌ tert-butyl ether","ETBE","637-92-3","C6H14O","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Ethyｌ tert-butyl ether","ETBE","637-92-3","C6H14O","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Ethyｌ tert-butyl ether","ETBE","637-92-3","C6H14O","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～12000ppm"]
["Ethyｌ tert-butyl ether","ETBE","637-92-3","C6H14O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～12000ppm"]
["Ethyｌ tert-butyl ether","ETBE","637-92-3","C6H14O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～12000ppm"]
["Ethyｌ tert-butyl ether","ETBE","637-92-3","C6H14O","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～12000ppm"]
["Ethyｌ tert-butyl ether","ETBE","637-92-3","C6H14O","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～12000ppm"]
["Ethyl Vinyl Ether","VEE","109-92-2","C4H8O","SG","SG-8521","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Ethyl Vinyl Ether","VEE","109-92-2","C4H8O","SG","SG-8521","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Ethyl Vinyl Ether","VEE","109-92-2","C4H8O","SG","SG-8521","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Ethyl Vinyl Ether","VEE","109-92-2","C4H8O","SG","SG-8521","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Ethyl-1,3-cyclopentadiene","EtCPD","26519-92-6","C7H10","SG","SG-8511","Fixed","GD-A80V Series","0～2000ppm/0～3000ppm/0～5000ppm"]
["Ethyl-1,3-cyclopentadiene","EtCPD","26519-92-6","C7H10","SG","SG-8511","Fixed","GD-D58・GH Series","0～2000ppm/0～3000ppm/0～5000ppm"]
["Ethyl-1,3-cyclopentadiene","EtCPD","26519-92-6","C7H10","SG","SG-8511","Fixed","SD-1GH Series","0～2000ppm/0～3000ppm/0～5000ppm"]
["Ethyl-1,3-cyclopentadiene","EtCPD","26519-92-6","C7H10","SG","SG-8511","Fixed","SD-D58・GH Series","0～2000ppm/0～3000ppm/0～5000ppm"]
["Ethylamine","C2H5NH2","75-04-7","C2H7N","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Ethylamine","C2H5NH2","75-04-7","C2H7N","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Ethylamine","C2H5NH2","75-04-7","C2H7N","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～35000ppm"]
["Ethylamine","C2H5NH2","75-04-7","C2H7N","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～35000ppm"]
["Ethylamine","C2H5NH2","75-04-7","C2H7N","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～35000ppm"]
["Ethylamine","C2H5NH2","75-04-7","C2H7N","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～35000ppm"]
["Ethylamine","C2H5NH2","75-04-7","C2H7N","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～35000ppm"]
["Ethylcyclohexane","C8H16","1678-91-7","C8H16","SG","SGU-8521","Fixed","GD-70D Series","0～2000ppm"]
["Ethylcyclohexane","C8H16","1678-91-7","C8H16","SG","SGU-8521","Fixed","TP-70D","0～2000ppm"]
["Ethylcyclohexane","C8H16","1678-91-7","C8H16","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Ethylcyclohexane","C8H16","1678-91-7","C8H16","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Ethylcyclohexane","C8H16","1678-91-7","C8H16","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～9000ppm"]
["Ethylcyclohexane","C8H16","1678-91-7","C8H16","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～9000ppm"]
["Ethylcyclohexane","C8H16","1678-91-7","C8H16","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～9000ppm"]
["Ethylcyclohexane","C8H16","1678-91-7","C8H16","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～9000ppm"]
["Ethylcyclohexane","C8H16","1678-91-7","C8H16","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～9000ppm"]
["Ethylcyclohexane","C8H16","1678-91-7","C8H16","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Ethylcyclohexane","C8H16","1678-91-7","C8H16","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Ethylcyclohexane","C8H16","1678-91-7","C8H16","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Ethylcyclohexane","C8H16","1678-91-7","C8H16","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Ethylcyclohexane","C8H16","1678-91-7","C8H16","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Ethylcyclohexane","C8H16","1678-91-7","C8H16","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Ethylcyclohexane","C8H16","1678-91-7","C8H16","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Ethylcyclohexane","C8H16","1678-91-7","C8H16","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["Ethylcyclohexane","C8H16","1678-91-7","C8H16","SG","SG-8521","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Ethylcyclohexane","C8H16","1678-91-7","C8H16","SG","SG-8521","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Ethylcyclohexane","C8H16","1678-91-7","C8H16","SG","SG-8521","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Ethylcyclohexane","C8H16","1678-91-7","C8H16","SG","SG-8521","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Ethylene","C2H4","74-85-1","C2H4","HW","NC-6215","Portable","GP-1000(HC/CH4)","0～100%LEL"]
["Ethylene","C2H4","74-85-1","C2H4","HW","NC-6307","Portable","NC-1000(HC/CH4)","0～10000ppm"]
["Ethylene","C2H4","74-85-1","C2H4","SH","SH-8662","Portable","SP-220(TYPE SC)","0～10ppm"]
["Ethylene","C2H4","74-85-1","C2H4","SH","SH-8661","Portable","SP-220(TYPE H2)","0～10000ppm"]
["Ethylene","C2H4","74-85-1","C2H4","SG","SGU-8521","Fixed","GD-70D Series","0～500ppm"]
["Ethylene","C2H4","74-85-1","C2H4","SG","SGU-8521","Fixed","TP-70D","0～500ppm"]
["Ethylene","C2H4","74-85-1","C2H4","SG","SGU-8521","Fixed","GD-70D Series","0～1000ppm"]
["Ethylene","C2H4","74-85-1","C2H4","SG","SGU-8521","Fixed","TP-70D","0～1000ppm"]
["Ethylene","C2H4","74-85-1","C2H4","SG","SGU-8521","Fixed","GD-70D Series","0～2000ppm"]
["Ethylene","C2H4","74-85-1","C2H4","SG","SGU-8521","Fixed","TP-70D","0～2000ppm"]
["Ethylene","C2H4","74-85-1","C2H4","SG","SGU-8582","Fixed","GD-70D Series","0～500ppm"]
["Ethylene","C2H4","74-85-1","C2H4","SG","SGU-8582","Fixed","TP-70D","0～500ppm"]
["Ethylene","C2H4","74-85-1","C2H4","HW","NCU-6211","Fixed","GD-70D Series","0～100%LEL","Confirm that GD-70D is non-explosion proof"]
["Ethylene","C2H4","74-85-1","C2H4","HW","NCU-6211","Fixed","TP-70D","0～100%LEL","Confirm that GD-70D is non-explosion proof"]
["Ethylene","C2H4","74-85-1","C2H4","RI","DE-3315-1","Fixed","SD-1RI Series","0～100%LEL"]
["Ethylene","C2H4","74-85-1","C2H4","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Ethylene","C2H4","74-85-1","C2H4","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Ethylene","C2H4","74-85-1","C2H4","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～27000ppm"]
["Ethylene","C2H4","74-85-1","C2H4","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～27000ppm"]
["Ethylene","C2H4","74-85-1","C2H4","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～27000ppm"]
["Ethylene","C2H4","74-85-1","C2H4","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～27000ppm"]
["Ethylene","C2H4","74-85-1","C2H4","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～27000ppm"]
["Ethylene","C2H4","74-85-1","C2H4","HW","HW-6213/NC-6213","Fixed","GD-A80 Series","0～100%LEL/0～27000ppm"]
["Ethylene","C2H4","74-85-1","C2H4","HW","HW-6213/NC-6213","Fixed","GD-D58(TYPE GP) Series","0～100%LEL/0～27000ppm"]
["Ethylene","C2H4","74-85-1","C2H4","HW","HW-6213/NC-6213","Fixed","GD-D58(TYPE NC) Series","0～100%LEL/0～27000ppm"]
["Ethylene","C2H4","74-85-1","C2H4","HW","HW-6239","Fixed","GD-A80-70 Series","0～100%LEL"]
["Ethylene","C2H4","74-85-1","C2H4","HW","HW-6239","Fixed","SD-1(TYPE GP) Series","0～100%LEL"]
["Ethylene","C2H4","74-85-1","C2H4","HW","HW-6239","Fixed","SD-D58(TYPE GP) Series","0～100%LEL"]
["Ethylene","C2H4","74-85-1","C2H4","HW","HW-6239/NC-6239","Fixed","GD-A80 Series","0～100%LEL/0～27000ppm"]
["Ethylene","C2H4","74-85-1","C2H4","HW","HW-6239/NC-6239","Fixed","GD-D58(TYPE GP) Series","0～100%LEL/0～27000ppm"]
["Ethylene","C2H4","74-85-1","C2H4","HW","HW-6239/NC-6239","Fixed","GD-D58(TYPE NC) Series","0～100%LEL/0～27000ppm"]
["Ethylene","C2H4","74-85-1","C2H4","HW","HW-6239/NC-6239","Fixed","SD-1(TYPE NC) Series","0～100%LEL/0～27000ppm"]
["Ethylene","C2H4","74-85-1","C2H4","HW","HW-6239/NC-6239","Fixed","SD-D58(TYPE NC) Series","0～100%LEL/0～27000ppm"]
["Ethylene","C2H4","74-85-1","C2H4","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Ethylene","C2H4","74-85-1","C2H4","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Ethylene","C2H4","74-85-1","C2H4","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Ethylene","C2H4","74-85-1","C2H4","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Ethylene","C2H4","74-85-1","C2H4","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Ethylene","C2H4","74-85-1","C2H4","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Ethylene","C2H4","74-85-1","C2H4","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Ethylene","C2H4","74-85-1","C2H4","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["Ethylene","C2H4","74-85-1","C2H4","SG","SG-8511","Fixed","GD-A80V Series","0～10000ppm"]
["Ethylene","C2H4","74-85-1","C2H4","SG","SG-8511","Fixed","GD-D58・GH Series","0～10000ppm"]
["Ethylene","C2H4","74-85-1","C2H4","SG","SG-8511","Fixed","SD-1GH Series","0～10000ppm"]
["Ethylene","C2H4","74-85-1","C2H4","SG","SG-8511","Fixed","SD-D58・GH Series","0～10000ppm"]
["Ethylene","C2H4","74-85-1","C2H4","SG","SG-8521","Fixed","GD-A80V Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Ethylene","C2H4","74-85-1","C2H4","SG","SG-8521","Fixed","GD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Ethylene","C2H4","74-85-1","C2H4","SG","SG-8521","Fixed","SD-1GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Ethylene","C2H4","74-85-1","C2H4","SG","SG-8521","Fixed","SD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Ethylene","C2H4","74-85-1","C2H4","SG","SG-8582","Fixed","GD-A80V Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Ethylene","C2H4","74-85-1","C2H4","SG","SG-8582","Fixed","GD-D58・GH Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Ethylene","C2H4","74-85-1","C2H4","SG","SG-8582","Fixed","SD-1GH Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Ethylene","C2H4","74-85-1","C2H4","SG","SG-8582","Fixed","SD-D58・GH Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Ethylene dibromide","C2H4Br2","106-93-4","C2H4Br2","SH","SH-8662","Portable","SP-220(TYPE FUM)","0～30ppm"]
["Ethylene glycol","C2H6O2","107-21-1","C2H6O2","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Ethylene glycol","C2H6O2","107-21-1","C2H6O2","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Ethylene glycol","C2H6O2","107-21-1","C2H6O2","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Ethylene glycol","C2H6O2","107-21-1","C2H6O2","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Ethylene glycol","C2H6O2","107-21-1","C2H6O2","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Ethylene glycol","C2H6O2","107-21-1","C2H6O2","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Ethylene glycol","C2H6O2","107-21-1","C2H6O2","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Ethylene Glycol Dimethyl Ether","EGDME","110-71-4","C4H10O2","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Ethylene Glycol Dimethyl Ether","EGDME","110-71-4","C4H10O2","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Ethylene Glycol Dimethyl Ether","EGDME","110-71-4","C4H10O2","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～16000ppm"]
["Ethylene Glycol Dimethyl Ether","EGDME","110-71-4","C4H10O2","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～16000ppm"]
["Ethylene Glycol Dimethyl Ether","EGDME","110-71-4","C4H10O2","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～16000ppm"]
["Ethylene Glycol Dimethyl Ether","EGDME","110-71-4","C4H10O2","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～16000ppm"]
["Ethylene Glycol Dimethyl Ether","EGDME","110-71-4","C4H10O2","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～16000ppm"]
["Ethylene Glycol Dimethyl Ether","EGDME","110-71-4","C4H10O2","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Ethylene Glycol Dimethyl Ether","EGDME","110-71-4","C4H10O2","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Ethylene Glycol Dimethyl Ether","EGDME","110-71-4","C4H10O2","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Ethylene Glycol Dimethyl Ether","EGDME","110-71-4","C4H10O2","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Ethylene Glycol Dimethyl Ether","EGDME","110-71-4","C4H10O2","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Ethylene Glycol Dimethyl Ether","EGDME","110-71-4","C4H10O2","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Ethylene Glycol Dimethyl Ether","EGDME","110-71-4","C4H10O2","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Ethylene Glycol Dimethyl Ether","EGDME","110-71-4","C4H10O2","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["Ethylene Glycol Dimethyl Ether","EGDME","110-71-4","C4H10O2","SG","SG-8521","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm"]
["Ethylene Glycol Dimethyl Ether","EGDME","110-71-4","C4H10O2","SG","SG-8521","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm"]
["Ethylene Glycol Dimethyl Ether","EGDME","110-71-4","C4H10O2","SG","SG-8521","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm"]
["Ethylene Glycol Dimethyl Ether","EGDME","110-71-4","C4H10O2","SG","SG-8521","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm"]
["Ethylene oxide","EO","75-21-8","C2H4O","SH","SH-8662","Portable","SP-220(TYPE SC)","0～10ppm"]
["Ethylene oxide","EO","75-21-8","C2H4O","HW","NC-6215","Portable","GP-1000(Specified cal.gas)","0～100%LEL"]
["Ethylene oxide","EO","75-21-8","C2H4O","HW","NC-6307","Portable","NC-1000(Specified cal. Gas)","0～10000ppm"]
["Ethylene oxide","EO","75-21-8","C2H4O","SG","SGU-8563","Fixed","GD-70D Series","0～50ppm"]
["Ethylene oxide","EO","75-21-8","C2H4O","SG","SGU-8563","Fixed","TP-70D","0～50ppm"]
["Ethylene oxide","EO","75-21-8","C2H4O","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Ethylene oxide","EO","75-21-8","C2H4O","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Ethylene oxide","EO","75-21-8","C2H4O","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～30000ppm"]
["Ethylene oxide","EO","75-21-8","C2H4O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～30000ppm"]
["Ethylene oxide","EO","75-21-8","C2H4O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～30000ppm"]
["Ethylene oxide","EO","75-21-8","C2H4O","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～30000ppm"]
["Ethylene oxide","EO","75-21-8","C2H4O","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～30000ppm"]
["Ethylene oxide","EO","75-21-8","C2H4O","SG","SG-8521","Fixed","GD-A80V Series","0～50ppm/0～100ppm/0～150ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Ethylene oxide","EO","75-21-8","C2H4O","SG","SG-8521","Fixed","GD-D58・GH Series","0～50ppm/0～100ppm/0～150ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Ethylene oxide","EO","75-21-8","C2H4O","SG","SG-8521","Fixed","SD-1GH Series","0～50ppm/0～100ppm/0～150ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Ethylene oxide","EO","75-21-8","C2H4O","SG","SG-8521","Fixed","SD-D58・GH Series","0～50ppm/0～100ppm/0～150ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Ethylene oxide","EO","75-21-8","C2H4O","SG","SG-8563","Fixed","GD-A80V Series","0～20ppm/0～30ppm/0～50ppm/0～100ppm/0～150ppm/0～200ppm/0～300ppm/0～500ppm"]
["Ethylene oxide","EO","75-21-8","C2H4O","SG","SG-8563","Fixed","GD-D58・GH Series","0～20ppm/0～30ppm/0～50ppm/0～100ppm/0～150ppm/0～200ppm/0～300ppm/0～500ppm"]
["Ethylene oxide","EO","75-21-8","C2H4O","SG","SG-8563","Fixed","SD-1GH Series","0～20ppm/0～30ppm/0～50ppm/0～100ppm/0～150ppm/0～200ppm/0～300ppm/0～500ppm"]
["Ethylene oxide","EO","75-21-8","C2H4O","SG","SG-8563","Fixed","SD-D58・GH Series","0～20ppm/0～30ppm/0～50ppm/0～100ppm/0～150ppm/0～200ppm/0～300ppm/0～500ppm"]
["Ethylene oxide","EO","75-21-8","C2H4O","SG","SG-8563","Fixed","GD-A80V Series","0～1000ppm"]
["Ethylene oxide","EO","75-21-8","C2H4O","SG","SG-8563","Fixed","GD-D58・GH Series","0～1000ppm"]
["Ethylene oxide","EO","75-21-8","C2H4O","SG","SG-8563","Fixed","SD-1GH Series","0～1000ppm"]
["Ethylene oxide","EO","75-21-8","C2H4O","SG","SG-8563","Fixed","SD-D58・GH Series","0～1000ppm"]
["Ethylene oxide","EO","75-21-8","C2H4O","SG","SG-8563","Fixed","GD-A80V Series","0～75ppm"]
["Ethylene oxide","EO","75-21-8","C2H4O","SG","SG-8563","Fixed","GD-D58・GH Series","0～75ppm"]
["Ethylene oxide","EO","75-21-8","C2H4O","SG","SG-8563","Fixed","SD-1GH Series","0～75ppm"]
["Ethylene oxide","EO","75-21-8","C2H4O","SG","SG-8563","Fixed","SD-D58・GH Series","0～75ppm"]
["Ethylenediamine","C2H8N2","107-15-3","C2H8N2","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Ethylenediamine","C2H8N2","107-15-3","C2H8N2","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Ethylenediamine","C2H8N2","107-15-3","C2H8N2","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～27000ppm"]
["Ethylenediamine","C2H8N2","107-15-3","C2H8N2","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～27000ppm"]
["Ethylenediamine","C2H8N2","107-15-3","C2H8N2","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～27000ppm"]
["Ethylenediamine","C2H8N2","107-15-3","C2H8N2","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～27000ppm"]
["Ethylenediamine","C2H8N2","107-15-3","C2H8N2","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～27000ppm"]
["Ethylenediamine","C2H8N2","107-15-3","C2H8N2","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Ethylenediamine","C2H8N2","107-15-3","C2H8N2","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Ethylenediamine","C2H8N2","107-15-3","C2H8N2","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Ethylenediamine","C2H8N2","107-15-3","C2H8N2","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Ethylenediamine","C2H8N2","107-15-3","C2H8N2","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Ethylenediamine","C2H8N2","107-15-3","C2H8N2","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Ethylenediamine","C2H8N2","107-15-3","C2H8N2","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Ethylenediamine","C2H8N2","107-15-3","C2H8N2","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["Ethylmethylamine","EMA","624-78-2","C3H9N","ES","ESU-23RVM","Fixed","GD-70D Series","0～15ppm","Updated against electrolyte reduction"]
["Ethylmethylamine","EMA","624-78-2","C3H9N","ES","ESU-23RVM","Fixed","TP-70D","0～15ppm","Updated against electrolyte reduction"]
["Ethylmethylamine","EMA","624-78-2","C3H9N","ES","ESM-23RV","Fixed","GD-K88Ai Series","0～15ppm"]
["Ethylmethylamine","EMA","624-78-2","C3H9N","ES","ESM-23RV","Fixed","GD-K88Di Series","0～15ppm"]
["Ethylmethylamine","EMA","624-78-2","C3H9N","ES","ESM-23RVM","Fixed","GD-K88Ai Series","0～15ppm","Updated against electrolyte reduction"]
["Ethylmethylamine","EMA","624-78-2","C3H9N","ES","ESM-23RVM","Fixed","GD-K88Di Series","0～15ppm","Updated against electrolyte reduction"]
["Fluorine","F2","7782-41-4","F2","ES","ESM-K233","Portable","SC-8000","0～3ppm"]
["Fluorine","F2","7782-41-4","F2","ES","ESM-K235","Portable","SC-8000","0～3ppm"]
["Fluorine","F2","7782-41-4","F2","ES","ESU-K233","Fixed","GD-70D Series","0～3ppm"]
["Fluorine","F2","7782-41-4","F2","ES","ESU-K233","Fixed","TP-70D","0～3ppm"]
["Fluorine","F2","7782-41-4","F2","ES","ESU-K233L","Fixed","GD-70D Series","0～3ppm","Sensor for low humidity/Range： 20～62%RH"]
["Fluorine","F2","7782-41-4","F2","ES","ESU-K233L","Fixed","TP-70D","0～3ppm","Sensor for low humidity/Range： 20～62%RH"]
["Fluorine","F2","7782-41-4","F2","ES","ESU-K235","Fixed","GD-70D Series","0～3ppm"]
["Fluorine","F2","7782-41-4","F2","ES","ESU-K235","Fixed","TP-70D","0～3ppm"]
["Fluorine","F2","7782-41-4","F2","ES","ESU-K235L","Fixed","GD-70D Series","0～3ppm","Sensor for low humidity/Range： 20～65%RH"]
["Fluorine","F2","7782-41-4","F2","ES","ESU-K235L","Fixed","TP-70D","0～3ppm","Sensor for low humidity/Range： 20～65%RH"]
["Fluorine","F2","7782-41-4","F2","ES","ESM-K233","Fixed","GD-K88Ai Series","0～3ppm"]
["Fluorine","F2","7782-41-4","F2","ES","ESM-K233","Fixed","GD-K88Di Series","0～3ppm"]
["Fluorine","F2","7782-41-4","F2","ES","ESM-K235","Fixed","GD-K88Ai Series","0～3ppm"]
["Fluorine","F2","7782-41-4","F2","ES","ESM-K235","Fixed","GD-K88Di Series","0～3ppm"]
["Fluorine","F2","7782-41-4","F2","ES","ESM-K233C","Fixed","GD-K88Ai Series","0～3ppm"]
["Fluorine","F2","7782-41-4","F2","ES","ESM-K233C","Fixed","GD-K88Di Series","0～3ppm"]
["Fluorine","F2","7782-41-4","F2","ES","ESM-K233L","Fixed","GD-K88Ai Series","0～3ppm"]
["Fluorine","F2","7782-41-4","F2","ES","ESM-K233L","Fixed","GD-K88Di Series","0～3ppm"]
["Fluorine","F2","7782-41-4","F2","ES","ESM-K235L","Fixed","GD-K88Ai Series","0～3ppm"]
["Fluorine","F2","7782-41-4","F2","ES","ESM-K235L","Fixed","GD-K88Di Series","0～3ppm"]
["Fluorinert FC-3283","FC-3283","86508-42-1","-","RI","DE-2113-35","Fixed","RI-257","0～5000ppm"]
["Fluorinert FC-40","FC-40","86508-42-1","-","RI","DE-2113-37","Fixed","RI-257","0～1000ppm"]
["Formaldehyde","HCHO","50-00-0","CH2O","SH","SH-8662","Portable","SP-220(TYPE SC)","0～50ppm"]
["Formaldehyde","HCHO","50-00-0","CH2O","FP","TAB 008","Portable","FP-31","0～0.4ppm"]
["Formaldehyde","HCHO","50-00-0","CH2O","FP","TAB 009","Portable","FP-31","0～1ppm"]
["Formaldehyde","CH2O","50-00-0","CH2O","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～25%LEL/～17500ppm"]
["Formaldehyde","CH2O","50-00-0","CH2O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～25%LEL/～17500ppm"]
["Formaldehyde","CH2O","50-00-0","CH2O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～25%LEL/～17500ppm"]
["Formaldehyde","CH2O","50-00-0","CH2O","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～25%LEL/～17500ppm"]
["Formaldehyde","CH2O","50-00-0","CH2O","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～25%LEL/～17500ppm"]
["Formaldehyde","CH2O","50-00-0","CH2O","SG","SG-8511","Fixed","GD-A80V Series","0～10000ppm"]
["Formaldehyde","CH2O","50-00-0","CH2O","SG","SG-8511","Fixed","GD-D58・GH Series","0～10000ppm"]
["Formaldehyde","CH2O","50-00-0","CH2O","SG","SG-8511","Fixed","SD-1GH Series","0～10000ppm"]
["Formaldehyde","CH2O","50-00-0","CH2O","SG","SG-8511","Fixed","SD-D58・GH Series","0～10000ppm"]
["Formaldehyde","CH2O","50-00-0","CH2O","SG","SG-8521","Fixed","GD-A80V Series","0～30ppm/0～50ppm/0～100ppm/0～150ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～4000ppm/0～5000ppm"]
["Formaldehyde","CH2O","50-00-0","CH2O","SG","SG-8521","Fixed","GD-D58・GH Series","0～30ppm/0～50ppm/0～100ppm/0～150ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～4000ppm/0～5000ppm"]
["Formaldehyde","CH2O","50-00-0","CH2O","SG","SG-8521","Fixed","SD-1GH Series","0～30ppm/0～50ppm/0～100ppm/0～150ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～4000ppm/0～5000ppm"]
["Formaldehyde","CH2O","50-00-0","CH2O","SG","SG-8521","Fixed","SD-D58・GH Series","0～30ppm/0～50ppm/0～100ppm/0～150ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～4000ppm/0～5000ppm"]
["Formic acid","CH2O2","64-18-6","CH2O2","ES","ESU-K233M","Fixed","GD-70D Series","0～15ppm"]
["Formic acid","CH2O2","64-18-6","CH2O2","ES","ESU-K233M","Fixed","TP-70D","0～15ppm"]
["Formic acid","CH2O2","64-18-6","CH2O2","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～40%LEL/～72000ppm"]
["Formic acid","CH2O2","64-18-6","CH2O2","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～40%LEL/～72000ppm"]
["Formic acid","CH2O2","64-18-6","CH2O2","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～40%LEL/～72000ppm"]
["Formic acid","CH2O2","64-18-6","CH2O2","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～40%LEL/～72000ppm"]
["Formic acid","CH2O2","64-18-6","CH2O2","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～40%LEL/～72000ppm"]
["Formic acid","CH2O2","64-18-6","CH2O2","SG","SG-8521","Fixed","GD-A80V Series","0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Formic acid","CH2O2","64-18-6","CH2O2","SG","SG-8521","Fixed","GD-D58・GH Series","0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Formic acid","CH2O2","64-18-6","CH2O2","SG","SG-8521","Fixed","SD-1GH Series","0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Formic acid","CH2O2","64-18-6","CH2O2","SG","SG-8521","Fixed","SD-D58・GH Series","0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Freon 116","FC-116","76-16-4","C2F6","RI","DE-2113-37","Fixed","RI-257","0～5000ppm"]
["Furfural","C5H4O2","98-01-1","C5H4O2","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Furfural","C5H4O2","98-01-1","C5H4O2","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Furfural","C5H4O2","98-01-1","C5H4O2","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Furfural","C5H4O2","98-01-1","C5H4O2","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Furfural","C5H4O2","98-01-1","C5H4O2","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Furfural","C5H4O2","98-01-1","C5H4O2","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Furfural","C5H4O2","98-01-1","C5H4O2","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Furfural","C5H4O2","98-01-1","C5H4O2","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["Furfuryl alcohol","C5H6O2","98-00-0","C5H6O2","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Furfuryl alcohol","C5H6O2","98-00-0","C5H6O2","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Furfuryl alcohol","C5H6O2","98-00-0","C5H6O2","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Furfuryl alcohol","C5H6O2","98-00-0","C5H6O2","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Furfuryl alcohol","C5H6O2","98-00-0","C5H6O2","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Furfuryl alcohol","C5H6O2","98-00-0","C5H6O2","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Furfuryl alcohol","C5H6O2","98-00-0","C5H6O2","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Furfuryl alcohol","C5H6O2","98-00-0","C5H6O2","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["Galden HT135","HT-135","-","-","SG","SG-8521","Fixed","GD-A80V Series","0～2000ppm/0～3000ppm/0～5000ppm"]
["Galden HT135","HT-135","-","-","SG","SG-8521","Fixed","GD-D58・GH Series","0～2000ppm/0～3000ppm/0～5000ppm"]
["Galden HT135","HT-135","-","-","SG","SG-8521","Fixed","SD-1GH Series","0～2000ppm/0～3000ppm/0～5000ppm"]
["Galden HT135","HT-135","-","-","SG","SG-8521","Fixed","SD-D58・GH Series","0～2000ppm/0～3000ppm/0～5000ppm"]
["Galden ZT150","ZT-150","-","-","RI","DE-2113-35","Fixed","RI-257","0～1000ppm"]
["Galden ZT150","ZT-150","-","-","SG","SG-8562","Fixed","GD-A80V Series","0～1000ppm/0～2000ppm"]
["Galden ZT150","ZT-150","-","-","SG","SG-8562","Fixed","GD-D58・GH Series","0～1000ppm/0～2000ppm"]
["Galden ZT150","ZT-150","-","-","SG","SG-8562","Fixed","SD-1GH Series","0～1000ppm/0～2000ppm"]
["Galden ZT150","ZT-150","-","-","SG","SG-8562","Fixed","SD-D58・GH Series","0～1000ppm/0～2000ppm"]
["Gelmane","GeH4","7782-65-2","GeH4","SH","SH-8662","Portable","SP-220(TYPE SC)","0～0.2ppm"]
["Gelmane","GeH4","7782-65-2","GeH4","ES","ESM-23DH","Portable","SC-8000","0～0.8ppm"]
["Gelmane","GeH4","7782-65-2","GeH4","ES","ESU-23DH","Fixed","GD-70D Series","0～0.8ppm"]
["Gelmane","GeH4","7782-65-2","GeH4","ES","ESU-23DH","Fixed","TP-70D","0～0.8ppm"]
["Gelmane","GeH4","7782-65-2","GeH4","ES","ESU-23AY","Fixed","GD-70D Series","0～0.8ppm","Available only in cleanroom/Against C3H6 interference"]
["Gelmane","GeH4","7782-65-2","GeH4","ES","ESU-23AY","Fixed","TP-70D","0～0.8ppm","Available only in cleanroom/Against C3H6 interference"]
["Gelmane","GeH4","7782-65-2","GeH4","ES","ESM-23DH","Fixed","GD-K88Ai Series","0～0.8ppm"]
["Gelmane","GeH4","7782-65-2","GeH4","ES","ESM-23DH","Fixed","GD-K88Di Series","0～0.8ppm"]
["HCFC-225","AK-225","-","C3HF5CL2","RI","DE-2113-35","Fixed","RI-257","0～5000ppm"]
["HCFC-225","AK-225","-","C3HF5CL2","SG","SG-8513","Fixed","GD-A80V Series","0～10000ppm"]
["HCFC-225","AK-225","-","C3HF5CL2","SG","SG-8513","Fixed","GD-D58・GH Series","0～10000ppm"]
["HCFC-225","AK-225","-","C3HF5CL2","SG","SG-8513","Fixed","SD-1GH Series","0～10000ppm"]
["HCFC-225","AK-225","-","C3HF5CL2","SG","SG-8513","Fixed","SD-D58・GH Series","0～10000ppm"]
["Helium","He","7440-59-7","He","TE","TE-7515W","Portable","NP-1000(CH4)","0～100vol%"]
["Hexafluoro-1,3-butadiene","C4F6","685-63-2","C4F6","ES","ESU-K235L","Fixed","TP-70DGⅡ Series","0～5ppm","Only for TP-70DGⅡ"]
["Hexafluoro-1,3-butadiene","C4F6","685-63-2","C4F6","SG","SGU-8521","Fixed","GD-70D Series","0～200ppm"]
["Hexafluoro-1,3-butadiene","C4F6","685-63-2","C4F6","SG","SGU-8521","Fixed","TP-70D","0～200ppm"]
["Hexafluoro-1,3-butadiene","C4F6","685-63-2","C4F6","SG","SGU-8521","Fixed","GD-70D Series","0～2000ppm"]
["Hexafluoro-1,3-butadiene","C4F6","685-63-2","C4F6","SG","SGU-8521","Fixed","TP-70D","0～2000ppm"]
["Hexafluoro-1,3-butadiene","C4F6","685-63-2","C4F6","SG","SGU-8521","Fixed","GD-70D Series","0～5000ppm"]
["Hexafluoro-1,3-butadiene","C4F6","685-63-2","C4F6","SG","SGU-8521","Fixed","TP-70D","0～5000ppm"]
["Hexafluoro-1,3-butadiene","C4F6","685-63-2","C4F6","SG","SG-8521","Fixed","GD-A80V Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Hexafluoro-1,3-butadiene","C4F6","685-63-2","C4F6","SG","SG-8521","Fixed","GD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Hexafluoro-1,3-butadiene","C4F6","685-63-2","C4F6","SG","SG-8521","Fixed","SD-1GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Hexafluoro-1,3-butadiene","C4F6","685-63-2","C4F6","SG","SG-8521","Fixed","SD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Hexafluoroacetylacetone","Hhfac","1522-22-1","C5H2O2F6","ES","ESU-K235","Fixed","GD-70D Series","0～20ppm"]
["Hexafluoroacetylacetone","Hhfac","1522-22-1","C5H2O2F6","ES","ESU-K235","Fixed","TP-70D","0～20ppm"]
["Hexafluoroacetylacetone","Hhfac","1522-22-1","C5H2O2F6","ES","ESU-K235L","Fixed","GD-70D Series","0～20ppm","Sensor for low humidity/Range： 20～65%RH"]
["Hexafluoroacetylacetone","Hhfac","1522-22-1","C5H2O2F6","ES","ESU-K235L","Fixed","TP-70D","0～20ppm","Sensor for low humidity/Range： 20～65%RH"]
["Hexafluorobenzene","C6F6","392-56-3","C6F6","SG","SG-8511","Fixed","GD-A80V Series","0～3000ppm/0～5000ppm"]
["Hexafluorobenzene","C6F6","392-56-3","C6F6","SG","SG-8511","Fixed","GD-D58・GH Series","0～3000ppm/0～5000ppm"]
["Hexafluorobenzene","C6F6","392-56-3","C6F6","SG","SG-8511","Fixed","SD-1GH Series","0～3000ppm/0～5000ppm"]
["Hexafluorobenzene","C6F6","392-56-3","C6F6","SG","SG-8511","Fixed","SD-D58・GH Series","0～3000ppm/0～5000ppm"]
["Hexafluoropropylene","C3F6","116-15-4","C3F6","SG","SGU-8521","Fixed","GD-70D Series","0～2000ppm"]
["Hexafluoropropylene","C3F6","116-15-4","C3F6","SG","SGU-8521","Fixed","TP-70D","0～2000ppm"]
["Hexafluoropropylene","C3F6","116-15-4","C3F6","SG","SG-8521","Fixed","GD-A80V Series","0～2000ppm/0～3000ppm/0～5000ppm"]
["Hexafluoropropylene","C3F6","116-15-4","C3F6","SG","SG-8521","Fixed","GD-D58・GH Series","0～2000ppm/0～3000ppm/0～5000ppm"]
["Hexafluoropropylene","C3F6","116-15-4","C3F6","SG","SG-8521","Fixed","SD-1GH Series","0～2000ppm/0～3000ppm/0～5000ppm"]
["Hexafluoropropylene","C3F6","116-15-4","C3F6","SG","SG-8521","Fixed","SD-D58・GH Series","0～2000ppm/0～3000ppm/0～5000ppm"]
["Hexafluoropropylene oxide","C3F6O","-","C3OF6","SG","SG-8521","Fixed","GD-A80V Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Hexafluoropropylene oxide","C3F6O","-","C3OF6","SG","SG-8521","Fixed","GD-D58・GH Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Hexafluoropropylene oxide","C3F6O","-","C3OF6","SG","SG-8521","Fixed","SD-1GH Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Hexafluoropropylene oxide","C3F6O","-","C3OF6","SG","SG-8521","Fixed","SD-D58・GH Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Hexamethyldisiloxane","HMDSO","107-46-0","C6H18OSi2","SS","SSU-1925","Fixed","GD-70D+PLU Series","0～5ppm","PLU-70 required"]
["Hexamethyldisiloxane","HMDSO","107-46-0","C6H18OSi2","SS","SSU-1925","Fixed","GD-70DG","0～5ppm","PLU-70 required"]
["Hexamethyldisiloxane","HMDSO","107-46-0","C6H18OSi2","RI","DE-2113-37","Fixed","RI-257","0～5000ppm"]
["Hexyl Acetate","C8H16O2","142-92-7","C8H16O2","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～5000ppm"]
["Hexyl Acetate","C8H16O2","142-92-7","C8H16O2","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～5000ppm"]
["Hexyl Acetate","C8H16O2","142-92-7","C8H16O2","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～5000ppm"]
["Hexyl Acetate","C8H16O2","142-92-7","C8H16O2","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～5000ppm"]
["Hexyl Acetate","C8H16O2","142-92-7","C8H16O2","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～5000ppm"]
["Hexyl Acetate","C8H16O2","142-92-7","C8H16O2","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Hexyl Acetate","C8H16O2","142-92-7","C8H16O2","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Hexyl Acetate","C8H16O2","142-92-7","C8H16O2","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Hexyl Acetate","C8H16O2","142-92-7","C8H16O2","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Hexyl Acetate","C8H16O2","142-92-7","C8H16O2","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Hexyl Acetate","C8H16O2","142-92-7","C8H16O2","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Hexyl Acetate","C8H16O2","142-92-7","C8H16O2","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Hexyl Acetate","C8H16O2","142-92-7","C8H16O2","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["Hexyl Acetate","C8H16O2","142-92-7","C8H16O2","SG","SG-8521","Fixed","GD-A80V Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Hexyl Acetate","C8H16O2","142-92-7","C8H16O2","SG","SG-8521","Fixed","GD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Hexyl Acetate","C8H16O2","142-92-7","C8H16O2","SG","SG-8521","Fixed","SD-1GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Hexyl Acetate","C8H16O2","142-92-7","C8H16O2","SG","SG-8521","Fixed","SD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["HFE-7100","HFE7100","163702-08-07,163702-07-06,07-6378-9","C5H3OF9","RI","DE-2113-35","Fixed","RI-257","0～5000ppm"]
["HFE-7200","HFE7200","-","C6H5OF9","SG","SGU-8511","Fixed","GD-70D Series","0～2000ppm"]
["HFE-7200","HFE7200","-","C6H5OF9","SG","SGU-8511","Fixed","TP-70D","0～2000ppm"]
["HFE-7200","HFE7200","-","C6H5OF9","SG","SG-8511","Fixed","GD-A80V Series","0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["HFE-7200","HFE7200","-","C6H5OF9","SG","SG-8511","Fixed","GD-D58・GH Series","0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["HFE-7200","HFE7200","-","C6H5OF9","SG","SG-8511","Fixed","SD-1GH Series","0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["HFE-7200","HFE7200","-","C6H5OF9","SG","SG-8511","Fixed","SD-D58・GH Series","0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Hydrazine","N2H4","302-01-2","N2H4","ES","ESM-23E","Portable","SC-8000","0～5ppm"]
["Hydrazine","N2H4","302-01-2","N2H4","ES","ESU-23E","Fixed","GD-70D Series","0～5ppm"]
["Hydrazine","N2H4","302-01-2","N2H4","ES","ESU-23E","Fixed","TP-70D","0～5ppm"]
["Hydrazine","N2H4","302-01-2","N2H4","ES","ESM-23E","Fixed","GD-K88Ai Series","0～5ppm"]
["Hydrazine","N2H4","302-01-2","N2H4","ES","ESM-23E","Fixed","GD-K88Di Series","0～5ppm"]
["Hydrazine","N2H4","302-01-2","N2H4","ES","ESM-23E","Fixed","GD-K88Ai Series","0～10ppm"]
["Hydrazine","N2H4","302-01-2","N2H4","ES","ESM-23E","Fixed","GD-K88Di Series","0～10ppm"]
["Hydrogen","H2","1333-74-0","H2","HW","NC-6215","Portable","GX-8000","0～100%LEL"]
["Hydrogen","H2","1333-74-0","H2","HW","NC-6215","Portable","GX-8000(TYPE LEL)","0～100%LEL"]
["Hydrogen","H2","1333-74-0","H2","HW","NC-6215","Portable","GP-1000(HC/CH4)","0～100%LEL"]
["Hydrogen","H2","1333-74-0","H2","TE","TE-7515","Portable","GX-8000","0～100vol%"]
["Hydrogen","H2","1333-74-0","H2","HW","NC-6307","Portable","NC-1000(HC/CH4)","0～10000ppm"]
["Hydrogen","H2","1333-74-0","H2","TE","TE-7515W","Portable","NP-1000(H2)","0～100vol%"]
["Hydrogen","H2","1333-74-0","H2","SH","SH-8662","Portable","SP-220(TYPE SC)","0～10ppm"]
["Hydrogen","H2","1333-74-0","H2","SH","SH-8661","Portable","SP-220(TYPE H2)","0～10000ppm"]
["Hydrogen","H2","1333-74-0","H2","ES","ESU-23DHF","Fixed","GD-70D Series","0～2000ppm"]
["Hydrogen","H2","1333-74-0","H2","ES","ESU-23DHF","Fixed","TP-70D","0～2000ppm"]
["Hydrogen","H2","1333-74-0","H2","ES","ESU-23DHF-J","Fixed","GD-70D Series","0～1000ppm","With lifetime prediction"]
["Hydrogen","H2","1333-74-0","H2","ES","ESU-23DHF-J","Fixed","TP-70D","0～1000ppm","With lifetime prediction"]
["Hydrogen","H2","1333-74-0","H2","SG","SGU-8511","Fixed","GD-70D Series","0～2.00vol%"]
["Hydrogen","H2","1333-74-0","H2","SG","SGU-8511","Fixed","TP-70D","0～2.00vol%"]
["Hydrogen","H2","1333-74-0","H2","SG","SGU-8541","Fixed","GD-70D Series","0～100ppm"]
["Hydrogen","H2","1333-74-0","H2","SG","SGU-8541","Fixed","TP-70D","0～100ppm"]
["Hydrogen","H2","1333-74-0","H2","SG","SGU-8521","Fixed","GD-70D Series","0～500ppm"]
["Hydrogen","H2","1333-74-0","H2","SG","SGU-8521","Fixed","TP-70D","0～500ppm"]
["Hydrogen","H2","1333-74-0","H2","SG","SGU-8521","Fixed","GD-70D Series","0～1000ppm"]
["Hydrogen","H2","1333-74-0","H2","SG","SGU-8521","Fixed","TP-70D","0～1000ppm"]
["Hydrogen","H2","1333-74-0","H2","SG","SGU-8541","Fixed","GD-70D Series","0～200ppm"]
["Hydrogen","H2","1333-74-0","H2","SG","SGU-8541","Fixed","TP-70D","0～200ppm"]
["Hydrogen","H2","1333-74-0","H2","SG","SGU-8541","Fixed","GD-70D Series","0～500ppm"]
["Hydrogen","H2","1333-74-0","H2","SG","SGU-8541","Fixed","TP-70D","0～500ppm"]
["Hydrogen","H2","1333-74-0","H2","SG","SGU-8541","Fixed","GD-70D Series","0～1000ppm"]
["Hydrogen","H2","1333-74-0","H2","SG","SGU-8541","Fixed","TP-70D","0～1000ppm"]
["Hydrogen","H2","1333-74-0","H2","SG","SGU-8541","Fixed","GD-70D Series","0～2000ppm"]
["Hydrogen","H2","1333-74-0","H2","SG","SGU-8541","Fixed","TP-70D","0～2000ppm"]
["Hydrogen","H2","1333-74-0","H2","SG","SGU-8541","Fixed","GD-70D Series","0～4000ppm"]
["Hydrogen","H2","1333-74-0","H2","SG","SGU-8541","Fixed","TP-70D","0～4000ppm"]
["Hydrogen","H2","1333-74-0","H2","HW","NCU-6211","Fixed","GD-70D Series","0～2vol%"]
["Hydrogen","H2","1333-74-0","H2","HW","NCU-6211","Fixed","TP-70D","0～2vol%"]
["Hydrogen","H2","1333-74-0","H2","HW","NCU-6211","Fixed","GD-70D Series","0～100%LEL","Confirm that GD-70D is non-explosion proof"]
["Hydrogen","H2","1333-74-0","H2","HW","NCU-6211","Fixed","TP-70D","0～100%LEL","Confirm that GD-70D is non-explosion proof"]
["Hydrogen","H2","1333-74-0","H2","HW","NCU-6211","Fixed","GD-70D Series","0～1vol%"]
["Hydrogen","H2","1333-74-0","H2","HW","NCU-6211","Fixed","TP-70D","0～1vol%"]
["Hydrogen","H2","1333-74-0","H2","HW","NCU-6211","Fixed","GD-70D Series","0～4vol%","Confirm that GD-70D is non-explosion proof"]
["Hydrogen","H2","1333-74-0","H2","HW","NCU-6211","Fixed","TP-70D","0～4vol%","Confirm that GD-70D is non-explosion proof"]
["Hydrogen","H2","1333-74-0","H2","HW","NCU-6244A","Fixed","GD-70D Series","0～100%LEL","Confirm that GD-70D is non-explosion proof"]
["Hydrogen","H2","1333-74-0","H2","HW","NCU-6244A","Fixed","TP-70D","0～100%LEL","Confirm that GD-70D is non-explosion proof"]
["Hydrogen","H2","1333-74-0","H2","HW","NCU-6244A","Fixed","GD-70D Series","0～2vol%"]
["Hydrogen","H2","1333-74-0","H2","HW","NCU-6244A","Fixed","TP-70D","0～2vol%"]
["Hydrogen","H2","1333-74-0","H2","HW","NCU-6244A","Fixed","GD-70D Series","0～2000ppm"]
["Hydrogen","H2","1333-74-0","H2","HW","NCU-6244A","Fixed","TP-70D","0～2000ppm"]
["Hydrogen","H2","1333-74-0","H2","SH","SHU-8644","Fixed","GD-70D Series","0～2000ppm"]
["Hydrogen","H2","1333-74-0","H2","ES","ESM-23DHF","Fixed","GD-K88Ai Series","0～2000ppm"]
["Hydrogen","H2","1333-74-0","H2","ES","ESM-23DHF","Fixed","GD-K88Di Series","0～2000ppm"]
["Hydrogen","H2","1333-74-0","H2","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Hydrogen","H2","1333-74-0","H2","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Hydrogen","H2","1333-74-0","H2","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～40000ppm"]
["Hydrogen","H2","1333-74-0","H2","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～40000ppm"]
["Hydrogen","H2","1333-74-0","H2","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～40000ppm"]
["Hydrogen","H2","1333-74-0","H2","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～40000ppm"]
["Hydrogen","H2","1333-74-0","H2","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～40000ppm"]
["Hydrogen","H2","1333-74-0","H2","HW","HW-6213/NC-6213","Fixed","GD-A80 Series","0～100%LEL/0～40000ppm"]
["Hydrogen","H2","1333-74-0","H2","HW","HW-6213/NC-6213","Fixed","GD-D58(TYPE GP) Series","0～100%LEL/0～40000ppm"]
["Hydrogen","H2","1333-74-0","H2","HW","HW-6213/NC-6213","Fixed","GD-D58(TYPE NC) Series","0～100%LEL/0～40000ppm"]
["Hydrogen","H2","1333-74-0","H2","HW","HW-6239","Fixed","GD-A80-70 Series","0～100%LEL"]
["Hydrogen","H2","1333-74-0","H2","HW","HW-6239","Fixed","SD-1(TYPE GP) Series","0～100%LEL"]
["Hydrogen","H2","1333-74-0","H2","HW","HW-6239","Fixed","SD-D58(TYPE GP) Series","0～100%LEL"]
["Hydrogen","H2","1333-74-0","H2","HW","HW-6239/NC-6239","Fixed","GD-A80 Series","0～100%LEL/0～40000ppm"]
["Hydrogen","H2","1333-74-0","H2","HW","HW-6239/NC-6239","Fixed","GD-D58(TYPE GP) Series","0～100%LEL/0～40000ppm"]
["Hydrogen","H2","1333-74-0","H2","HW","HW-6239/NC-6239","Fixed","GD-D58(TYPE NC) Series","0～100%LEL/0～40000ppm"]
["Hydrogen","H2","1333-74-0","H2","HW","HW-6239/NC-6239","Fixed","SD-1(TYPE NC) Series","0～100%LEL/0～40000ppm"]
["Hydrogen","H2","1333-74-0","H2","HW","HW-6239/NC-6239","Fixed","SD-D58(TYPE NC) Series","0～100%LEL/0～40000ppm"]
["Hydrogen","H2","1333-74-0","H2","HW","NC-6240A","Fixed","GD-A80 Series","0～100%LEL/0～40000ppm"]
["Hydrogen","H2","1333-74-0","H2","HW","NC-6240A","Fixed","GD-D58(TYPE NC) Series","0～100%LEL/0～40000ppm"]
["Hydrogen","H2","1333-74-0","H2","HW","NC-6240A","Fixed","SD-1(TYPE NC) Series","0～100%LEL/0～40000ppm"]
["Hydrogen","H2","1333-74-0","H2","HW","NC-6240A","Fixed","SD-D58(TYPE NC) Series","0～100%LEL/0～40000ppm"]
["Hydrogen","H2","1333-74-0","H2","HW","NC-6245","Fixed","GD-A80 Series","0～100%LEL"]
["Hydrogen","H2","1333-74-0","H2","HW","NC-6245","Fixed","GD-D58(TYPE NC) Series","0～100%LEL"]
["Hydrogen","H2","1333-74-0","H2","HW","NC-6245","Fixed","SD-1(TYPE NC) Series","0～100%LEL"]
["Hydrogen","H2","1333-74-0","H2","HW","NC-6245","Fixed","SD-D58(TYPE NC) Series","0～100%LEL"]
["Hydrogen","H2","1333-74-0","H2","HW","NC-6250","Fixed","GD-A80 Series","0～100%LEL/0～40000ppm"]
["Hydrogen","H2","1333-74-0","H2","HW","NC-6250","Fixed","GD-D58(TYPE NC) Series","0～100%LEL/0～40000ppm"]
["Hydrogen","H2","1333-74-0","H2","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Hydrogen","H2","1333-74-0","H2","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Hydrogen","H2","1333-74-0","H2","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Hydrogen","H2","1333-74-0","H2","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Hydrogen","H2","1333-74-0","H2","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Hydrogen","H2","1333-74-0","H2","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Hydrogen","H2","1333-74-0","H2","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Hydrogen","H2","1333-74-0","H2","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["Hydrogen","H2","1333-74-0","H2","HW","NC-6244","Fixed","GD-A80 Series","0～100%LEL"]
["Hydrogen","H2","1333-74-0","H2","HW","NC-6244","Fixed","GD-D58(TYPE NC) Series","0～100%LEL"]
["Hydrogen","H2","1333-74-0","H2","HW","NC-6244A","Fixed","GD-A80 Series","0～100%LEL/0～40000ppm"]
["Hydrogen","H2","1333-74-0","H2","HW","NC-6244A","Fixed","GD-D58(TYPE NC) Series","0～100%LEL/0～40000ppm"]
["Hydrogen","H2","1333-74-0","H2","HW","NC-6244A","Fixed","SD-1(TYPE NC) Series","0～100%LEL/0～40000ppm"]
["Hydrogen","H2","1333-74-0","H2","HW","NC-6244A","Fixed","SD-D58(TYPE NC) Series","0～100%LEL/0～40000ppm"]
["Hydrogen","H2","1333-74-0","H2","SG","SG-8511","Fixed","GD-A80V Series","0～3000ppm/0～4000ppm/0～5000ppm/0～10000ppm/0～20000ppm/0～40000ppm/0～50%LEL/0～100%LEL/0～1vol%/0～2vol%/0～4vol%"]
["Hydrogen","H2","1333-74-0","H2","SG","SG-8511","Fixed","GD-D58・GH Series","0～3000ppm/0～4000ppm/0～5000ppm/0～10000ppm/0～20000ppm/0～40000ppm/0～50%LEL/0～100%LEL/0～1vol%/0～2vol%/0～4vol%"]
["Hydrogen","H2","1333-74-0","H2","SG","SG-8511","Fixed","SD-1GH Series","0～3000ppm/0～4000ppm/0～5000ppm/0～10000ppm/0～20000ppm/0～40000ppm/0～50%LEL/0～100%LEL/0～1vol%/0～2vol%/0～4vol%"]
["Hydrogen","H2","1333-74-0","H2","SG","SG-8511","Fixed","SD-D58・GH Series","0～3000ppm/0～4000ppm/0～5000ppm/0～10000ppm/0～20000ppm/0～40000ppm/0～50%LEL/0～100%LEL/0～1vol%/0～2vol%/0～4vol%"]
["Hydrogen","H2","1333-74-0","H2","SG","SG-8521","Fixed","GD-A80V Series","★0～50ppm/★0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm","★Range easily affected by environmental conditions and other"]
["Hydrogen","H2","1333-74-0","H2","SG","SG-8521","Fixed","GD-D58・GH Series","★0～50ppm/★0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm","★Range easily affected by environmental conditions and other"]
["Hydrogen","H2","1333-74-0","H2","SG","SG-8521","Fixed","SD-1GH Series","★0～50ppm/★0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm","★Range easily affected by environmental conditions and other"]
["Hydrogen","H2","1333-74-0","H2","SG","SG-8521","Fixed","SD-D58・GH Series","★0～50ppm/★0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm","★Range easily affected by environmental conditions and other"]
["Hydrogen","H2","1333-74-0","H2","SG","SG-8541","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Hydrogen","H2","1333-74-0","H2","SG","SG-8541","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Hydrogen","H2","1333-74-0","H2","SG","SG-8541","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Hydrogen","H2","1333-74-0","H2","SG","SG-8541","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Hydrogen Bromide","HBr","10035-10-6","HBr","SH","SH-8662","Portable","SP-220(TYPE SC)","0～10ppm"]
["Hydrogen Bromide","HBr","10035-10-6","HBr","ES","ESM-23E","Portable","SC-8000","0～6ppm"]
["Hydrogen Bromide","HBr","10035-10-6","HBr","ES","ESM-23E","Portable","SC-8000","0～9ppm"]
["Hydrogen Bromide","HBr","10035-10-6","HBr","ES","ESU-23E","Fixed","GD-70D Series","0～6ppm"]
["Hydrogen Bromide","HBr","10035-10-6","HBr","ES","ESU-23E","Fixed","TP-70D","0～6ppm"]
["Hydrogen Bromide","HBr","10035-10-6","HBr","ES","ESU-23E-G","Fixed","GD-70D Series","0～6ppm","Alternate gas factor (HCL) granted"]
["Hydrogen Bromide","HBr","10035-10-6","HBr","ES","ESU-23E-G","Fixed","TP-70D","0～6ppm","Alternate gas factor (HCL) granted"]
["Hydrogen Bromide","HBr","10035-10-6","HBr","ES","ESU-23E-G","Fixed","GD-70D Series","0～9ppm","Alternate gas factor (HCL) granted"]
["Hydrogen Bromide","HBr","10035-10-6","HBr","ES","ESU-23E-G","Fixed","TP-70D","0～9ppm","Alternate gas factor (HCL) granted"]
["Hydrogen Bromide","HBr","10035-10-6","HBr","ES","ESM-23E-G","Fixed","GD-K88Ai Series","0～6ppm"]
["Hydrogen Bromide","HBr","10035-10-6","HBr","ES","ESM-23E-G","Fixed","GD-K88Di Series","0～6ppm"]
["Hydrogen Bromide","HBr","10035-10-6","HBr","ES","ESM-23E-G","Fixed","GD-K88Ai Series","0～9ppm"]
["Hydrogen Bromide","HBr","10035-10-6","HBr","ES","ESM-23E-G","Fixed","GD-K88Di Series","0～9ppm"]
["Hydrogen Chloride","HCL","7647-01-0","HCL","SH","SH-8662","Portable","SP-220(TYPE SC)","0～10ppm"]
["Hydrogen Chloride","HCL","7647-01-0","HCL","ES","ESM-23E","Portable","SC-8000","0～6ppm"]
["Hydrogen Chloride","HCL","7647-01-0","HCL","ES","ESM-23E","Portable","SC-8000","0～15ppm"]
["Hydrogen Chloride","HCL","7647-01-0","HCL","ES","ESM-K235","Portable","SC-8000","0～6ppm"]
["Hydrogen Chloride","HCL","7647-01-0","HCL","ES","ESM-23E","Portable","SC-8000","0～5ppm"]
["Hydrogen Chloride","HCL","7647-01-0","HCL","ES","ESU-23E","Fixed","GD-70D Series","0～5ppm"]
["Hydrogen Chloride","HCL","7647-01-0","HCL","ES","ESU-23E","Fixed","TP-70D","0～5ppm"]
["Hydrogen Chloride","HCL","7647-01-0","HCL","ES","ESU-23E","Fixed","GD-70D Series","0～6ppm"]
["Hydrogen Chloride","HCL","7647-01-0","HCL","ES","ESU-23E","Fixed","TP-70D","0～6ppm"]
["Hydrogen Chloride","HCL","7647-01-0","HCL","ES","ESU-23E","Fixed","GD-70D Series","0～15ppm"]
["Hydrogen Chloride","HCL","7647-01-0","HCL","ES","ESU-23E","Fixed","TP-70D","0～15ppm"]
["Hydrogen Chloride","HCL","7647-01-0","HCL","ES","ESU-K233","Fixed","GD-70D Series","0～15ppm"]
["Hydrogen Chloride","HCL","7647-01-0","HCL","ES","ESU-K233","Fixed","TP-70D","0～15ppm"]
["Hydrogen Chloride","HCL","7647-01-0","HCL","ES","ESU-K235","Fixed","GD-70D Series","0～6ppm"]
["Hydrogen Chloride","HCL","7647-01-0","HCL","ES","ESU-K235","Fixed","TP-70D","0～6ppm"]
["Hydrogen Chloride","HCL","7647-01-0","HCL","ES","ESU-K235L","Fixed","GD-70D Series","0～6 ppm","Sensor for low humidity/Range： 20～65%RH"]
["Hydrogen Chloride","HCL","7647-01-0","HCL","ES","ESU-K235L","Fixed","TP-70D","0～6 ppm","Sensor for low humidity/Range： 20～65%RH"]
["Hydrogen Chloride","HCL","7647-01-0","HCL","ES","ESM-23E","Fixed","GD-K88Ai Series","0～15ppm"]
["Hydrogen Chloride","HCL","7647-01-0","HCL","ES","ESM-23E","Fixed","GD-K88Di Series","0～15ppm"]
["Hydrogen Chloride","HCL","7647-01-0","HCL","ES","ESM-23E","Fixed","GD-K88Ai Series","0～6ppm"]
["Hydrogen Chloride","HCL","7647-01-0","HCL","ES","ESM-23E","Fixed","GD-K88Di Series","0～6ppm"]
["Hydrogen Chloride","HCL","7647-01-0","HCL","ES","ESM-23E","Fixed","GD-K88Ai Series","0～5ppm"]
["Hydrogen Chloride","HCL","7647-01-0","HCL","ES","ESM-23E","Fixed","GD-K88Di Series","0～5ppm"]
["Hydrogen Chloride","HCL","7647-01-0","HCL","ES","ESM-K233","Fixed","GD-K88Ai Series","0～15ppm"]
["Hydrogen Chloride","HCL","7647-01-0","HCL","ES","ESM-K233","Fixed","GD-K88Di Series","0～15ppm"]
["Hydrogen Chloride","HCL","7647-01-0","HCL","ES","ESM-K235","Fixed","GD-K88Ai Series","0～6ppm"]
["Hydrogen Chloride","HCL","7647-01-0","HCL","ES","ESM-K235","Fixed","GD-K88Di Series","0～6ppm"]
["Hydrogen Chloride","HCL","7647-01-0","HCL","ES","ESM-K233C","Fixed","GD-K88Ai Series","0～15ppm"]
["Hydrogen Chloride","HCL","7647-01-0","HCL","ES","ESM-K233C","Fixed","GD-K88Di Series","0～15ppm"]
["Hydrogen Chloride","HCL","7647-01-0","HCL","ES","ESM-K233L","Fixed","GD-K88Ai Series","0～15ppm"]
["Hydrogen Chloride","HCL","7647-01-0","HCL","ES","ESM-K233L","Fixed","GD-K88Di Series","0～15ppm"]
["Hydrogen Chloride","HCL","7647-01-0","HCL","ES","ESM-K235L","Fixed","GD-K88Ai Series","0～6ppm"]
["Hydrogen Chloride","HCL","7647-01-0","HCL","ES","ESM-K235L","Fixed","GD-K88Di Series","0～6ppm"]
["Hydrogen Cyanide","HCN","74-90-8","CHN","SH","SH-8662","Portable","SP-220(TYPE FUM)","0～1ppm"]
["Hydrogen Cyanide","HCN","74-90-8","CHN","ES","ESS-03DH","Portable","GX-6000","0～15ppm"]
["Hydrogen Cyanide","HCN","74-90-8","CHN","ES","ESM-01DH-D","Portable","SC-01","0～15ppm"]
["Hydrogen Cyanide","HCN","74-90-8","CHN","ES","ESM-23DH","Portable","SC-8000","0.3～15ppm"]
["Hydrogen Cyanide","HCN","74-90-8","CHN","ES","ESU-23DH-EX","Fixed","GD-70D Series","0.9～15ppm","Export limited：unable to measure under 6%FS"]
["Hydrogen Cyanide","HCN","74-90-8","CHN","ES","ESU-23DH-EX","Fixed","TP-70D","0.9～15ppm","Export limited：unable to measure under 6%FS"]
["Hydrogen Cyanide","HCN","74-90-8","CHN","ES","ESU-23DH-EX","Fixed","GD-70D Series","0.4～30ppm","Export limited：unable to measure under 0.4ppm"]
["Hydrogen Cyanide","HCN","74-90-8","CHN","ES","ESU-23DH-EX","Fixed","TP-70D","0.4～30ppm","Export limited：unable to measure under 0.4ppm"]
["Hydrogen Cyanide","HCN","74-90-8","CHN","ES","ESM-23DH","Fixed","GD-K88Ai Series","0.9～15ppm","Export limited：unable to measure under 6%FS"]
["Hydrogen Cyanide","HCN","74-90-8","CHN","ES","ESM-23DH","Fixed","GD-K88Di Series","0.9～15ppm","Export limited：unable to measure under 6%FS"]
["Hydrogen Cyanide","HCN","74-90-8","CHN","ES","ESM-23DH","Fixed","GD-K88Ai Series","0.4～30ppm","Export limited：unable to measure under 0.4ppm"]
["Hydrogen Cyanide","HCN","74-90-8","CHN","ES","ESM-23DH","Fixed","GD-K88Di Series","0.4～30ppm","Export limited：unable to measure under 0.4ppm"]
["Hydrogen Fluoride","HF","7664-39-3","HF","ES","ESM-K233","Portable","SC-8000","0.4～9ppm"]
["Hydrogen Fluoride","HF","7664-39-3","HF","ES","ESU-K233-EX","Fixed","GD-70D Series","0.4～9ppm","Export limited：unable to measure under 0.4ppm"]
["Hydrogen Fluoride","HF","7664-39-3","HF","ES","ESU-K233-EX","Fixed","TP-70D","0.4～9ppm","Export limited：unable to measure under 0.4ppm"]
["Hydrogen Fluoride","HF","7664-39-3","HF","ES","ESU-K233-S-EX","Fixed","GD-70D Series","0.4～3ppm","Export limited：unable to measure under 0.4ppm"]
["Hydrogen Fluoride","HF","7664-39-3","HF","ES","ESU-K233-S-EX","Fixed","TP-70D","0.4～3ppm","Export limited：unable to measure under 0.4ppm"]
["Hydrogen Fluoride","HF","7664-39-3","HF","ES","ESU-K233L-EX","Fixed","GD-70D Series","0.4～9ppm","Sensor for low humidity/Range： 20～62%RH/Export limited：unable to measure under 0.4ppm"]
["Hydrogen Fluoride","HF","7664-39-3","HF","ES","ESU-K233L-EX","Fixed","TP-70D","0.4～9ppm","Sensor for low humidity/Range： 20～62%RH/Export limited：unable to measure under 0.4ppm"]
["Hydrogen Fluoride","HF","7664-39-3","HF","ES","ESU-K233L-S-EX","Fixed","GD-70D Series","0.4～3ppm","Sensor for low humidity/Range： 20～62%RH/Export limited：unable to measure under 0.4ppm"]
["Hydrogen Fluoride","HF","7664-39-3","HF","ES","ESU-K233L-S-EX","Fixed","TP-70D","0.4～3ppm","Sensor for low humidity/Range： 20～62%RH/Export limited：unable to measure under 0.4ppm"]
["Hydrogen Fluoride","HF","7664-39-3","HF","ES","ESU-K235-EX","Fixed","GD-70D Series","0.4～1.5ppm","Export limited：unable to measure under 0.4ppm"]
["Hydrogen Fluoride","HF","7664-39-3","HF","ES","ESU-K235-EX","Fixed","TP-70D","0.4～1.5ppm","Export limited：unable to measure under 0.4ppm"]
["Hydrogen Fluoride","HF","7664-39-3","HF","ES","ESU-K235L-EX","Fixed","GD-70D Series","0.4～1.5ppm","Sensor for low humidity/Range： 20～65%RH/Export limited：unable to measure under 0.4ppm"]
["Hydrogen Fluoride","HF","7664-39-3","HF","ES","ESU-K235L-EX","Fixed","TP-70D","0.4～1.5ppm","Sensor for low humidity/Range： 20～65%RH/Export limited：unable to measure under 0.4ppm"]
["Hydrogen Fluoride","HF","7664-39-3","HF","ES","ESM-K233","Fixed","GD-K88Ai Series","0.4～9ppm","Export limited：unable to measure under 0.4ppm"]
["Hydrogen Fluoride","HF","7664-39-3","HF","ES","ESM-K233","Fixed","GD-K88Di Series","0.4～9ppm","Export limited：unable to measure under 0.4ppm"]
["Hydrogen Fluoride","HF","7664-39-3","HF","ES","ESM-K233-S","Fixed","GD-K88Ai Series","0.4～3ppm","Export limited：unable to measure under 0.4ppm"]
["Hydrogen Fluoride","HF","7664-39-3","HF","ES","ESM-K233-S","Fixed","GD-K88Di Series","0.4～3ppm","Export limited：unable to measure under 0.4ppm"]
["Hydrogen Fluoride","HF","7664-39-3","HF","ES","ESM-K233-S","Fixed","GD-K88Ai Series","0.4～5ppm","Export limited：unable to measure under 0.4ppm"]
["Hydrogen Fluoride","HF","7664-39-3","HF","ES","ESM-K233-S","Fixed","GD-K88Di Series","0.4～5ppm","Export limited：unable to measure under 0.4ppm"]
["Hydrogen Fluoride","HF","7664-39-3","HF","ES","ESM-K235","Fixed","GD-K88Ai Series","0.4～1.5ppm","Export limited：unable to measure under 0.4ppm"]
["Hydrogen Fluoride","HF","7664-39-3","HF","ES","ESM-K235","Fixed","GD-K88Di Series","0.4～1.5ppm","Export limited：unable to measure under 0.4ppm"]
["Hydrogen Fluoride","HF","7664-39-3","HF","ES","ESM-K233L","Fixed","GD-K88Ai Series","0.4～9ppm","Sensor for low humidity/Range： 20～62%RH/Export limited：unable to measure under 0.4ppm"]
["Hydrogen Fluoride","HF","7664-39-3","HF","ES","ESM-K233L","Fixed","GD-K88Di Series","0.4～9ppm","Sensor for low humidity/Range： 20～62%RH/Export limited：unable to measure under 0.4ppm"]
["Hydrogen Fluoride","HF","7664-39-3","HF","ES","ESM-K233L-S","Fixed","GD-K88Ai Series","0.4～3ppm","Sensor for low humidity/Range： 20～62%RH/Export limited：unable to measure under 0.4ppm"]
["Hydrogen Fluoride","HF","7664-39-3","HF","ES","ESM-K233L-S","Fixed","GD-K88Di Series","0.4～3ppm","Sensor for low humidity/Range： 20～62%RH/Export limited：unable to measure under 0.4ppm"]
["Hydrogen Fluoride","HF","7664-39-3","HF","ES","ESM-K233L-S","Fixed","GD-K88Ai Series","0.4～5ppm","Sensor for low humidity/Range： 20～62%RH/Export limited：unable to measure under 0.4ppm"]
["Hydrogen Fluoride","HF","7664-39-3","HF","ES","ESM-K233L-S","Fixed","GD-K88Di Series","0.4～5ppm","Sensor for low humidity/Range： 20～62%RH/Export limited：unable to measure under 0.4ppm"]
["Hydrogen Fluoride","HF","7664-39-3","HF","ES","ESM-K235L","Fixed","GD-K88Ai Series","0.4～1.5ppm","Sensor for low humidity/Range： 20～65%RH/Export limited：unable to measure under 0.4ppm"]
["Hydrogen Fluoride","HF","7664-39-3","HF","ES","ESM-K235L","Fixed","GD-K88Di Series","0.4～1.5ppm","Sensor for low humidity/Range： 20～65%RH/Export limited：unable to measure under 0.4ppm"]
["Hydrogen Iodine","HI","10034-85-2","HI","ES","ESM-23E","Portable","SC-8000","0～5ppm"]
["Hydrogen Iodine","HI","10034-85-2","HI","ES","ESU-23E","Fixed","GD-70D Series","0～5ppm"]
["Hydrogen Iodine","HI","10034-85-2","HI","ES","ESU-23E","Fixed","TP-70D","0～5ppm"]
["Hydrogen Iodine","HI","10034-85-2","HI","ES","ESM-23E","Fixed","GD-K88Ai Series","0～5ppm"]
["Hydrogen Iodine","HI","10034-85-2","HI","ES","ESM-23E","Fixed","GD-K88Di Series","0～5ppm"]
["Hydrogen Peroxide","H2O2","7722-84-1","H2O2","ES","ESM-23DH","Portable","SC-8000","0～3ppm"]
["Hydrogen Peroxide","H2O2","7722-84-1","H2O2","ES","ESU-23DH","Fixed","GD-70D Series","0～3ppm"]
["Hydrogen Peroxide","H2O2","7722-84-1","H2O2","ES","ESU-23DH","Fixed","TP-70D","0～3ppm"]
["Hydrogen Peroxide","H2O2","7722-84-1","H2O2","ES","ESM-23DH","Fixed","GD-K88Ai Series","0～3ppm"]
["Hydrogen Peroxide","H2O2","7722-84-1","H2O2","ES","ESM-23DH","Fixed","GD-K88Di Series","0～3ppm"]
["Hydrogen Selenide","H2Se","7783-07-5","H2Se","SH","SH-8662","Portable","SP-220(TYPE SC)","0～0.5ppm"]
["Hydrogen Selenide","H2Se","7783-07-5","H2Se","ES","ESM-23SD","Portable","SC-8000","0～0.2ppm"]
["Hydrogen Selenide","H2Se","7783-07-5","H2Se","ES","ESU-23SD","Fixed","GD-70D Series","0～0.2ppm"]
["Hydrogen Selenide","H2Se","7783-07-5","H2Se","ES","ESU-23SD","Fixed","TP-70D","0～0.2ppm"]
["Hydrogen Selenide","H2Se","7783-07-5","H2Se","ES","ESM-23SD","Fixed","GD-K88Ai Series","0～0.2ppm"]
["Hydrogen Selenide","H2Se","7783-07-5","H2Se","ES","ESM-23SD","Fixed","GD-K88Di Series","0～0.2ppm"]
["Hydrogen Sulfide","H2S","7783-06-4","H2S","ES","ES-1827i","Portable","GX-2009","0～30ppm"]
["Hydrogen Sulfide","H2S","7783-06-4","H2S","ES","ES-1827i","Portable","GX-2012","0～30ppm"]
["Hydrogen Sulfide","H2S","7783-06-4","H2S","ES","ES-1827i","Portable","GX-6000","0～30ppm"]
["Hydrogen Sulfide","H2S","7783-06-4","H2S","ES","ES-1827i","Portable","HS-03","0～30ppm"]
["Hydrogen Sulfide","H2S","7783-06-4","H2S","ES","ES-037i","Portable","GX-8000","0～30ppm"]
["Hydrogen Sulfide","H2S","7783-06-4","H2S","ES","ES-037R","Portable","RX-8700","0～30ppm"]
["Hydrogen Sulfide","H2S","7783-06-4","H2S","ES","ES-037RM","Portable","RX-8700","0～1000ppm"]
["Hydrogen Sulfide","H2S","7783-06-4","H2S","SH","SH-8662","Portable","SP-220(TYPE SC)","0～0.1ppm"]
["Hydrogen Sulfide","H2S","7783-06-4","H2S","ES","ESM-017i","Portable","SC-01","0～30ppm"]
["Hydrogen Sulfide","H2S","7783-06-4","H2S","ES","ESM-237iF","Portable","SC-8000","0～30ppm"]
["Hydrogen Sulfide","H2S","7783-06-4","H2S","ES","ESM-237iF","Portable","SC-8000","0～3ppm"]
["Hydrogen Sulfide","H2S","7783-06-4","H2S","ES","ESM-237iF","Portable","SC-8000","0～1ppm"]
["Hydrogen Sulfide","H2S","7783-06-4","H2S","ES","ESU-237","Fixed","GD-70D Series","0～30ppm"]
["Hydrogen Sulfide","H2S","7783-06-4","H2S","ES","ESU-237","Fixed","TP-70D","0～30ppm"]
["Hydrogen Sulfide","H2S","7783-06-4","H2S","ES","ESU-237iF","Fixed","GD-70D Series","0～1ppm"]
["Hydrogen Sulfide","H2S","7783-06-4","H2S","ES","ESU-237iF","Fixed","TP-70D","0～1ppm"]
["Hydrogen Sulfide","H2S","7783-06-4","H2S","ES","ESU-237iF","Fixed","GD-70D Series","0～3ppm"]
["Hydrogen Sulfide","H2S","7783-06-4","H2S","ES","ESU-237iF","Fixed","TP-70D","0～3ppm"]
["Hydrogen Sulfide","H2S","7783-06-4","H2S","ES","ESU-237iF","Fixed","GD-70D Series","0～30ppm"]
["Hydrogen Sulfide","H2S","7783-06-4","H2S","ES","ESU-237iF","Fixed","TP-70D","0～30ppm"]
["Hydrogen Sulfide","H2S","7783-06-4","H2S","ES","ES-837RP","Fixed","SD-1EC Series","0～30ppm/0～50ppm/0～100ppm"]
["Hydrogen Sulfide","H2S","7783-06-4","H2S","ES","ES-837RP","Fixed","SDWL-1EC Series","0～30ppm/0～50ppm/0～100ppm"]
["Hydrogen Sulfide","H2S","7783-06-4","H2S","ES","ESM-237","Fixed","GD-K88Ai Series","0～30ppm"]
["Hydrogen Sulfide","H2S","7783-06-4","H2S","ES","ESM-237","Fixed","GD-K88Di Series","0～30ppm"]
["Hydrogen Sulfide","H2S","7783-06-4","H2S","ES","ESM-237iF","Fixed","GD-K88Ai Series","0～1ppm"]
["Hydrogen Sulfide","H2S","7783-06-4","H2S","ES","ESM-237iF","Fixed","GD-K88Di Series","0～1ppm"]
["Hydrogen Sulfide","H2S","7783-06-4","H2S","ES","ESM-237iF","Fixed","GD-K88Ai Series","0～3ppm"]
["Hydrogen Sulfide","H2S","7783-06-4","H2S","ES","ESM-237iF","Fixed","GD-K88Di Series","0～3ppm"]
["Hydrogen Sulfide","H2S","7783-06-4","H2S","ES","ESM-237iF","Fixed","GD-K88Ai Series","0～30ppm"]
["Hydrogen Sulfide","H2S","7783-06-4","H2S","ES","ESM-237iF","Fixed","GD-K88Di Series","0～30ppm"]
["Hydrogen Sulfide","H2S","7783-06-4","H2S","ES","ESM-237iH","Fixed","GD-K88Ai Series","0～3ppm"]
["Hydrogen Sulfide","H2S","7783-06-4","H2S","ES","ESM-237iH","Fixed","GD-K88Di Series","0～3ppm"]
["Hydrogen Sulfide","H2S","7783-06-4","H2S","ES","ESM-237iH","Fixed","GD-K88Ai Series","0～30ppm"]
["Hydrogen Sulfide","H2S","7783-06-4","H2S","ES","ESM-237iH","Fixed","GD-K88Di Series","0～30ppm"]
["Hydrogen Sulfide","H2S","7783-06-4","H2S","ES","ESM-23AH","Fixed","GD-K88Ai Series","0～1ppm"]
["Hydrogen Sulfide","H2S","7783-06-4","H2S","ES","ESM-23AH","Fixed","GD-K88Di Series","0～1ppm"]
["Hydrogen Sulfide","H2S","7783-06-4","H2S","SG","SG-8564","Fixed","GD-A80V Series","0～20ppm/0～30ppm/0～50ppm/0～100ppm"]
["Hydrogen Sulfide","H2S","7783-06-4","H2S","SG","SG-8564","Fixed","GD-D58・GH Series","0～20ppm/0～30ppm/0～50ppm/0～100ppm"]
["Hydrogen Sulfide","H2S","7783-06-4","H2S","SG","SG-8564","Fixed","SD-1GH Series","0～20ppm/0～30ppm/0～50ppm/0～100ppm"]
["Hydrogen Sulfide","H2S","7783-06-4","H2S","SG","SG-8564","Fixed","SD-D58・GH Series","0～20ppm/0～30ppm/0～50ppm/0～100ppm"]
["Hydroxylamine","NH2OH","7803-49-8","NH2OH","SG","SG-8562","Fixed","GD-A80V Series","0～500ppm","50% solution"]
["Hydroxylamine","NH2OH","7803-49-8","NH2OH","SG","SG-8562","Fixed","GD-D58・GH Series","0～500ppm","50% solution"]
["Hydroxylamine","NH2OH","7803-49-8","NH2OH","SG","SG-8562","Fixed","SD-1GH Series","0～500ppm","50% solution"]
["Hydroxylamine","NH2OH","7803-49-8","NH2OH","SG","SG-8562","Fixed","SD-D58・GH Series","0～500ppm","50% solution"]
["i-Butyraldehyde","i-C4H8O","78-84-2","C4H8O","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["i-Butyraldehyde","i-C4H8O","78-84-2","C4H8O","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["i-Butyraldehyde","i-C4H8O","78-84-2","C4H8O","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～16000ppm"]
["i-Butyraldehyde","i-C4H8O","78-84-2","C4H8O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～16000ppm"]
["i-Butyraldehyde","i-C4H8O","78-84-2","C4H8O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～16000ppm"]
["i-Butyraldehyde","i-C4H8O","78-84-2","C4H8O","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～16000ppm"]
["i-Butyraldehyde","i-C4H8O","78-84-2","C4H8O","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～16000ppm"]
["Iodine","I2","7553-56-2","I2","ES","ESM-K233","Portable","SC-8000","0～1ppm"]
["Iodine","I2","7553-56-2","I2","ES","ESU-K233","Fixed","GD-70D Series","0～1ppm"]
["Iodine","I2","7553-56-2","I2","ES","ESU-K233","Fixed","TP-70D","0～1ppm"]
["Iodine","I2","7553-56-2","I2","ES","ESM-K233","Fixed","GD-K88Ai Series","0～1ppm"]
["Iodine","I2","7553-56-2","I2","ES","ESM-K233","Fixed","GD-K88Di Series","0～1ppm"]
["Iodotrifluoromethane","CF3I","2314-97-8","CF3I","RI","DE-2113-35","Fixed","RI-257","0～5000ppm"]
["Isobutane","i-C4H10","75-28-5","C4H10","HW","NC-6264AZP","Portable","GX-2009","0～100%LEL"]
["Isobutane","i-C4H10","75-28-5","C4H10","HW","NC-6264AZP","Portable","GX-2012","0～100%LEL"]
["Isobutane","i-C4H10","75-28-5","C4H10","HW","NC-6264AZP","Portable","GX-2012GT","0～100%LEL"]
["Isobutane","i-C4H10","75-28-5","C4H10","HW","NC-6264AZP","Portable","GX-6000","0～100%LEL"]
["Isobutane","i-C4H10","75-28-5","C4H10","HW","NC-6264AZP","Portable","GP-03","0～100%LEL"]
["Isobutane","i-C4H10","75-28-5","C4H10","HW","NC-6215","Portable","GX-8000","0～100%LEL"]
["Isobutane","i-C4H10","75-28-5","C4H10","HW","NC-6215","Portable","GX-8000(TYPE LEL)","0～100%LEL"]
["Isobutane","i-C4H10","75-28-5","C4H10","HW","NC-6215","Portable","GP-1000(HC/CH4)","0～100%LEL"]
["Isobutane","i-C4H10","75-28-5","C4H10","SH","SH-8641","Portable","GX-2012GT","0～2000ppm"]
["Isobutane","i-C4H10","75-28-5","C4H10","TE","TE-7515","Portable","GX-8000","0～100vol%"]
["Isobutane","i-C4H10","75-28-5","C4H10","RI","DE-3123-4","Portable","RX-8000","0～100%LEL～100vol%"]
["Isobutane","i-C4H10","75-28-5","C4H10","RI","DE-3123-4","Portable","RX-8700","0～100%LEL～100vol%"]
["Isobutane","i-C4H10","75-28-5","C4H10","HW","NC-6307","Portable","NC-1000(HC/CH4)","0～10000ppm"]
["Isobutane","i-C4H10","75-28-5","C4H10","TE","TE-7515W","Portable","NP-1000(CH4)","0～100vol%"]
["Isobutane","i-C4H10","75-28-5","C4H10","SH","SH-8662","Portable","SP-220(TYPE SC)","0～10ppm"]
["Isobutane","i-C4H10","75-28-5","C4H10","SH","SH-8661","Portable","SP-220(TYPE L)","0～10000ppm"]
["Isobutane","i-C4H10","75-28-5","C4H10","SH","SH-8661","Portable","SP-220(TYPE ML)","0～10000ppm"]
["Isobutane","i-C4H10","75-28-5","C4H10","SH","SH-8661","Portable","SP-220(TYPE F)","0～10000ppm"]
["Isobutane","i-C4H10","75-28-5","C4H10","SH","SH-8661","Portable","SP-220(TYPE H2)","0～10000ppm"]
["Isobutane","i-C4H10","75-28-5","C4H10","RI","DES-3311-2","Portable","GX-6000","0～100%LEL～30vol%"]
["Isobutane","i-C4H10","75-28-5","C4H10","SG","SGU-8521","Fixed","GD-70D Series","0～2000ppm"]
["Isobutane","i-C4H10","75-28-5","C4H10","SG","SGU-8521","Fixed","TP-70D","0～2000ppm"]
["Isobutane","i-C4H10","75-28-5","C4H10","HW","NCU-6211","Fixed","GD-70D Series","0～100%LEL","Confirm that GD-70D is non-explosion proof"]
["Isobutane","i-C4H10","75-28-5","C4H10","HW","NCU-6211","Fixed","TP-70D","0～100%LEL","Confirm that GD-70D is non-explosion proof"]
["Isobutane","i-C4H10","75-28-5","C4H10","RI","DET-6520-2","Fixed","SDWL-1RI Series","0～100%LEL"]
["Isobutane","i-C4H10","75-28-5","C4H10","RI","DE-2113-62","Fixed","RI-557","0～2vol%"]
["Isobutane","i-C4H10","75-28-5","C4H10","RI","DE-2113-58","Fixed","RI-557","0～5vol%"]
["Isobutane","i-C4H10","75-28-5","C4H10","RI","DE-2113-60","Fixed","RI-557","0～20vol%"]
["Isobutane","i-C4H10","75-28-5","C4H10","RI","DE-3315-2","Fixed","SD-1RI Series","0～100%LEL"]
["Isobutane","i-C4H10","75-28-5","C4H10","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Isobutane","i-C4H10","75-28-5","C4H10","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Isobutane","i-C4H10","75-28-5","C4H10","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～18000ppm"]
["Isobutane","i-C4H10","75-28-5","C4H10","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～18000ppm"]
["Isobutane","i-C4H10","75-28-5","C4H10","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～18000ppm"]
["Isobutane","i-C4H10","75-28-5","C4H10","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～18000ppm"]
["Isobutane","i-C4H10","75-28-5","C4H10","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～18000ppm"]
["Isobutane","i-C4H10","75-28-5","C4H10","HW","HW-6213/NC-6213","Fixed","GD-A80 Series","0～100%LEL/0～40000ppm"]
["Isobutane","i-C4H10","75-28-5","C4H10","HW","HW-6213/NC-6213","Fixed","GD-D58(TYPE GP) Series","0～100%LEL/0～40000ppm"]
["Isobutane","i-C4H10","75-28-5","C4H10","HW","HW-6213/NC-6213","Fixed","GD-D58(TYPE NC) Series","0～100%LEL/0～40000ppm"]
["Isobutane","i-C4H10","75-28-5","C4H10","HW","HW-6239","Fixed","GD-A80-70 Series","0～100%LEL"]
["Isobutane","i-C4H10","75-28-5","C4H10","HW","HW-6239","Fixed","SD-1(TYPE GP) Series","0～100%LEL"]
["Isobutane","i-C4H10","75-28-5","C4H10","HW","HW-6239","Fixed","SD-D58(TYPE GP) Series","0～100%LEL"]
["Isobutane","i-C4H10","75-28-5","C4H10","HW","HW-6239/NC-6239","Fixed","GD-A80 Series","0～100%LEL/0～18000ppm"]
["Isobutane","i-C4H10","75-28-5","C4H10","HW","HW-6239/NC-6239","Fixed","GD-D58(TYPE GP) Series","0～100%LEL/0～18000ppm"]
["Isobutane","i-C4H10","75-28-5","C4H10","HW","HW-6239/NC-6239","Fixed","GD-D58(TYPE NC) Series","0～100%LEL/0～18000ppm"]
["Isobutane","i-C4H10","75-28-5","C4H10","HW","HW-6239/NC-6239","Fixed","SD-1(TYPE NC) Series","0～100%LEL/0～18000ppm"]
["Isobutane","i-C4H10","75-28-5","C4H10","HW","HW-6239/NC-6239","Fixed","SD-D58(TYPE NC) Series","0～100%LEL/0～18000ppm"]
["Isobutane","i-C4H10","75-28-5","C4H10","HW","NC-6240A","Fixed","GD-A80 Series","0～100%LEL/0～18000ppm"]
["Isobutane","i-C4H10","75-28-5","C4H10","HW","NC-6240A","Fixed","GD-D58(TYPE NC) Series","0～100%LEL/0～18000ppm"]
["Isobutane","i-C4H10","75-28-5","C4H10","HW","NC-6240A","Fixed","SD-1(TYPE NC) Series","0～100%LEL/0～18000ppm"]
["Isobutane","i-C4H10","75-28-5","C4H10","HW","NC-6240A","Fixed","SD-D58(TYPE NC) Series","0～100%LEL/0～18000ppm"]
["Isobutane","i-C4H10","75-28-5","C4H10","HW","NC-6245","Fixed","GD-A80 Series","0～100%LEL"]
["Isobutane","i-C4H10","75-28-5","C4H10","HW","NC-6245","Fixed","GD-D58(TYPE NC) Series","0～100%LEL"]
["Isobutane","i-C4H10","75-28-5","C4H10","HW","NC-6245","Fixed","SD-1(TYPE NC) Series","0～100%LEL"]
["Isobutane","i-C4H10","75-28-5","C4H10","HW","NC-6245","Fixed","SD-D58(TYPE NC) Series","0～100%LEL"]
["Isobutane","i-C4H10","75-28-5","C4H10","HW","NC-6250","Fixed","GD-A80 Series","0～100%LEL/0～18000ppm"]
["Isobutane","i-C4H10","75-28-5","C4H10","HW","NC-6250","Fixed","GD-D58(TYPE NC) Series","0～100%LEL/0～18000ppm"]
["Isobutane","i-C4H10","75-28-5","C4H10","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Isobutane","i-C4H10","75-28-5","C4H10","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Isobutane","i-C4H10","75-28-5","C4H10","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Isobutane","i-C4H10","75-28-5","C4H10","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Isobutane","i-C4H10","75-28-5","C4H10","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Isobutane","i-C4H10","75-28-5","C4H10","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Isobutane","i-C4H10","75-28-5","C4H10","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Isobutane","i-C4H10","75-28-5","C4H10","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["Isobutane","i-C4H10","75-28-5","C4H10","SG","SG-8511","Fixed","GD-A80V Series","0～3000ppm//0～3500ppm0～5000ppm/0～7000ppm/0～10000ppm/0～18000ppm/0～50%LEL/0～100%LEL"]
["Isobutane","i-C4H10","75-28-5","C4H10","SG","SG-8511","Fixed","GD-D58・GH Series","0～3000ppm//0～3500ppm0～5000ppm/0～7000ppm/0～10000ppm/0～18000ppm/0～50%LEL/0～100%LEL"]
["Isobutane","i-C4H10","75-28-5","C4H10","SG","SG-8511","Fixed","SD-1GH Series","0～3000ppm//0～3500ppm0～5000ppm/0～7000ppm/0～10000ppm/0～18000ppm/0～50%LEL/0～100%LEL"]
["Isobutane","i-C4H10","75-28-5","C4H10","SG","SG-8511","Fixed","SD-D58・GH Series","0～3000ppm//0～3500ppm0～5000ppm/0～7000ppm/0～10000ppm/0～18000ppm/0～50%LEL/0～100%LEL"]
["Isobutane","i-C4H10","75-28-5","C4H10","SG","SG-8521","Fixed","GD-A80V Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Isobutane","i-C4H10","75-28-5","C4H10","SG","SG-8521","Fixed","GD-D58・GH Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Isobutane","i-C4H10","75-28-5","C4H10","SG","SG-8521","Fixed","SD-1GH Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Isobutane","i-C4H10","75-28-5","C4H10","SG","SG-8521","Fixed","SD-D58・GH Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Isobutane","i-C4H10","75-28-5","C4H10","SG","SG-8582","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Isobutane","i-C4H10","75-28-5","C4H10","SG","SG-8582","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Isobutane","i-C4H10","75-28-5","C4H10","SG","SG-8582","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Isobutane","i-C4H10","75-28-5","C4H10","SG","SG-8582","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Isobutane","i-C4H10","75-28-5","C4H10","SG","SG-8586","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Isobutane","i-C4H10","75-28-5","C4H10","SG","SG-8586","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Isobutane","i-C4H10","75-28-5","C4H10","SG","SG-8586","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Isobutane","i-C4H10","75-28-5","C4H10","SG","SG-8586","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Isobutanol","IBA","78-83-1","C4H10O","HW","NC-6215","Portable","GP-1000(Specified cal.gas)","0～100%LEL"]
["Isobutanol","IBA","78-83-1","C4H10O","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Isobutanol","IBA","78-83-1","C4H10O","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Isobutanol","IBA","78-83-1","C4H10O","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～17000ppm"]
["Isobutanol","IBA","78-83-1","C4H10O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～17000ppm"]
["Isobutanol","IBA","78-83-1","C4H10O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～17000ppm"]
["Isobutanol","IBA","78-83-1","C4H10O","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～17000ppm"]
["Isobutanol","IBA","78-83-1","C4H10O","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～17000ppm"]
["Isobutanol","IBA","78-83-1","C4H10O","SG","SG-8521","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Isobutanol","IBA","78-83-1","C4H10O","SG","SG-8521","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Isobutanol","IBA","78-83-1","C4H10O","SG","SG-8521","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Isobutanol","IBA","78-83-1","C4H10O","SG","SG-8521","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Isobuten","i-C4H8","115-11-7","C4H8","SH","SH-8661","Portable","SP-220(TYPE H2)","0～10000ppm"]
["Isobuten","i-C4H8","115-11-7","C4H8","PID","PSI-001","Portable","GX-6000","0～50000ppb"]
["Isobuten","i-C4H8","115-11-7","C4H8","PID","PSI-002","Portable","GX-6000","0～6000ppm"]
["Isobuten","i-C4H8","115-11-7","C4H8","PID","PSI-003","Portable","GX-6000","0～100ppm"]
["Isobuten","i-C4H8","115-11-7","C4H8","HW","NC-6215","Portable","GP-1000(Specified cal.gas)","0～100%LEL"]
["Isobuten","i-C4H8","115-11-7","C4H8","SG","SGU-8521","Fixed","GD-70D Series","0～2000ppm"]
["Isobuten","i-C4H8","115-11-7","C4H8","SG","SGU-8521","Fixed","TP-70D","0～2000ppm"]
["Isobuten","i-C4H8","115-11-7","C4H8","RI","DE-3315-2","Fixed","SD-1RI Series","0～100%LEL"]
["Isobuten","i-C4H8","115-11-7","C4H8","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Isobuten","i-C4H8","115-11-7","C4H8","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Isobuten","i-C4H8","115-11-7","C4H8","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～18000ppm"]
["Isobuten","i-C4H8","115-11-7","C4H8","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～18000ppm"]
["Isobuten","i-C4H8","115-11-7","C4H8","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～18000ppm"]
["Isobuten","i-C4H8","115-11-7","C4H8","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～18000ppm"]
["Isobuten","i-C4H8","115-11-7","C4H8","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～18000ppm"]
["Isobuten","i-C4H8","115-11-7","C4H8","HW","HW-6239","Fixed","GD-A80-70 Series","0～100%LEL"]
["Isobuten","i-C4H8","115-11-7","C4H8","HW","HW-6239","Fixed","SD-1(TYPE GP) Series","0～100%LEL"]
["Isobuten","i-C4H8","115-11-7","C4H8","HW","HW-6239","Fixed","SD-D58(TYPE GP) Series","0～100%LEL"]
["Isobuten","i-C4H8","115-11-7","C4H8","HW","HW-6239/NC-6239","Fixed","GD-A80 Series","0～100%LEL/0～18000ppm"]
["Isobuten","i-C4H8","115-11-7","C4H8","HW","HW-6239/NC-6239","Fixed","GD-D58(TYPE GP) Series","0～100%LEL/0～18000ppm"]
["Isobuten","i-C4H8","115-11-7","C4H8","HW","HW-6239/NC-6239","Fixed","GD-D58(TYPE NC) Series","0～100%LEL/0～18000ppm"]
["Isobuten","i-C4H8","115-11-7","C4H8","HW","HW-6239/NC-6239","Fixed","SD-1(TYPE NC) Series","0～100%LEL/0～18000ppm"]
["Isobuten","i-C4H8","115-11-7","C4H8","HW","HW-6239/NC-6239","Fixed","SD-D58(TYPE NC) Series","0～100%LEL/0～18000ppm"]
["Isobuten","i-C4H8","115-11-7","C4H8","SG","SG-8521","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Isobuten","i-C4H8","115-11-7","C4H8","SG","SG-8521","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Isobuten","i-C4H8","115-11-7","C4H8","SG","SG-8521","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Isobuten","i-C4H8","115-11-7","C4H8","SG","SG-8521","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Isobutyl acetate","AcOBu","110-19-0","C6H12O2","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Isobutyl acetate","AcOBu","110-19-0","C6H12O2","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Isobutyl acetate","AcOBu","110-19-0","C6H12O2","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～13000ppm"]
["Isobutyl acetate","AcOBu","110-19-0","C6H12O2","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～13000ppm"]
["Isobutyl acetate","AcOBu","110-19-0","C6H12O2","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～13000ppm"]
["Isobutyl acetate","AcOBu","110-19-0","C6H12O2","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～13000ppm"]
["Isobutyl acetate","AcOBu","110-19-0","C6H12O2","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～13000ppm"]
["Isobutyl Acrylate","i-BA","106-63-8","C7H12O2","SG","SG-8521","Fixed","GD-A80V Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["Isobutyl Acrylate","i-BA","106-63-8","C7H12O2","SG","SG-8521","Fixed","GD-D58・GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["Isobutyl Acrylate","i-BA","106-63-8","C7H12O2","SG","SG-8521","Fixed","SD-1GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["Isobutyl Acrylate","i-BA","106-63-8","C7H12O2","SG","SG-8521","Fixed","SD-D58・GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["Isododecane","iC12H26","31807-55-3","C12H26","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Isododecane","iC12H26","31807-55-3","C12H26","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Isododecane","iC12H26","31807-55-3","C12H26","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Isododecane","iC12H26","31807-55-3","C12H26","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Isododecane","iC12H26","31807-55-3","C12H26","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Isododecane","iC12H26","31807-55-3","C12H26","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Isododecane","iC12H26","31807-55-3","C12H26","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Isododecane","iC12H26","31807-55-3","C12H26","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["Isododecane","iC12H26","31807-55-3","C12H26","SG","SG-8521","Fixed","GD-A80V Series","0～30ppm/0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Isododecane","iC12H26","31807-55-3","C12H26","SG","SG-8521","Fixed","GD-D58・GH Series","0～30ppm/0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Isododecane","iC12H26","31807-55-3","C12H26","SG","SG-8521","Fixed","SD-1GH Series","0～30ppm/0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Isododecane","iC12H26","31807-55-3","C12H26","SG","SG-8521","Fixed","SD-D58・GH Series","0～30ppm/0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Isohexane","i-C6H14","110-54-3","C6H14","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Isohexane","i-C6H14","110-54-3","C6H14","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Isohexane","i-C6H14","110-54-3","C6H14","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～11000ppm"]
["Isohexane","i-C6H14","110-54-3","C6H14","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～11000ppm"]
["Isohexane","i-C6H14","110-54-3","C6H14","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～11000ppm"]
["Isohexane","i-C6H14","110-54-3","C6H14","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～11000ppm"]
["Isohexane","i-C6H14","110-54-3","C6H14","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～11000ppm"]
["Isooctane","i-C8H18","540-84-1","C8H18","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Isooctane","i-C8H18","540-84-1","C8H18","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Isooctane","i-C8H18","540-84-1","C8H18","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～8000ppm"]
["Isooctane","i-C8H18","540-84-1","C8H18","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～8000ppm"]
["Isooctane","i-C8H18","540-84-1","C8H18","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～8000ppm"]
["Isooctane","i-C8H18","540-84-1","C8H18","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～8000ppm"]
["Isooctane","i-C8H18","540-84-1","C8H18","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～8000ppm"]
["ISOPAR H FLUID","ISOPARH","64742-48-9","-","HW","NC-6307","Portable","NC-1000(Specified cal. Gas)","0～10000ppm"]
["IsoPentane","i-C5H12","78-78-4","C5H12","RI","DE-3315-2","Fixed","SD-1RI Series","0～100%LEL"]
["IsoPentane","i-C5H12","78-78-4","C5H12","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["IsoPentane","i-C5H12","78-78-4","C5H12","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["IsoPentane","i-C5H12","78-78-4","C5H12","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～13000ppm"]
["IsoPentane","i-C5H12","78-78-4","C5H12","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～13000ppm"]
["IsoPentane","i-C5H12","78-78-4","C5H12","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～13000ppm"]
["IsoPentane","i-C5H12","78-78-4","C5H12","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～13000ppm"]
["IsoPentane","i-C5H12","78-78-4","C5H12","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～13000ppm"]
["IsoPentane","i-C5H12","78-78-4","C5H12","SG","SG-8521","Fixed","GD-A80V Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["IsoPentane","i-C5H12","78-78-4","C5H12","SG","SG-8521","Fixed","GD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["IsoPentane","i-C5H12","78-78-4","C5H12","SG","SG-8521","Fixed","SD-1GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["IsoPentane","i-C5H12","78-78-4","C5H12","SG","SG-8521","Fixed","SD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Isopentyl acetate","iPenOAc","123-92-2","C7H14O2","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Isopentyl acetate","iPenOAc","123-92-2","C7H14O2","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Isopentyl acetate","iPenOAc","123-92-2","C7H14O2","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～10000ppm"]
["Isopentyl acetate","iPenOAc","123-92-2","C7H14O2","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～10000ppm"]
["Isopentyl acetate","iPenOAc","123-92-2","C7H14O2","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～10000ppm"]
["Isopentyl acetate","iPenOAc","123-92-2","C7H14O2","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～10000ppm"]
["Isopentyl acetate","iPenOAc","123-92-2","C7H14O2","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～10000ppm"]
["Isopentyl acetate","iPenOAc","123-92-2","C7H14O2","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Isopentyl acetate","iPenOAc","123-92-2","C7H14O2","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Isopentyl acetate","iPenOAc","123-92-2","C7H14O2","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Isopentyl acetate","iPenOAc","123-92-2","C7H14O2","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Isopentyl acetate","iPenOAc","123-92-2","C7H14O2","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Isopentyl acetate","iPenOAc","123-92-2","C7H14O2","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Isopentyl acetate","iPenOAc","123-92-2","C7H14O2","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Isopentyl acetate","iPenOAc","123-92-2","C7H14O2","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["Isophorone","C9H14O","78-59-1","C9H14O","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Isophorone","C9H14O","78-59-1","C9H14O","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Isophorone","C9H14O","78-59-1","C9H14O","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Isophorone","C9H14O","78-59-1","C9H14O","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Isophorone","C9H14O","78-59-1","C9H14O","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Isophorone","C9H14O","78-59-1","C9H14O","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Isophorone","C9H14O","78-59-1","C9H14O","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Isophorone","C9H14O","78-59-1","C9H14O","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["Isophorone","C9H14O","78-59-1","C9H14O","SG","SG-8521","Fixed","GD-A80V Series","0～50ppm/0～100ppm"]
["Isophorone","C9H14O","78-59-1","C9H14O","SG","SG-8521","Fixed","GD-D58・GH Series","0～50ppm/0～100ppm"]
["Isophorone","C9H14O","78-59-1","C9H14O","SG","SG-8521","Fixed","SD-1GH Series","0～50ppm/0～100ppm"]
["Isophorone","C9H14O","78-59-1","C9H14O","SG","SG-8521","Fixed","SD-D58・GH Series","0～50ppm/0～100ppm"]
["Isoprene","C5H8","78-79-5","C5H8","HW","NC-6215","Portable","GP-1000(Specified cal.gas)","0～100%LEL"]
["Isoprene","C5H8","78-79-5","C5H8","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Isoprene","C5H8","78-79-5","C5H8","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Isoprene","C5H8","78-79-5","C5H8","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～10000ppm"]
["Isoprene","C5H8","78-79-5","C5H8","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～10000ppm"]
["Isoprene","C5H8","78-79-5","C5H8","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～10000ppm"]
["Isoprene","C5H8","78-79-5","C5H8","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～10000ppm"]
["Isoprene","C5H8","78-79-5","C5H8","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～10000ppm"]
["Isoprene","C5H8","78-79-5","C5H8","HW","NC-6250","Fixed","GD-A80 Series","0～100%LEL/0～10000ppm"]
["Isoprene","C5H8","78-79-5","C5H8","HW","NC-6250","Fixed","GD-D58(TYPE NC) Series","0～100%LEL/0～10000ppm"]
["Isoprene","C5H8","78-79-5","C5H8","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Isoprene","C5H8","78-79-5","C5H8","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Isoprene","C5H8","78-79-5","C5H8","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Isoprene","C5H8","78-79-5","C5H8","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Isoprene","C5H8","78-79-5","C5H8","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Isoprene","C5H8","78-79-5","C5H8","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Isoprene","C5H8","78-79-5","C5H8","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Isoprene","C5H8","78-79-5","C5H8","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["Isoprene","C5H8","78-79-5","C5H8","SG","SG-8521","Fixed","GD-A80V Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Isoprene","C5H8","78-79-5","C5H8","SG","SG-8521","Fixed","GD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Isoprene","C5H8","78-79-5","C5H8","SG","SG-8521","Fixed","SD-1GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Isoprene","C5H8","78-79-5","C5H8","SG","SG-8521","Fixed","SD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Isopropyl Alcohol","IPA","67-63-0","C3H8O","HW","NC-6215","Portable","GP-1000(HC/CH4)","0～100%LEL"]
["Isopropyl Alcohol","IPA","67-63-0","C3H8O","HW","NC-6307","Portable","NC-1000(HC/CH4)","0～10000ppm"]
["Isopropyl Alcohol","IPA","67-63-0","C3H8O","SH","SH-8662","Portable","SP-220(TYPE SC)","0～10ppm"]
["Isopropyl Alcohol","IPA","67-63-0","C3H8O","SG","SGU-8521","Fixed","GD-70D Series","0～2000ppm"]
["Isopropyl Alcohol","IPA","67-63-0","C3H8O","SG","SGU-8521","Fixed","TP-70D","0～2000ppm"]
["Isopropyl Alcohol","IPA","67-63-0","C3H8O","HW","NCU-6211","Fixed","GD-70D Series","0～100%LEL","Confirm that GD-70D is non-explosion proof"]
["Isopropyl Alcohol","IPA","67-63-0","C3H8O","HW","NCU-6211","Fixed","TP-70D","0～100%LEL","Confirm that GD-70D is non-explosion proof"]
["Isopropyl Alcohol","IPA","67-63-0","C3H8O","HW","NCU-6250","Fixed","GD-70D Series","0～100%LEL","Confirm that GD-70D is non-explosion proof"]
["Isopropyl Alcohol","IPA","67-63-0","C3H8O","HW","NCU-6250","Fixed","TP-70D","0～100%LEL","Confirm that GD-70D is non-explosion proof"]
["Isopropyl Alcohol","IPA","67-63-0","C3H8O","RI","DE-2113-35","Fixed","RI-257","0～10000ppm"]
["Isopropyl Alcohol","IPA","67-63-0","C3H8O","RI","DE-3315-2","Fixed","SD-1RI Series","0～100%LEL"]
["Isopropyl Alcohol","IPA","67-63-0","C3H8O","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Isopropyl Alcohol","IPA","67-63-0","C3H8O","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Isopropyl Alcohol","IPA","67-63-0","C3H8O","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～20000ppm"]
["Isopropyl Alcohol","IPA","67-63-0","C3H8O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～20000ppm"]
["Isopropyl Alcohol","IPA","67-63-0","C3H8O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～20000ppm"]
["Isopropyl Alcohol","IPA","67-63-0","C3H8O","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～20000ppm"]
["Isopropyl Alcohol","IPA","67-63-0","C3H8O","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～20000ppm"]
["Isopropyl Alcohol","IPA","67-63-0","C3H8O","HW","NC-6250","Fixed","GD-A80 Series","0～100%LEL/0～20000ppm"]
["Isopropyl Alcohol","IPA","67-63-0","C3H8O","HW","NC-6250","Fixed","GD-D58(TYPE NC) Series","0～100%LEL/0～20000ppm"]
["Isopropyl Alcohol","IPA","67-63-0","C3H8O","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Isopropyl Alcohol","IPA","67-63-0","C3H8O","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Isopropyl Alcohol","IPA","67-63-0","C3H8O","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Isopropyl Alcohol","IPA","67-63-0","C3H8O","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Isopropyl Alcohol","IPA","67-63-0","C3H8O","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Isopropyl Alcohol","IPA","67-63-0","C3H8O","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Isopropyl Alcohol","IPA","67-63-0","C3H8O","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Isopropyl Alcohol","IPA","67-63-0","C3H8O","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["Isopropyl Alcohol","IPA","67-63-0","C3H8O","SG","SG-8511","Fixed","GD-A80V Series","0～3000ppm/0～5000ppm/0～10000ppm"]
["Isopropyl Alcohol","IPA","67-63-0","C3H8O","SG","SG-8511","Fixed","GD-D58・GH Series","0～3000ppm/0～5000ppm/0～10000ppm"]
["Isopropyl Alcohol","IPA","67-63-0","C3H8O","SG","SG-8511","Fixed","SD-1GH Series","0～3000ppm/0～5000ppm/0～10000ppm"]
["Isopropyl Alcohol","IPA","67-63-0","C3H8O","SG","SG-8511","Fixed","SD-D58・GH Series","0～3000ppm/0～5000ppm/0～10000ppm"]
["Isopropyl Alcohol","IPA","67-63-0","C3H8O","SG","SG-8521","Fixed","GD-A80V Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Isopropyl Alcohol","IPA","67-63-0","C3H8O","SG","SG-8521","Fixed","GD-D58・GH Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Isopropyl Alcohol","IPA","67-63-0","C3H8O","SG","SG-8521","Fixed","SD-1GH Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Isopropyl Alcohol","IPA","67-63-0","C3H8O","SG","SG-8521","Fixed","SD-D58・GH Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Isopropyl Alcohol","IPA","67-63-0","C3H8O","SG","SG-8565","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Isopropyl Alcohol","IPA","67-63-0","C3H8O","SG","SG-8565","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Isopropyl Alcohol","IPA","67-63-0","C3H8O","SG","SG-8565","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Isopropyl Alcohol","IPA","67-63-0","C3H8O","SG","SG-8565","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Isopropyl chloride","IPC","75-29-6","C3H7CL","SG","SG-8523","Fixed","GD-A80V Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Isopropyl chloride","IPC","75-29-6","C3H7CL","SG","SG-8523","Fixed","GD-D58・GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Isopropyl chloride","IPC","75-29-6","C3H7CL","SG","SG-8523","Fixed","SD-1GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Isopropyl chloride","IPC","75-29-6","C3H7CL","SG","SG-8523","Fixed","SD-D58・GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Isopropyl ether","IPE","108-20-3","C6H14O","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Isopropyl ether","IPE","108-20-3","C6H14O","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Isopropyl ether","IPE","108-20-3","C6H14O","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～14000ppm"]
["Isopropyl ether","IPE","108-20-3","C6H14O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～14000ppm"]
["Isopropyl ether","IPE","108-20-3","C6H14O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～14000ppm"]
["Isopropyl ether","IPE","108-20-3","C6H14O","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～14000ppm"]
["Isopropyl ether","IPE","108-20-3","C6H14O","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～14000ppm"]
["Isopropyl ether","IPE","108-20-3","C6H14O","SG","SG-8521","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Isopropyl ether","IPE","108-20-3","C6H14O","SG","SG-8521","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Isopropyl ether","IPE","108-20-3","C6H14O","SG","SG-8521","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Isopropyl ether","IPE","108-20-3","C6H14O","SG","SG-8521","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["JET-A1","JET-A1","-","-","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["JET-A1","JET-A1","-","-","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["JET-A1","JET-A1","-","-","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～7000ppm"]
["JET-A1","JET-A1","-","-","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～7000ppm"]
["JET-A1","JET-A1","-","-","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～7000ppm"]
["JET-A1","JET-A1","-","-","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～7000ppm"]
["JET-A1","JET-A1","-","-","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～7000ppm"]
["JP-4","JP-4","-","-","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～50%LEL/～5000ppm"]
["JP-4","JP-4","-","-","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～50%LEL/～5000ppm"]
["JP-4","JP-4","-","-","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～50%LEL/～5000ppm"]
["JP-4","JP-4","-","-","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～50%LEL/～5000ppm"]
["JP-4","JP-4","-","-","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～50%LEL/～5000ppm"]
["JP-4","JP-4","-","-","SG","SG-8521","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["JP-4","JP-4","-","-","SG","SG-8521","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["JP-4","JP-4","-","-","SG","SG-8521","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["JP-4","JP-4","-","-","SG","SG-8521","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["JP-5","JP-5","-","-","SG","SG-8521","Fixed","GD-A80V Series","0～100ppm/0～200ppm"]
["JP-5","JP-5","-","-","SG","SG-8521","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm"]
["JP-5","JP-5","-","-","SG","SG-8521","Fixed","SD-1GH Series","0～100ppm/0～200ppm"]
["JP-5","JP-5","-","-","SG","SG-8521","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm"]
["JP-8","JP-8","-","-","HW","NC-6211","Fixed","GD-A80 Series","～50%LEL/～4500ppm"]
["JP-8","JP-8","-","-","HW","NC-6211","Fixed","GD-D58(TYPE GP) Series","～50%LEL/～4500ppm"]
["JP-8","JP-8","-","-","HW","NC-6211","Fixed","GD-D58(TYPE NC) Series","～50%LEL/～4500ppm"]
["JP-8","JP-8","-","-","HW","NC-6211","Fixed","SD-1(TYPE NC) Series","～50%LEL/～4500ppm"]
["JP-8","JP-8","-","-","HW","NC-6211","Fixed","SD-D58(TYPE NC) Series","～50%LEL/～4500ppm"]
["Kerosene","KEROSEN","8008-20-6","-","HW","NC-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL/～7000ppm"]
["Kerosene","KEROSEN","8008-20-6","-","HW","NC-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL/～7000ppm"]
["Kerosene","KEROSEN","8008-20-6","-","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Kerosene","KEROSEN","8008-20-6","-","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Kerosene","KEROSEN","8008-20-6","-","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Kerosene","KEROSEN","8008-20-6","-","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Kerosene","KEROSEN","8008-20-6","-","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Kerosene","KEROSEN","8008-20-6","-","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Kerosene","KEROSEN","8008-20-6","-","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Kerosene","KEROSEN","8008-20-6","-","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["Kerosene","KEROSEN","8008-20-6","-","SG","SG-8521","Fixed","GD-A80V Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Kerosene","KEROSEN","8008-20-6","-","SG","SG-8521","Fixed","GD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Kerosene","KEROSEN","8008-20-6","-","SG","SG-8521","Fixed","SD-1GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Kerosene","KEROSEN","8008-20-6","-","SG","SG-8521","Fixed","SD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Limonene","LIMONEN","138-86-3,5989-27-5","C10H16","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～90%LEL/～6300ppm"]
["Limonene","LIMONEN","138-86-3,5989-27-5","C10H16","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～90%LEL/～6300ppm"]
["Limonene","LIMONEN","138-86-3,5989-27-5","C10H16","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～90%LEL/～6300ppm"]
["Limonene","LIMONEN","138-86-3,5989-27-5","C10H16","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～90%LEL/～6300ppm"]
["Limonene","LIMONEN","138-86-3,5989-27-5","C10H16","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～90%LEL/～6300ppm"]
["LPG","LPG","-","-","SG","SGU-8511","Fixed","GD-70D Series","0～10000ppm","Isobutane representative "]
["LPG","LPG","-","-","SG","SGU-8511","Fixed","TP-70D","0～10000ppm","Isobutane representative "]
["Mesityl oxide","MO","141-79-7","C6H10O","SG","SG-8521","Fixed","GD-A80V Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Mesityl oxide","MO","141-79-7","C6H10O","SG","SG-8521","Fixed","GD-D58・GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Mesityl oxide","MO","141-79-7","C6H10O","SG","SG-8521","Fixed","SD-1GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Mesityl oxide","MO","141-79-7","C6H10O","SG","SG-8521","Fixed","SD-D58・GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Methacrolein","C4H6O","78-85-3","C4H6O","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Methacrolein","C4H6O","78-85-3","C4H6O","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Methacrolein","C4H6O","78-85-3","C4H6O","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～11000ppm"]
["Methacrolein","C4H6O","78-85-3","C4H6O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～11000ppm"]
["Methacrolein","C4H6O","78-85-3","C4H6O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～11000ppm"]
["Methacrolein","C4H6O","78-85-3","C4H6O","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～11000ppm"]
["Methacrolein","C4H6O","78-85-3","C4H6O","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～11000ppm"]
["Methacrolein","C4H6O","78-85-3","C4H6O","SG","SG-8521","Fixed","GD-A80V Series","0～500ppm/0～1000ppm/0～2000ppm"]
["Methacrolein","C4H6O","78-85-3","C4H6O","SG","SG-8521","Fixed","GD-D58・GH Series","0～500ppm/0～1000ppm/0～2000ppm"]
["Methacrolein","C4H6O","78-85-3","C4H6O","SG","SG-8521","Fixed","SD-1GH Series","0～500ppm/0～1000ppm/0～2000ppm"]
["Methacrolein","C4H6O","78-85-3","C4H6O","SG","SG-8521","Fixed","SD-D58・GH Series","0～500ppm/0～1000ppm/0～2000ppm"]
["Methacrylic acid","MAA","79-41-4","C4H6O2","HW","NC-6211","Fixed","GD-A80 Series","～25%LEL/～4000ppm"]
["Methacrylic acid","MAA","79-41-4","C4H6O2","HW","NC-6211","Fixed","GD-D58(TYPE GP) Series","～25%LEL/～4000ppm"]
["Methacrylic acid","MAA","79-41-4","C4H6O2","HW","NC-6211","Fixed","GD-D58(TYPE NC) Series","～25%LEL/～4000ppm"]
["Methacrylic acid","MAA","79-41-4","C4H6O2","HW","NC-6211","Fixed","SD-1(TYPE NC) Series","～25%LEL/～4000ppm"]
["Methacrylic acid","MAA","79-41-4","C4H6O2","HW","NC-6211","Fixed","SD-D58(TYPE NC) Series","～25%LEL/～4000ppm"]
["Methacrylic acid","MAA","79-41-4","C4H6O2","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Methacrylic acid","MAA","79-41-4","C4H6O2","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Methacrylic acid","MAA","79-41-4","C4H6O2","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Methacrylic acid","MAA","79-41-4","C4H6O2","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Methacrylic acid","MAA","79-41-4","C4H6O2","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Methacrylic acid","MAA","79-41-4","C4H6O2","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Methacrylic acid","MAA","79-41-4","C4H6O2","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Methacrylic acid","MAA","79-41-4","C4H6O2","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["Methacrylic acid","MAA","79-41-4","C4H6O2","SG","SG-8562","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Methacrylic acid","MAA","79-41-4","C4H6O2","SG","SG-8562","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Methacrylic acid","MAA","79-41-4","C4H6O2","SG","SG-8562","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Methacrylic acid","MAA","79-41-4","C4H6O2","SG","SG-8562","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Methane","CH4","74-82-8","CH4","HW","NC-6264AZP","Portable","GX-2009","0～100%LEL"]
["Methane","CH4","74-82-8","CH4","HW","NC-6264AZP","Portable","GX-2012","0～100%LEL"]
["Methane","CH4","74-82-8","CH4","HW","NC-6264AZP","Portable","GX-2012GT","0～100%LEL"]
["Methane","CH4","74-82-8","CH4","HW","NC-6264AZP","Portable","GX-6000","0～100%LEL"]
["Methane","CH4","74-82-8","CH4","HW","NC-6264AZP","Portable","GP-03","0～100%LEL"]
["Methane","CH4","74-82-8","CH4","HW","NC-6215","Portable","GX-8000","0～100%LEL"]
["Methane","CH4","74-82-8","CH4","HW","NC-6215","Portable","GX-8000(TYPE LEL)","0～100%LEL"]
["Methane","CH4","74-82-8","CH4","HW","NC-6215","Portable","GP-1000(CH4)","0～100%LEL"]
["Methane","CH4","74-82-8","CH4","TE","TE-7561","Portable","GX-2012","0～100vol%"]
["Methane","CH4","74-82-8","CH4","TE","TE-7561","Portable","GX-2012GT","0～100vol%"]
["Methane","CH4","74-82-8","CH4","SH","SH-8641","Portable","GX-2012GT","0～500ppm"]
["Methane","CH4","74-82-8","CH4","TE","TE-7515","Portable","GX-8000","0～100vol%"]
["Methane","CH4","74-82-8","CH4","RI","DE-3113-13","Portable","RX-8000","0～100%LEL～100vol%"]
["Methane","CH4","74-82-8","CH4","RI","DE-3123-5","Portable","RX-8500","0～100%LEL～100vol%"]
["Methane","CH4","74-82-8","CH4","HW","NC-6307","Portable","NC-1000(CH4)","0～10000ppm"]
["Methane","CH4","74-82-8","CH4","TE","TE-7515W","Portable","NP-1000(CH4)","0～100vol%"]
["Methane","CH4","74-82-8","CH4","SH","SH-8662","Portable","SP-220(TYPE SC)","0～20ppm"]
["Methane","CH4","74-82-8","CH4","SH","SH-8661","Portable","SP-220(TYPE M)","0～10000ppm"]
["Methane","CH4","74-82-8","CH4","SH","SH-8661","Portable","SP-220(TYPE ML)","0～10000ppm"]
["Methane","CH4","74-82-8","CH4","SH","SH-8661","Portable","SP-220(TYPE H2)","0～10000ppm"]
["Methane","CH4","74-82-8","CH4","RI","DES-3311-3","Portable","GX-6000","0～100%LEL～100vol%"]
["Methane","CH4","74-82-8","CH4","SG","SGU-8511","Fixed","GD-70D Series","0～2.00vol%"]
["Methane","CH4","74-82-8","CH4","SG","SGU-8511","Fixed","TP-70D","0～2.00vol%"]
["Methane","CH4","74-82-8","CH4","SG","SGU-8511","Fixed","GD-70D Series","0～5000ppm"]
["Methane","CH4","74-82-8","CH4","SG","SGU-8511","Fixed","TP-70D","0～5000ppm"]
["Methane","CH4","74-82-8","CH4","SG","SGU-8581","Fixed","GD-70D Series","0～2000ppm"]
["Methane","CH4","74-82-8","CH4","SG","SGU-8581","Fixed","TP-70D","0～2000ppm"]
["Methane","CH4","74-82-8","CH4","SG","SGU-8581A","Fixed","GD-70D Series","0～2000ppm","Only for TSMC"]
["Methane","CH4","74-82-8","CH4","SG","SGU-8581A","Fixed","TP-70D","0～2000ppm","Only for TSMC"]
["Methane","CH4","74-82-8","CH4","SG","SGU-8581","Fixed","GD-70D Series","0～5000ppm"]
["Methane","CH4","74-82-8","CH4","SG","SGU-8581","Fixed","TP-70D","0～5000ppm"]
["Methane","CH4","74-82-8","CH4","HW","NCU-6213","Fixed","GD-70D Series","0～100%LEL","Confirm that GD-70D is non-explosion proof"]
["Methane","CH4","74-82-8","CH4","HW","NCU-6213","Fixed","TP-70D","0～100%LEL","Confirm that GD-70D is non-explosion proof"]
["Methane","CH4","74-82-8","CH4","HW","NCU-6213","Fixed","GD-70D Series","0～2vol%"]
["Methane","CH4","74-82-8","CH4","HW","NCU-6213","Fixed","TP-70D","0～2vol%"]
["Methane","CH4","74-82-8","CH4","HW","NCU-6213","Fixed","GD-70D Series","0～20000ppm"]
["Methane","CH4","74-82-8","CH4","HW","NCU-6213","Fixed","TP-70D","0～20000ppm"]
["Methane","CH4","74-82-8","CH4","HW","NCU-6239","Fixed","GD-70D Series","0～100%LEL","Confirm that GD-70D is non-explosion proof"]
["Methane","CH4","74-82-8","CH4","HW","NCU-6239","Fixed","TP-70D","0～100%LEL","Confirm that GD-70D is non-explosion proof"]
["Methane","CH4","74-82-8","CH4","RI","DET-6520-1","Fixed","SDWL-1RI Series","0～100%LEL"]
["Methane","CH4","74-82-8","CH4","RI","DE-2113-50","Fixed","RI-557","0～5vol%"]
["Methane","CH4","74-82-8","CH4","RI","DE-2113-51","Fixed","RI-557","0～20vol%"]
["Methane","CH4","74-82-8","CH4","RI","DE-2113-52","Fixed","RI-557","0～100vol%"]
["Methane","CH4","74-82-8","CH4","RI","DE-3315-1","Fixed","SD-1RI Series","0～100%LEL"]
["Methane","CH4","74-82-8","CH4","RI","DE-3315-1","Fixed","SD-1RI Series","0～100vol%"]
["Methane","CH4","74-82-8","CH4","HW","HW-6213/NC-6213","Fixed","GD-A80 Series","0～100%LEL/0～50000ppm"]
["Methane","CH4","74-82-8","CH4","HW","HW-6213/NC-6213","Fixed","GD-D58(TYPE GP) Series","0～100%LEL/0～50000ppm"]
["Methane","CH4","74-82-8","CH4","HW","HW-6213/NC-6213","Fixed","GD-D58(TYPE NC) Series","0～100%LEL/0～50000ppm"]
["Methane","CH4","74-82-8","CH4","HW","HW-6239","Fixed","GD-A80-70 Series","0～100%LEL"]
["Methane","CH4","74-82-8","CH4","HW","HW-6239","Fixed","SD-1(TYPE GP) Series","0～100%LEL"]
["Methane","CH4","74-82-8","CH4","HW","HW-6239","Fixed","SD-D58(TYPE GP) Series","0～100%LEL"]
["Methane","CH4","74-82-8","CH4","HW","HW-6239/NC-6239","Fixed","GD-A80 Series","0～100%LEL/0～50000ppm"]
["Methane","CH4","74-82-8","CH4","HW","HW-6239/NC-6239","Fixed","GD-D58(TYPE GP) Series","0～100%LEL/0～50000ppm"]
["Methane","CH4","74-82-8","CH4","HW","HW-6239/NC-6239","Fixed","GD-D58(TYPE NC) Series","0～100%LEL/0～50000ppm"]
["Methane","CH4","74-82-8","CH4","HW","HW-6239/NC-6239","Fixed","SD-1(TYPE NC) Series","0～100%LEL/0～50000ppm"]
["Methane","CH4","74-82-8","CH4","HW","HW-6239/NC-6239","Fixed","SD-D58(TYPE NC) Series","0～100%LEL/0～50000ppm"]
["Methane","CH4","74-82-8","CH4","HW","NC-6240A","Fixed","GD-A80 Series","0～100%LEL/0～50000ppm"]
["Methane","CH4","74-82-8","CH4","HW","NC-6240A","Fixed","GD-D58(TYPE NC) Series","0～100%LEL/0～50000ppm"]
["Methane","CH4","74-82-8","CH4","HW","NC-6240A","Fixed","SD-1(TYPE NC) Series","0～100%LEL/0～50000ppm"]
["Methane","CH4","74-82-8","CH4","HW","NC-6240A","Fixed","SD-D58(TYPE NC) Series","0～100%LEL/0～50000ppm"]
["Methane","CH4","74-82-8","CH4","HW","NC-6245","Fixed","GD-A80 Series","0～100%LEL"]
["Methane","CH4","74-82-8","CH4","HW","NC-6245","Fixed","GD-D58(TYPE NC) Series","0～100%LEL"]
["Methane","CH4","74-82-8","CH4","HW","NC-6245","Fixed","SD-1(TYPE NC) Series","0～100%LEL"]
["Methane","CH4","74-82-8","CH4","HW","NC-6245","Fixed","SD-D58(TYPE NC) Series","0～100%LEL"]
["Methane","CH4","74-82-8","CH4","SG","SG-8511","Fixed","GD-A80V Series","0～1000ppm/0～2000ppm/0～2500ppm/0～3000ppm/0～3500ppm/0～5000ppm/0～10000ppm/0～12500ppm/0～15000ppm/0～20000ppm/0～30000ppm/0～50000ppm/0～50%LEL/0～100%LEL"]
["Methane","CH4","74-82-8","CH4","SG","SG-8511","Fixed","GD-D58・GH Series","0～1000ppm/0～2000ppm/0～2500ppm/0～3000ppm/0～3500ppm/0～5000ppm/0～10000ppm/0～12500ppm/0～15000ppm/0～20000ppm/0～30000ppm/0～50000ppm/0～50%LEL/0～100%LEL"]
["Methane","CH4","74-82-8","CH4","SG","SG-8511","Fixed","SD-1GH Series","0～1000ppm/0～2000ppm/0～2500ppm/0～3000ppm/0～3500ppm/0～5000ppm/0～10000ppm/0～12500ppm/0～15000ppm/0～20000ppm/0～30000ppm/0～50000ppm/0～50%LEL/0～100%LEL"]
["Methane","CH4","74-82-8","CH4","SG","SG-8511","Fixed","SD-D58・GH Series","0～1000ppm/0～2000ppm/0～2500ppm/0～3000ppm/0～3500ppm/0～5000ppm/0～10000ppm/0～12500ppm/0～15000ppm/0～20000ppm/0～30000ppm/0～50000ppm/0～50%LEL/0～100%LEL"]
["Methane","CH4","74-82-8","CH4","SG","SG-8581","Fixed","GD-A80V Series","0～500ppm/0～1000ppm/0～2000ppm"]
["Methane","CH4","74-82-8","CH4","SG","SG-8581","Fixed","GD-D58・GH Series","0～500ppm/0～1000ppm/0～2000ppm"]
["Methane","CH4","74-82-8","CH4","SG","SG-8581","Fixed","SD-1GH Series","0～500ppm/0～1000ppm/0～2000ppm"]
["Methane","CH4","74-82-8","CH4","SG","SG-8581","Fixed","SD-D58・GH Series","0～500ppm/0～1000ppm/0～2000ppm"]
["Methane","CH4","74-82-8","CH4","SG","SG-8585","Fixed","GD-A80V Series","0～500ppm/0～1000ppm/0～2000ppm"]
["Methane","CH4","74-82-8","CH4","SG","SG-8585","Fixed","GD-D58・GH Series","0～500ppm/0～1000ppm/0～2000ppm"]
["Methane","CH4","74-82-8","CH4","SG","SG-8585","Fixed","SD-1GH Series","0～500ppm/0～1000ppm/0～2000ppm"]
["Methane","CH4","74-82-8","CH4","SG","SG-8585","Fixed","SD-D58・GH Series","0～500ppm/0～1000ppm/0～2000ppm"]
["Methanol","CH3OH","67-56-1","CH4O","HW","NC-6215","Portable","GX-8000(TYPE LEL)","0～100%LEL"]
["Methanol","CH3OH","67-56-1","CH4O","HW","NC-6215","Portable","GP-1000(HC/CH4)","0～100%LEL"]
["Methanol","CH3OH","67-56-1","CH4O","HW","NC-6307","Portable","NC-1000(HC/CH4)","0～10000ppm"]
["Methanol","CH3OH","67-56-1","CH4O","SH","SH-8662","Portable","SP-220(TYPE SC)","0～10ppm"]
["Methanol","CH3OH","67-56-1","CH4O","SG","SGU-8521","Fixed","GD-70D Series","0～1000ppm"]
["Methanol","CH3OH","67-56-1","CH4O","SG","SGU-8521","Fixed","TP-70D","0～1000ppm"]
["Methanol","CH3OH","67-56-1","CH4O","SG","SGU-8521","Fixed","GD-70D Series","0～2000ppm"]
["Methanol","CH3OH","67-56-1","CH4O","SG","SGU-8521","Fixed","TP-70D","0～2000ppm"]
["Methanol","CH3OH","67-56-1","CH4O","HW","NCU-6211","Fixed","GD-70D Series","0～100%LEL","Confirm that GD-70D is non-explosion proof"]
["Methanol","CH3OH","67-56-1","CH4O","HW","NCU-6211","Fixed","TP-70D","0～100%LEL","Confirm that GD-70D is non-explosion proof"]
["Methanol","CH3OH","67-56-1","CH4O","HW","NCU-6211","Fixed","GD-70D Series","0～5000ppm"]
["Methanol","CH3OH","67-56-1","CH4O","HW","NCU-6211","Fixed","TP-70D","0～5000ppm"]
["Methanol","CH3OH","67-56-1","CH4O","RI","DE-3315-2","Fixed","SD-1RI Series","0～100%LEL"]
["Methanol","CH3OH","67-56-1","CH4O","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Methanol","CH3OH","67-56-1","CH4O","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Methanol","CH3OH","67-56-1","CH4O","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～55000ppm"]
["Methanol","CH3OH","67-56-1","CH4O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～55000ppm"]
["Methanol","CH3OH","67-56-1","CH4O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～55000ppm"]
["Methanol","CH3OH","67-56-1","CH4O","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～55000ppm"]
["Methanol","CH3OH","67-56-1","CH4O","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～55000ppm"]
["Methanol","CH3OH","67-56-1","CH4O","HW","HW-6213/NC-6213","Fixed","GD-A80 Series","0～100%LEL/0～55000ppm"]
["Methanol","CH3OH","67-56-1","CH4O","HW","HW-6213/NC-6213","Fixed","GD-D58(TYPE GP) Series","0～100%LEL/0～55000ppm"]
["Methanol","CH3OH","67-56-1","CH4O","HW","HW-6213/NC-6213","Fixed","GD-D58(TYPE NC) Series","0～100%LEL/0～55000ppm"]
["Methanol","CH3OH","67-56-1","CH4O","HW","NC-6240A","Fixed","GD-A80 Series","0～100%LEL/0～55000ppm"]
["Methanol","CH3OH","67-56-1","CH4O","HW","NC-6240A","Fixed","GD-D58(TYPE NC) Series","0～100%LEL/0～55000ppm"]
["Methanol","CH3OH","67-56-1","CH4O","HW","NC-6240A","Fixed","SD-1(TYPE NC) Series","0～100%LEL/0～55000ppm"]
["Methanol","CH3OH","67-56-1","CH4O","HW","NC-6240A","Fixed","SD-D58(TYPE NC) Series","0～100%LEL/0～55000ppm"]
["Methanol","CH3OH","67-56-1","CH4O","HW","NC-6245","Fixed","GD-A80 Series","0～100%LEL"]
["Methanol","CH3OH","67-56-1","CH4O","HW","NC-6245","Fixed","GD-D58(TYPE NC) Series","0～100%LEL"]
["Methanol","CH3OH","67-56-1","CH4O","HW","NC-6245","Fixed","SD-1(TYPE NC) Series","0～100%LEL"]
["Methanol","CH3OH","67-56-1","CH4O","HW","NC-6245","Fixed","SD-D58(TYPE NC) Series","0～100%LEL"]
["Methanol","CH3OH","67-56-1","CH4O","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Methanol","CH3OH","67-56-1","CH4O","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Methanol","CH3OH","67-56-1","CH4O","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Methanol","CH3OH","67-56-1","CH4O","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Methanol","CH3OH","67-56-1","CH4O","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Methanol","CH3OH","67-56-1","CH4O","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Methanol","CH3OH","67-56-1","CH4O","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Methanol","CH3OH","67-56-1","CH4O","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["Methanol","CH3OH","67-56-1","CH4O","SG","SG-8511","Fixed","GD-A80V Series","0～3000ppm/0～5000ppm"]
["Methanol","CH3OH","67-56-1","CH4O","SG","SG-8511","Fixed","GD-D58・GH Series","0～3000ppm/0～5000ppm"]
["Methanol","CH3OH","67-56-1","CH4O","SG","SG-8511","Fixed","SD-1GH Series","0～3000ppm/0～5000ppm"]
["Methanol","CH3OH","67-56-1","CH4O","SG","SG-8511","Fixed","SD-D58・GH Series","0～3000ppm/0～5000ppm"]
["Methanol","CH3OH","67-56-1","CH4O","SG","SG-8521","Fixed","GD-A80V Series","0～30ppm/0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～600ppm/0～800ppm/0～1000ppm/0～2000ppm"]
["Methanol","CH3OH","67-56-1","CH4O","SG","SG-8521","Fixed","GD-D58・GH Series","0～30ppm/0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～600ppm/0～800ppm/0～1000ppm/0～2000ppm"]
["Methanol","CH3OH","67-56-1","CH4O","SG","SG-8521","Fixed","SD-1GH Series","0～30ppm/0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～600ppm/0～800ppm/0～1000ppm/0～2000ppm"]
["Methanol","CH3OH","67-56-1","CH4O","SG","SG-8521","Fixed","SD-D58・GH Series","0～30ppm/0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～600ppm/0～800ppm/0～1000ppm/0～2000ppm"]
["Methanol","CH3OH","67-56-1","CH4O","SG","SG-8565","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Methanol","CH3OH","67-56-1","CH4O","SG","SG-8565","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Methanol","CH3OH","67-56-1","CH4O","SG","SG-8565","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Methanol","CH3OH","67-56-1","CH4O","SG","SG-8565","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Methyl acetate","MeOAc","79-20-9","C3H6O2","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Methyl acetate","MeOAc","79-20-9","C3H6O2","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Methyl acetate","MeOAc","79-20-9","C3H6O2","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～31000ppm"]
["Methyl acetate","MeOAc","79-20-9","C3H6O2","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～31000ppm"]
["Methyl acetate","MeOAc","79-20-9","C3H6O2","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～31000ppm"]
["Methyl acetate","MeOAc","79-20-9","C3H6O2","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～31000ppm"]
["Methyl acetate","MeOAc","79-20-9","C3H6O2","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～31000ppm"]
["Methyl acetate","MeOAc","79-20-9","C3H6O2","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Methyl acetate","MeOAc","79-20-9","C3H6O2","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Methyl acetate","MeOAc","79-20-9","C3H6O2","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Methyl acetate","MeOAc","79-20-9","C3H6O2","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Methyl acetate","MeOAc","79-20-9","C3H6O2","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Methyl acetate","MeOAc","79-20-9","C3H6O2","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Methyl acetate","MeOAc","79-20-9","C3H6O2","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Methyl acetate","MeOAc","79-20-9","C3H6O2","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["Methyl acetate","MeOAc","79-20-9","C3H6O2","SG","SG-8511","Fixed","GD-A80V Series","0～3000ppm/0～5000ppm"]
["Methyl acetate","MeOAc","79-20-9","C3H6O2","SG","SG-8511","Fixed","GD-D58・GH Series","0～3000ppm/0～5000ppm"]
["Methyl acetate","MeOAc","79-20-9","C3H6O2","SG","SG-8511","Fixed","SD-1GH Series","0～3000ppm/0～5000ppm"]
["Methyl acetate","MeOAc","79-20-9","C3H6O2","SG","SG-8511","Fixed","SD-D58・GH Series","0～3000ppm/0～5000ppm"]
["Methyl acetate","MeOAc","79-20-9","C3H6O2","SG","SG-8521","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Methyl acetate","MeOAc","79-20-9","C3H6O2","SG","SG-8521","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Methyl acetate","MeOAc","79-20-9","C3H6O2","SG","SG-8521","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Methyl acetate","MeOAc","79-20-9","C3H6O2","SG","SG-8521","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Methyl acrylate","C4H6O2","96-33-3","C4H6O2","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Methyl acrylate","C4H6O2","96-33-3","C4H6O2","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Methyl acrylate","C4H6O2","96-33-3","C4H6O2","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～24000ppm"]
["Methyl acrylate","C4H6O2","96-33-3","C4H6O2","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～24000ppm"]
["Methyl acrylate","C4H6O2","96-33-3","C4H6O2","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～24000ppm"]
["Methyl acrylate","C4H6O2","96-33-3","C4H6O2","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～24000ppm"]
["Methyl acrylate","C4H6O2","96-33-3","C4H6O2","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～24000ppm"]
["Methyl acrylate","C4H6O2","96-33-3","C4H6O2","SG","SG-8521","Fixed","GD-A80V Series","0～50ppm/0～100ppm/0～150ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Methyl acrylate","C4H6O2","96-33-3","C4H6O2","SG","SG-8521","Fixed","GD-D58・GH Series","0～50ppm/0～100ppm/0～150ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Methyl acrylate","C4H6O2","96-33-3","C4H6O2","SG","SG-8521","Fixed","SD-1GH Series","0～50ppm/0～100ppm/0～150ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Methyl acrylate","C4H6O2","96-33-3","C4H6O2","SG","SG-8521","Fixed","SD-D58・GH Series","0～50ppm/0～100ppm/0～150ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Methyl bromide","CH3Br","74-83-9","CH3Br","SH","SH-8662","Portable","SP-220(TYPE FUM)","0～100ppm"]
["Methyl bromide","CH3Br","74-83-9","CH3Br","SH","SH-8662","Portable","SP-220(TYPE SC)","0～20ppm"]
["Methyl bromide","CH3Br","74-83-9","CH3Br","SG","SG-8511","Fixed","GD-A80V Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Methyl bromide","CH3Br","74-83-9","CH3Br","SG","SG-8511","Fixed","GD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Methyl bromide","CH3Br","74-83-9","CH3Br","SG","SG-8511","Fixed","SD-1GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Methyl bromide","CH3Br","74-83-9","CH3Br","SG","SG-8511","Fixed","SD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Methyl chloride","CH3CL","74-87-3","CH3CL","SH","SH-8662","Portable","SP-220(TYPE SC)","0～10ppm"]
["Methyl chloride","CH3CL","74-87-3","CH3CL","RI","DE-3315-2","Fixed","SD-1RI Series","0～100%LEL"]
["Methyl chloride","CH3CL","74-87-3","CH3CL","SG","SG-8513","Fixed","GD-A80V Series","0～200ppm/0～300ppm/0～500ppm/0～600ppm/0～1000ppm/0～2000ppm/0～3000ppm"]
["Methyl chloride","CH3CL","74-87-3","CH3CL","SG","SG-8513","Fixed","GD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～600ppm/0～1000ppm/0～2000ppm/0～3000ppm"]
["Methyl chloride","CH3CL","74-87-3","CH3CL","SG","SG-8513","Fixed","SD-1GH Series","0～200ppm/0～300ppm/0～500ppm/0～600ppm/0～1000ppm/0～2000ppm/0～3000ppm"]
["Methyl chloride","CH3CL","74-87-3","CH3CL","SG","SG-8513","Fixed","SD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～600ppm/0～1000ppm/0～2000ppm/0～3000ppm"]
["Methyl Chloroformate","MCF","79-22-1","C2H3O2CL","SG","SG-8523","Fixed","GD-A80V Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Methyl Chloroformate","MCF","79-22-1","C2H3O2CL","SG","SG-8523","Fixed","GD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Methyl Chloroformate","MCF","79-22-1","C2H3O2CL","SG","SG-8523","Fixed","SD-1GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Methyl Chloroformate","MCF","79-22-1","C2H3O2CL","SG","SG-8523","Fixed","SD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Methyl ethyl ketone","MEK","78-93-3","C4H8O","HW","NC-6215","Portable","GX-8000(TYPE LEL)","0～100%LEL"]
["Methyl ethyl ketone","MEK","78-93-3","C4H8O","HW","NC-6215","Portable","GP-1000(HC/CH4)","0～100%LEL"]
["Methyl ethyl ketone","MEK","78-93-3","C4H8O","HW","NC-6307","Portable","NC-1000(HC/CH4)","0～10000ppm"]
["Methyl ethyl ketone","MEK","78-93-3","C4H8O","SH","SH-8662","Portable","SP-220(TYPE SC)","0～10ppm"]
["Methyl ethyl ketone","MEK","78-93-3","C4H8O","RI","DE-3315-2","Fixed","SD-1RI Series","0～10000ppm"]
["Methyl ethyl ketone","MEK","78-93-3","C4H8O","RI","DE-3315-2","Fixed","SD-1RI Series","0～100%LEL"]
["Methyl ethyl ketone","MEK","78-93-3","C4H8O","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Methyl ethyl ketone","MEK","78-93-3","C4H8O","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Methyl ethyl ketone","MEK","78-93-3","C4H8O","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～18000ppm"]
["Methyl ethyl ketone","MEK","78-93-3","C4H8O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～18000ppm"]
["Methyl ethyl ketone","MEK","78-93-3","C4H8O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～18000ppm"]
["Methyl ethyl ketone","MEK","78-93-3","C4H8O","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～18000ppm"]
["Methyl ethyl ketone","MEK","78-93-3","C4H8O","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～18000ppm"]
["Methyl ethyl ketone","MEK","78-93-3","C4H8O","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Methyl ethyl ketone","MEK","78-93-3","C4H8O","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Methyl ethyl ketone","MEK","78-93-3","C4H8O","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Methyl ethyl ketone","MEK","78-93-3","C4H8O","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Methyl ethyl ketone","MEK","78-93-3","C4H8O","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Methyl ethyl ketone","MEK","78-93-3","C4H8O","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Methyl ethyl ketone","MEK","78-93-3","C4H8O","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Methyl ethyl ketone","MEK","78-93-3","C4H8O","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["Methyl ethyl ketone","MEK","78-93-3","C4H8O","SG","SG-8511","Fixed","GD-A80V Series","0～3000ppm/0～5000ppm"]
["Methyl ethyl ketone","MEK","78-93-3","C4H8O","SG","SG-8511","Fixed","GD-D58・GH Series","0～3000ppm/0～5000ppm"]
["Methyl ethyl ketone","MEK","78-93-3","C4H8O","SG","SG-8511","Fixed","SD-1GH Series","0～3000ppm/0～5000ppm"]
["Methyl ethyl ketone","MEK","78-93-3","C4H8O","SG","SG-8511","Fixed","SD-D58・GH Series","0～3000ppm/0～5000ppm"]
["Methyl ethyl ketone","MEK","78-93-3","C4H8O","SG","SG-8521","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Methyl ethyl ketone","MEK","78-93-3","C4H8O","SG","SG-8521","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Methyl ethyl ketone","MEK","78-93-3","C4H8O","SG","SG-8521","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Methyl ethyl ketone","MEK","78-93-3","C4H8O","SG","SG-8521","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Methyl formate","HCOOCH3","107-31-3","C2H4O2","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Methyl formate","HCOOCH3","107-31-3","C2H4O2","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Methyl formate","HCOOCH3","107-31-3","C2H4O2","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～45000ppm"]
["Methyl formate","HCOOCH3","107-31-3","C2H4O2","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～45000ppm"]
["Methyl formate","HCOOCH3","107-31-3","C2H4O2","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～45000ppm"]
["Methyl formate","HCOOCH3","107-31-3","C2H4O2","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～45000ppm"]
["Methyl formate","HCOOCH3","107-31-3","C2H4O2","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～45000ppm"]
["Methyl formate","HCOOCH3","107-31-3","C2H4O2","SG","SG-8521","Fixed","GD-A80V Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Methyl formate","HCOOCH3","107-31-3","C2H4O2","SG","SG-8521","Fixed","GD-D58・GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Methyl formate","HCOOCH3","107-31-3","C2H4O2","SG","SG-8521","Fixed","SD-1GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Methyl formate","HCOOCH3","107-31-3","C2H4O2","SG","SG-8521","Fixed","SD-D58・GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Methyl iodide","CH3I","74-88-4","CH3I","SH","SH-8662","Portable","SP-220(TYPE FUM)","0～30ppm"]
["Methyl iodide","CH3I","74-88-4","CH3I","SG","SG-8511","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Methyl iodide","CH3I","74-88-4","CH3I","SG","SG-8511","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Methyl iodide","CH3I","74-88-4","CH3I","SG","SG-8511","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Methyl iodide","CH3I","74-88-4","CH3I","SG","SG-8511","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Methyl isobutyl ketone","MIBK","108-10-1","C6H12O","HW","NC-6215","Portable","GP-1000(HC/CH4)","0～100%LEL"]
["Methyl isobutyl ketone","MIBK","108-10-1","C6H12O","HW","NC-6307","Portable","NC-1000(HC/CH4)","0～10000ppm"]
["Methyl isobutyl ketone","MIBK","108-10-1","C6H12O","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Methyl isobutyl ketone","MIBK","108-10-1","C6H12O","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Methyl isobutyl ketone","MIBK","108-10-1","C6H12O","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～12000ppm"]
["Methyl isobutyl ketone","MIBK","108-10-1","C6H12O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～12000ppm"]
["Methyl isobutyl ketone","MIBK","108-10-1","C6H12O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～12000ppm"]
["Methyl isobutyl ketone","MIBK","108-10-1","C6H12O","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～12000ppm"]
["Methyl isobutyl ketone","MIBK","108-10-1","C6H12O","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～12000ppm"]
["Methyl isobutyl ketone","MIBK","108-10-1","C6H12O","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Methyl isobutyl ketone","MIBK","108-10-1","C6H12O","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Methyl isobutyl ketone","MIBK","108-10-1","C6H12O","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Methyl isobutyl ketone","MIBK","108-10-1","C6H12O","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Methyl isobutyl ketone","MIBK","108-10-1","C6H12O","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Methyl isobutyl ketone","MIBK","108-10-1","C6H12O","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Methyl isobutyl ketone","MIBK","108-10-1","C6H12O","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Methyl isobutyl ketone","MIBK","108-10-1","C6H12O","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["Methyl isobutyl ketone","MIBK","108-10-1","C6H12O","SG","SG-8521","Fixed","GD-A80V Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/◆0～1000ppm/◆0～2000ppm","◆Accuracy near the F.S. concentration range is likely to deteriorate"]
["Methyl isobutyl ketone","MIBK","108-10-1","C6H12O","SG","SG-8521","Fixed","GD-D58・GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/◆0～1000ppm/◆0～2000ppm","◆Accuracy near the F.S. concentration range is likely to deteriorate"]
["Methyl isobutyl ketone","MIBK","108-10-1","C6H12O","SG","SG-8521","Fixed","SD-1GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/◆0～1000ppm/◆0～2000ppm","◆Accuracy near the F.S. concentration range is likely to deteriorate"]
["Methyl isobutyl ketone","MIBK","108-10-1","C6H12O","SG","SG-8521","Fixed","SD-D58・GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/◆0～1000ppm/◆0～2000ppm","◆Accuracy near the F.S. concentration range is likely to deteriorate"]
["Methyl isobutyrate","MIB","547-63-7","C5H10O2","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Methyl isobutyrate","MIB","547-63-7","C5H10O2","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Methyl isobutyrate","MIB","547-63-7","C5H10O2","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～16000ppm"]
["Methyl isobutyrate","MIB","547-63-7","C5H10O2","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～16000ppm"]
["Methyl isobutyrate","MIB","547-63-7","C5H10O2","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～16000ppm"]
["Methyl isobutyrate","MIB","547-63-7","C5H10O2","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～16000ppm"]
["Methyl isobutyrate","MIB","547-63-7","C5H10O2","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～16000ppm"]
["Methyl isobutyrate","MIB","547-63-7","C5H10O2","SG","SG-8521","Fixed","GD-A80V Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Methyl isobutyrate","MIB","547-63-7","C5H10O2","SG","SG-8521","Fixed","GD-D58・GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Methyl isobutyrate","MIB","547-63-7","C5H10O2","SG","SG-8521","Fixed","SD-1GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Methyl isobutyrate","MIB","547-63-7","C5H10O2","SG","SG-8521","Fixed","SD-D58・GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Methyl Lactate","LAM","547-64-8","C4H8O3","SG","SG-8521","Fixed","GD-A80V Series","0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Methyl Lactate","LAM","547-64-8","C4H8O3","SG","SG-8521","Fixed","GD-D58・GH Series","0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Methyl Lactate","LAM","547-64-8","C4H8O3","SG","SG-8521","Fixed","SD-1GH Series","0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Methyl Lactate","LAM","547-64-8","C4H8O3","SG","SG-8521","Fixed","SD-D58・GH Series","0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Methyl methacrylate","MMA","80-62-6","C5H8O2","HW","NC-6215","Portable","GP-1000(HC/CH4)","0～100%LEL"]
["Methyl methacrylate","MMA","80-62-6","C5H8O2","HW","NC-6307","Portable","NC-1000(HC/CH4)","0～10000ppm"]
["Methyl methacrylate","MMA","80-62-6","C5H8O2","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Methyl methacrylate","MMA","80-62-6","C5H8O2","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Methyl methacrylate","MMA","80-62-6","C5H8O2","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～17000ppm"]
["Methyl methacrylate","MMA","80-62-6","C5H8O2","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～17000ppm"]
["Methyl methacrylate","MMA","80-62-6","C5H8O2","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～17000ppm"]
["Methyl methacrylate","MMA","80-62-6","C5H8O2","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～17000ppm"]
["Methyl methacrylate","MMA","80-62-6","C5H8O2","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～17000ppm"]
["Methyl methacrylate","MMA","80-62-6","C5H8O2","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Methyl methacrylate","MMA","80-62-6","C5H8O2","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Methyl methacrylate","MMA","80-62-6","C5H8O2","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Methyl methacrylate","MMA","80-62-6","C5H8O2","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Methyl methacrylate","MMA","80-62-6","C5H8O2","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Methyl methacrylate","MMA","80-62-6","C5H8O2","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Methyl methacrylate","MMA","80-62-6","C5H8O2","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Methyl methacrylate","MMA","80-62-6","C5H8O2","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["Methyl methacrylate","MMA","80-62-6","C5H8O2","SG","SG-8521","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm"]
["Methyl methacrylate","MMA","80-62-6","C5H8O2","SG","SG-8521","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm"]
["Methyl methacrylate","MMA","80-62-6","C5H8O2","SG","SG-8521","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm"]
["Methyl methacrylate","MMA","80-62-6","C5H8O2","SG","SG-8521","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm"]
["Methyl n-amyl ketone","C7H14O","110-43-0","C7H14O","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Methyl n-amyl ketone","C7H14O","110-43-0","C7H14O","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Methyl n-amyl ketone","C7H14O","110-43-0","C7H14O","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～11000ppm"]
["Methyl n-amyl ketone","C7H14O","110-43-0","C7H14O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～11000ppm"]
["Methyl n-amyl ketone","C7H14O","110-43-0","C7H14O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～11000ppm"]
["Methyl n-amyl ketone","C7H14O","110-43-0","C7H14O","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～11000ppm"]
["Methyl n-amyl ketone","C7H14O","110-43-0","C7H14O","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～11000ppm"]
["Methyl n-amyl ketone","C7H14O","110-43-0","C7H14O","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Methyl n-amyl ketone","C7H14O","110-43-0","C7H14O","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Methyl n-amyl ketone","C7H14O","110-43-0","C7H14O","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Methyl n-amyl ketone","C7H14O","110-43-0","C7H14O","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Methyl n-amyl ketone","C7H14O","110-43-0","C7H14O","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Methyl n-amyl ketone","C7H14O","110-43-0","C7H14O","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Methyl n-amyl ketone","C7H14O","110-43-0","C7H14O","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Methyl n-amyl ketone","C7H14O","110-43-0","C7H14O","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["Methyl n-amyl ketone","C7H14O","110-43-0","C7H14O","SG","SG-8521","Fixed","GD-A80V Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm"]
["Methyl n-amyl ketone","C7H14O","110-43-0","C7H14O","SG","SG-8521","Fixed","GD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm"]
["Methyl n-amyl ketone","C7H14O","110-43-0","C7H14O","SG","SG-8521","Fixed","SD-1GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm"]
["Methyl n-amyl ketone","C7H14O","110-43-0","C7H14O","SG","SG-8521","Fixed","SD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm"]
["Methyl Propionate","PacidMt","554-12-1","C4H8O2","SG","SG-8562","Fixed","GD-A80V Series","0～20ppm/0～30ppm/0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Methyl Propionate","PacidMt","554-12-1","C4H8O2","SG","SG-8562","Fixed","GD-D58・GH Series","0～20ppm/0～30ppm/0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Methyl Propionate","PacidMt","554-12-1","C4H8O2","SG","SG-8562","Fixed","SD-1GH Series","0～20ppm/0～30ppm/0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Methyl Propionate","PacidMt","554-12-1","C4H8O2","SG","SG-8562","Fixed","SD-D58・GH Series","0～20ppm/0～30ppm/0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Methyl silicate","QMS","681-84-5","C4H12O4Si","SS","SSU-1925","Fixed","GD-70D+PLU Series","0‐15ppm","PLU-70 required"]
["Methyl silicate","QMS","681-84-5","C4H12O4Si","SS","SSU-1925","Fixed","GD-70DG","0‐15ppm","PLU-70 required"]
["Methyl Sulfide","C2H6S","75-18-3","C2H6S","SG","SG-8564","Fixed","GD-A80V Series","0～50ppm"]
["Methyl Sulfide","C2H6S","75-18-3","C2H6S","SG","SG-8564","Fixed","GD-D58・GH Series","0～50ppm"]
["Methyl Sulfide","C2H6S","75-18-3","C2H6S","SG","SG-8564","Fixed","SD-1GH Series","0～50ppm"]
["Methyl Sulfide","C2H6S","75-18-3","C2H6S","SG","SG-8564","Fixed","SD-D58・GH Series","0～50ppm"]
["Methyl tert-butyl ether","C5H12O","1634-04-4","C5H12O","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Methyl tert-butyl ether","C5H12O","1634-04-4","C5H12O","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Methyl tert-butyl ether","C5H12O","1634-04-4","C5H12O","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～16000ppm"]
["Methyl tert-butyl ether","C5H12O","1634-04-4","C5H12O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～16000ppm"]
["Methyl tert-butyl ether","C5H12O","1634-04-4","C5H12O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～16000ppm"]
["Methyl tert-butyl ether","C5H12O","1634-04-4","C5H12O","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～16000ppm"]
["Methyl tert-butyl ether","C5H12O","1634-04-4","C5H12O","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～16000ppm"]
["Methylacrylonitrile","C4H5N","126-98-7","C4H5N","SG","SG-8521","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Methylacrylonitrile","C4H5N","126-98-7","C4H5N","SG","SG-8521","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Methylacrylonitrile","C4H5N","126-98-7","C4H5N","SG","SG-8521","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Methylacrylonitrile","C4H5N","126-98-7","C4H5N","SG","SG-8521","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Methylal","DM-METN","109-87-5","C3H8O2","SG","SG-8521","Fixed","GD-A80V Series","0～30ppm/0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm"]
["Methylal","DM-METN","109-87-5","C3H8O2","SG","SG-8521","Fixed","GD-D58・GH Series","0～30ppm/0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm"]
["Methylal","DM-METN","109-87-5","C3H8O2","SG","SG-8521","Fixed","SD-1GH Series","0～30ppm/0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm"]
["Methylal","DM-METN","109-87-5","C3H8O2","SG","SG-8521","Fixed","SD-D58・GH Series","0～30ppm/0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm"]
["Methylamine","MMtA","74-89-5","CH5N","ES","ESU-23RV","Fixed","GD-70D Series","0～15ppm"]
["Methylamine","MMtA","74-89-5","CH5N","ES","ESU-23RV","Fixed","TP-70D","0～15ppm"]
["Methylamine","MMtA","74-89-5","CH5N","ES","ESU-23RVM","Fixed","GD-70D Series","0～15ppm","Updated against electrolyte reduction"]
["Methylamine","MMtA","74-89-5","CH5N","ES","ESU-23RVM","Fixed","TP-70D","0～15ppm","Updated against electrolyte reduction"]
["Methylamine","MMtA","74-89-5","CH5N","ES","ESM-23RV","Fixed","GD-K88Ai Series","0～15ppm"]
["Methylamine","MMtA","74-89-5","CH5N","ES","ESM-23RV","Fixed","GD-K88Di Series","0～15ppm"]
["Methylamine","MMtA","74-89-5","CH5N","ES","ESM-23RVM","Fixed","GD-K88Ai Series","0～15ppm","Updated against electrolyte reduction"]
["Methylamine","MMtA","74-89-5","CH5N","ES","ESM-23RVM","Fixed","GD-K88Di Series","0～15ppm","Updated against electrolyte reduction"]
["Methylamine","MMtA","74-89-5","CH5N","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Methylamine","MMtA","74-89-5","CH5N","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Methylamine","MMtA","74-89-5","CH5N","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～49000ppm"]
["Methylamine","MMtA","74-89-5","CH5N","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～49000ppm"]
["Methylamine","MMtA","74-89-5","CH5N","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～49000ppm"]
["Methylamine","MMtA","74-89-5","CH5N","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～49000ppm"]
["Methylamine","MMtA","74-89-5","CH5N","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～49000ppm"]
["Methylcyclohexane","C7H14","108-87-2","C7H14","HW","NC-6215","Portable","GP-1000(Specified cal.gas)","0～100%LEL"]
["Methylcyclohexane","C7H14","108-87-2","C7H14","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Methylcyclohexane","C7H14","108-87-2","C7H14","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Methylcyclohexane","C7H14","108-87-2","C7H14","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～11500ppm"]
["Methylcyclohexane","C7H14","108-87-2","C7H14","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～11500ppm"]
["Methylcyclohexane","C7H14","108-87-2","C7H14","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～11500ppm"]
["Methylcyclohexane","C7H14","108-87-2","C7H14","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～11500ppm"]
["Methylcyclohexane","C7H14","108-87-2","C7H14","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～11500ppm"]
["Methylcyclohexane","C7H14","108-87-2","C7H14","SG","SG-8521","Fixed","GD-A80V Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Methylcyclohexane","C7H14","108-87-2","C7H14","SG","SG-8521","Fixed","GD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Methylcyclohexane","C7H14","108-87-2","C7H14","SG","SG-8521","Fixed","SD-1GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Methylcyclohexane","C7H14","108-87-2","C7H14","SG","SG-8521","Fixed","SD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Methylcyclohexane","C7H14","108-87-2","C7H14","SG","SG-8562","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Methylcyclohexane","C7H14","108-87-2","C7H14","SG","SG-8562","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Methylcyclohexane","C7H14","108-87-2","C7H14","SG","SG-8562","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Methylcyclohexane","C7H14","108-87-2","C7H14","SG","SG-8562","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Methylmercaptan","CH3SH","74-93-1","CH4S","SG","SG-8513","Fixed","GD-A80V Series","0～50ppm"]
["Methylmercaptan","CH3SH","74-93-1","CH4S","SG","SG-8513","Fixed","GD-D58・GH Series","0～50ppm"]
["Methylmercaptan","CH3SH","74-93-1","CH4S","SG","SG-8513","Fixed","SD-1GH Series","0～50ppm"]
["Methylmercaptan","CH3SH","74-93-1","CH4S","SG","SG-8513","Fixed","SD-D58・GH Series","0～50ppm"]
["Monofluoromethane","R-41","593-53-3","CH3F","SG","SGU-8511","Fixed","GD-70D Series","0～10000ppm"]
["Monofluoromethane","R-41","593-53-3","CH3F","SG","SGU-8511","Fixed","TP-70D","0～10000ppm"]
["Monofluoromethane","R-41","593-53-3","CH3F","SG","SGU-8521","Fixed","GD-70D Series","0～2000ppm"]
["Monofluoromethane","R-41","593-53-3","CH3F","SG","SGU-8521","Fixed","TP-70D","0～2000ppm"]
["Monofluoromethane","R-41","593-53-3","CH3F","RI","DE-2113-35","Fixed","RI-257","0～5vol%"]
["Monofluoromethane","R-41","593-53-3","CH3F","SG","SG-8511","Fixed","GD-A80V Series","0～3000ppm/0～5000ppm/0～10000ppm"]
["Monofluoromethane","R-41","593-53-3","CH3F","SG","SG-8511","Fixed","GD-D58・GH Series","0～3000ppm/0～5000ppm/0～10000ppm"]
["Monofluoromethane","R-41","593-53-3","CH3F","SG","SG-8511","Fixed","SD-1GH Series","0～3000ppm/0～5000ppm/0～10000ppm"]
["Monofluoromethane","R-41","593-53-3","CH3F","SG","SG-8511","Fixed","SD-D58・GH Series","0～3000ppm/0～5000ppm/0～10000ppm"]
["Monofluoromethane","R-41","593-53-3","CH3F","SG","SG-8521","Fixed","GD-A80V Series","0～500ppm/0～1000ppm/0～2000ppm"]
["Monofluoromethane","R-41","593-53-3","CH3F","SG","SG-8521","Fixed","GD-D58・GH Series","0～500ppm/0～1000ppm/0～2000ppm"]
["Monofluoromethane","R-41","593-53-3","CH3F","SG","SG-8521","Fixed","SD-1GH Series","0～500ppm/0～1000ppm/0～2000ppm"]
["Monofluoromethane","R-41","593-53-3","CH3F","SG","SG-8521","Fixed","SD-D58・GH Series","0～500ppm/0～1000ppm/0～2000ppm"]
["Monofluoromethane","R-41","593-53-3","CH3F","SG","SG-8582","Fixed","GD-A80V Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm","Standard sensor: SG-8511, SG-8521"]
["Monofluoromethane","R-41","593-53-3","CH3F","SG","SG-8582","Fixed","GD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm","Standard sensor: SG-8511, SG-8521"]
["Monofluoromethane","R-41","593-53-3","CH3F","SG","SG-8582","Fixed","SD-1GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm","Standard sensor: SG-8511, SG-8521"]
["Monofluoromethane","R-41","593-53-3","CH3F","SG","SG-8582","Fixed","SD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm","Standard sensor: SG-8511, SG-8521"]
["Monomethylsilane","CH3SiH3","992-94-9","CH6Si","ES","ESU-23DH","Fixed","GD-70D Series","0～20ppm"]
["Monomethylsilane","CH3SiH3","992-94-9","CH6Si","ES","ESU-23DH","Fixed","TP-70D","0～20ppm"]
["Monomethylsilane","CH3SiH3","992-94-9","CH6Si","ES","ESM-23DH","Fixed","GD-K88Ai Series","0～20ppm"]
["Monomethylsilane","CH3SiH3","992-94-9","CH6Si","ES","ESM-23DH","Fixed","GD-K88Di Series","0～20ppm"]
["Morpholine","C4H8HNO","110-91-8","C4H9NO","SG","SG-8562","Fixed","GD-A80V Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Morpholine","C4H8HNO","110-91-8","C4H9NO","SG","SG-8562","Fixed","GD-D58・GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Morpholine","C4H8HNO","110-91-8","C4H9NO","SG","SG-8562","Fixed","SD-1GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Morpholine","C4H8HNO","110-91-8","C4H9NO","SG","SG-8562","Fixed","SD-D58・GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["N-(Trimethylsilyl)dimethylamine","TMS-DMA","2083-91-2","C5H15NSi","RI","DE-2113-37","Fixed","RI-257","0～10000ppm"]
["N,N,N',N'-Tetramethylethylenediamine","TMEDA","110-18-9","C6H16N2","SG","SG-8521","Fixed","GD-A80V Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["N,N,N',N'-Tetramethylethylenediamine","TMEDA","110-18-9","C6H16N2","SG","SG-8521","Fixed","GD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["N,N,N',N'-Tetramethylethylenediamine","TMEDA","110-18-9","C6H16N2","SG","SG-8521","Fixed","SD-1GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["N,N,N',N'-Tetramethylethylenediamine","TMEDA","110-18-9","C6H16N2","SG","SG-8521","Fixed","SD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["N,N-Dimethylacetamide","DMAC","127-19-5","C4H9NO","HW","NCU-6211","Fixed","GD-70D Series","0～4000ppm"]
["N,N-Dimethylacetamide","DMAC","127-19-5","C4H9NO","HW","NCU-6211","Fixed","TP-70D","0～4000ppm"]
["N,N-Dimethylacetamide","DMAC","127-19-5","C4H9NO","HW","NC-6211","Fixed","GD-A80 Series","～25%LEL/～5000ppm"]
["N,N-Dimethylacetamide","DMAC","127-19-5","C4H9NO","HW","NC-6211","Fixed","GD-D58(TYPE GP) Series","～25%LEL/～5000ppm"]
["N,N-Dimethylacetamide","DMAC","127-19-5","C4H9NO","HW","NC-6211","Fixed","GD-D58(TYPE NC) Series","～25%LEL/～5000ppm"]
["N,N-Dimethylacetamide","DMAC","127-19-5","C4H9NO","HW","NC-6211","Fixed","SD-1(TYPE NC) Series","～25%LEL/～5000ppm"]
["N,N-Dimethylacetamide","DMAC","127-19-5","C4H9NO","HW","NC-6211","Fixed","SD-D58(TYPE NC) Series","～25%LEL/～5000ppm"]
["N,N-Dimethylacetamide","DMAC","127-19-5","C4H9NO","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["N,N-Dimethylacetamide","DMAC","127-19-5","C4H9NO","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["N,N-Dimethylacetamide","DMAC","127-19-5","C4H9NO","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["N,N-Dimethylacetamide","DMAC","127-19-5","C4H9NO","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["N,N-Dimethylacetamide","DMAC","127-19-5","C4H9NO","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["N,N-Dimethylacetamide","DMAC","127-19-5","C4H9NO","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["N,N-Dimethylacetamide","DMAC","127-19-5","C4H9NO","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["N,N-Dimethylacetamide","DMAC","127-19-5","C4H9NO","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["N,N-Dimethylacetamide","DMAC","127-19-5","C4H9NO","SG","SG-8521","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["N,N-Dimethylacetamide","DMAC","127-19-5","C4H9NO","SG","SG-8521","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["N,N-Dimethylacetamide","DMAC","127-19-5","C4H9NO","SG","SG-8521","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["N,N-Dimethylacetamide","DMAC","127-19-5","C4H9NO","SG","SG-8521","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["N,N'-Dimethylethylenediamine","C4H12N2","110-70-3","C4H12N2","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["N,N'-Dimethylethylenediamine","C4H12N2","110-70-3","C4H12N2","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["N,N'-Dimethylethylenediamine","C4H12N2","110-70-3","C4H12N2","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["N,N'-Dimethylethylenediamine","C4H12N2","110-70-3","C4H12N2","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["N,N'-Dimethylethylenediamine","C4H12N2","110-70-3","C4H12N2","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["N,N'-Dimethylethylenediamine","C4H12N2","110-70-3","C4H12N2","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["N,N'-Dimethylethylenediamine","C4H12N2","110-70-3","C4H12N2","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["N,N'-Dimethylethylenediamine","C4H12N2","110-70-3","C4H12N2","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["Naphtha","NAPHTHA","8030-30-6","-","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Naphtha","NAPHTHA","8030-30-6","-","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Naphtha","NAPHTHA","8030-30-6","-","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～9000ppm"]
["Naphtha","NAPHTHA","8030-30-6","-","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～9000ppm"]
["Naphtha","NAPHTHA","8030-30-6","-","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～9000ppm"]
["Naphtha","NAPHTHA","8030-30-6","-","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～9000ppm"]
["Naphtha","NAPHTHA","8030-30-6","-","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～9000ppm"]
["Naphtha","NAPHTHA","8030-30-6","-","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Naphtha","NAPHTHA","8030-30-6","-","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Naphtha","NAPHTHA","8030-30-6","-","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Naphtha","NAPHTHA","8030-30-6","-","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Naphtha","NAPHTHA","8030-30-6","-","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Naphtha","NAPHTHA","8030-30-6","-","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Naphtha","NAPHTHA","8030-30-6","-","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Naphtha","NAPHTHA","8030-30-6","-","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["n-Butane","n-C4H10","106-97-8","C4H10","SH","SH-8661","Portable","SP-220(TYPE H2)","0～10000ppm"]
["n-Butane","n-C4H10","106-97-8","C4H10","HW","NC-6215","Portable","GP-1000(Specified cal.gas)","0～100%LEL"]
["n-Butane","n-C4H10","106-97-8","C4H10","HW","NC-6307","Portable","NC-1000(Specified cal. Gas)","0～10000ppm"]
["n-Butane","n-C4H10","106-97-8","C4H10","RI","DE-3315-2","Fixed","SD-1RI Series","0～100%LEL"]
["n-Butane","n-C4H10","106-97-8","C4H10","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["n-Butane","n-C4H10","106-97-8","C4H10","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["n-Butane","n-C4H10","106-97-8","C4H10","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～15000ppm"]
["n-Butane","n-C4H10","106-97-8","C4H10","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～15000ppm"]
["n-Butane","n-C4H10","106-97-8","C4H10","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～15000ppm"]
["n-Butane","n-C4H10","106-97-8","C4H10","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～15000ppm"]
["n-Butane","n-C4H10","106-97-8","C4H10","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～15000ppm"]
["n-Butane","n-C4H10","106-97-8","C4H10","HW","HW-6213/NC-6213","Fixed","GD-A80 Series","0～100%LEL/0～15000ppm"]
["n-Butane","n-C4H10","106-97-8","C4H10","HW","HW-6213/NC-6213","Fixed","GD-D58(TYPE GP) Series","0～100%LEL/0～15000ppm"]
["n-Butane","n-C4H10","106-97-8","C4H10","HW","HW-6213/NC-6213","Fixed","GD-D58(TYPE NC) Series","0～100%LEL/0～15000ppm"]
["n-Butane","n-C4H10","106-97-8","C4H10","HW","HW-6239","Fixed","GD-A80-70 Series","0～100%LEL"]
["n-Butane","n-C4H10","106-97-8","C4H10","HW","HW-6239","Fixed","SD-1(TYPE GP) Series","0～100%LEL"]
["n-Butane","n-C4H10","106-97-8","C4H10","HW","HW-6239","Fixed","SD-D58(TYPE GP) Series","0～100%LEL"]
["n-Butane","n-C4H10","106-97-8","C4H10","HW","HW-6239/NC-6239","Fixed","GD-A80 Series","0～100%LEL/0～15000ppm"]
["n-Butane","n-C4H10","106-97-8","C4H10","HW","HW-6239/NC-6239","Fixed","GD-D58(TYPE GP) Series","0～100%LEL/0～15000ppm"]
["n-Butane","n-C4H10","106-97-8","C4H10","HW","HW-6239/NC-6239","Fixed","GD-D58(TYPE NC) Series","0～100%LEL/0～15000ppm"]
["n-Butane","n-C4H10","106-97-8","C4H10","HW","HW-6239/NC-6239","Fixed","SD-1(TYPE NC) Series","0～100%LEL/0～15000ppm"]
["n-Butane","n-C4H10","106-97-8","C4H10","HW","HW-6239/NC-6239","Fixed","SD-D58(TYPE NC) Series","0～100%LEL/0～15000ppm"]
["n-Butane","n-C4H10","106-97-8","C4H10","HW","NC-6240A","Fixed","GD-A80 Series","0～100%LEL/0～15000ppm"]
["n-Butane","n-C4H10","106-97-8","C4H10","HW","NC-6240A","Fixed","GD-D58(TYPE NC) Series","0～100%LEL/0～15000ppm"]
["n-Butane","n-C4H10","106-97-8","C4H10","HW","NC-6240A","Fixed","SD-1(TYPE NC) Series","0～100%LEL/0～15000ppm"]
["n-Butane","n-C4H10","106-97-8","C4H10","HW","NC-6240A","Fixed","SD-D58(TYPE NC) Series","0～100%LEL/0～15000ppm"]
["n-Butane","n-C4H10","106-97-8","C4H10","HW","NC-6245","Fixed","GD-A80 Series","0～100%LEL"]
["n-Butane","n-C4H10","106-97-8","C4H10","HW","NC-6245","Fixed","GD-D58(TYPE NC) Series","0～100%LEL"]
["n-Butane","n-C4H10","106-97-8","C4H10","HW","NC-6245","Fixed","SD-1(TYPE NC) Series","0～100%LEL"]
["n-Butane","n-C4H10","106-97-8","C4H10","HW","NC-6245","Fixed","SD-D58(TYPE NC) Series","0～100%LEL"]
["n-Butane","n-C4H10","106-97-8","C4H10","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["n-Butane","n-C4H10","106-97-8","C4H10","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["n-Butane","n-C4H10","106-97-8","C4H10","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["n-Butane","n-C4H10","106-97-8","C4H10","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["n-Butane","n-C4H10","106-97-8","C4H10","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["n-Butane","n-C4H10","106-97-8","C4H10","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["n-Butane","n-C4H10","106-97-8","C4H10","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["n-Butane","n-C4H10","106-97-8","C4H10","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["n-Butane","n-C4H10","106-97-8","C4H10","SG","SG-8511","Fixed","GD-A80V Series","0～3000ppm/0～5000ppm"]
["n-Butane","n-C4H10","106-97-8","C4H10","SG","SG-8511","Fixed","GD-D58・GH Series","0～3000ppm/0～5000ppm"]
["n-Butane","n-C4H10","106-97-8","C4H10","SG","SG-8511","Fixed","SD-1GH Series","0～3000ppm/0～5000ppm"]
["n-Butane","n-C4H10","106-97-8","C4H10","SG","SG-8511","Fixed","SD-D58・GH Series","0～3000ppm/0～5000ppm"]
["n-Butane","n-C4H10","106-97-8","C4H10","SG","SG-8521","Fixed","GD-A80V Series","0～500ppm/0～1000ppm/0～2000ppm"]
["n-Butane","n-C4H10","106-97-8","C4H10","SG","SG-8521","Fixed","GD-D58・GH Series","0～500ppm/0～1000ppm/0～2000ppm"]
["n-Butane","n-C4H10","106-97-8","C4H10","SG","SG-8521","Fixed","SD-1GH Series","0～500ppm/0～1000ppm/0～2000ppm"]
["n-Butane","n-C4H10","106-97-8","C4H10","SG","SG-8521","Fixed","SD-D58・GH Series","0～500ppm/0～1000ppm/0～2000ppm"]
["n-Butane","n-C4H10","106-97-8","C4H10","SG","SG-8582","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["n-Butane","n-C4H10","106-97-8","C4H10","SG","SG-8582","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["n-Butane","n-C4H10","106-97-8","C4H10","SG","SG-8582","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["n-Butane","n-C4H10","106-97-8","C4H10","SG","SG-8582","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["n-Butanol","n-BuOH","71-36-3","C4H10O","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["n-Butanol","n-BuOH","71-36-3","C4H10O","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["n-Butanol","n-BuOH","71-36-3","C4H10O","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～14000ppm"]
["n-Butanol","n-BuOH","71-36-3","C4H10O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～14000ppm"]
["n-Butanol","n-BuOH","71-36-3","C4H10O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～14000ppm"]
["n-Butanol","n-BuOH","71-36-3","C4H10O","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～14000ppm"]
["n-Butanol","n-BuOH","71-36-3","C4H10O","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～14000ppm"]
["n-Butanol","n-BuOH","71-36-3","C4H10O","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["n-Butanol","n-BuOH","71-36-3","C4H10O","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["n-Butanol","n-BuOH","71-36-3","C4H10O","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["n-Butanol","n-BuOH","71-36-3","C4H10O","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["n-Butanol","n-BuOH","71-36-3","C4H10O","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["n-Butanol","n-BuOH","71-36-3","C4H10O","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["n-Butanol","n-BuOH","71-36-3","C4H10O","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["n-Butanol","n-BuOH","71-36-3","C4H10O","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["n-Butanol","n-BuOH","71-36-3","C4H10O","SG","SG-8511","Fixed","GD-A80V Series","0～2000ppm/0～3000ppm/0～5000ppm"]
["n-Butanol","n-BuOH","71-36-3","C4H10O","SG","SG-8511","Fixed","GD-D58・GH Series","0～2000ppm/0～3000ppm/0～5000ppm"]
["n-Butanol","n-BuOH","71-36-3","C4H10O","SG","SG-8511","Fixed","SD-1GH Series","0～2000ppm/0～3000ppm/0～5000ppm"]
["n-Butanol","n-BuOH","71-36-3","C4H10O","SG","SG-8511","Fixed","SD-D58・GH Series","0～2000ppm/0～3000ppm/0～5000ppm"]
["n-Butanol","n-BuOH","71-36-3","C4H10O","SG","SG-8521","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["n-Butanol","n-BuOH","71-36-3","C4H10O","SG","SG-8521","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["n-Butanol","n-BuOH","71-36-3","C4H10O","SG","SG-8521","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["n-Butanol","n-BuOH","71-36-3","C4H10O","SG","SG-8521","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["n-Butyl acetate","C6H12O2","123-86-4","C6H12O2","HW","NC-6307","Portable","NC-1000(Specified cal. Gas)","0～10000ppm"]
["n-Butyl acetate","C6H12O2","123-86-4","C6H12O2","RI","DE-3315-2","Fixed","SD-1RI Series","0～100%LEL"]
["n-Butyl acetate","C6H12O2","123-86-4","C6H12O2","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["n-Butyl acetate","C6H12O2","123-86-4","C6H12O2","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["n-Butyl acetate","C6H12O2","123-86-4","C6H12O2","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～14000ppm"]
["n-Butyl acetate","C6H12O2","123-86-4","C6H12O2","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～14000ppm"]
["n-Butyl acetate","C6H12O2","123-86-4","C6H12O2","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～14000ppm"]
["n-Butyl acetate","C6H12O2","123-86-4","C6H12O2","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～14000ppm"]
["n-Butyl acetate","C6H12O2","123-86-4","C6H12O2","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～14000ppm"]
["n-Butyl acetate","C6H12O2","123-86-4","C6H12O2","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["n-Butyl acetate","C6H12O2","123-86-4","C6H12O2","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["n-Butyl acetate","C6H12O2","123-86-4","C6H12O2","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["n-Butyl acetate","C6H12O2","123-86-4","C6H12O2","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["n-Butyl acetate","C6H12O2","123-86-4","C6H12O2","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["n-Butyl acetate","C6H12O2","123-86-4","C6H12O2","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["n-Butyl acetate","C6H12O2","123-86-4","C6H12O2","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["n-Butyl acetate","C6H12O2","123-86-4","C6H12O2","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["n-Butyl acetate","C6H12O2","123-86-4","C6H12O2","SG","SG-8511","Fixed","GD-A80V Series","0～3000ppm/0～5000ppm"]
["n-Butyl acetate","C6H12O2","123-86-4","C6H12O2","SG","SG-8511","Fixed","GD-D58・GH Series","0～3000ppm/0～5000ppm"]
["n-Butyl acetate","C6H12O2","123-86-4","C6H12O2","SG","SG-8511","Fixed","SD-1GH Series","0～3000ppm/0～5000ppm"]
["n-Butyl acetate","C6H12O2","123-86-4","C6H12O2","SG","SG-8511","Fixed","SD-D58・GH Series","0～3000ppm/0～5000ppm"]
["n-Butyl acetate","C6H12O2","123-86-4","C6H12O2","SG","SG-8521","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["n-Butyl acetate","C6H12O2","123-86-4","C6H12O2","SG","SG-8521","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["n-Butyl acetate","C6H12O2","123-86-4","C6H12O2","SG","SG-8521","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["n-Butyl acetate","C6H12O2","123-86-4","C6H12O2","SG","SG-8521","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["n-Butyl acrylate","C7H12O2","141-32-2","C7H12O2","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["n-Butyl acrylate","C7H12O2","141-32-2","C7H12O2","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["n-Butyl acrylate","C7H12O2","141-32-2","C7H12O2","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～15000ppm"]
["n-Butyl acrylate","C7H12O2","141-32-2","C7H12O2","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～15000ppm"]
["n-Butyl acrylate","C7H12O2","141-32-2","C7H12O2","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～15000ppm"]
["n-Butyl acrylate","C7H12O2","141-32-2","C7H12O2","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～15000ppm"]
["n-Butyl acrylate","C7H12O2","141-32-2","C7H12O2","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～15000ppm"]
["n-Butyl acrylate","C7H12O2","141-32-2","C7H12O2","SG","SG-8521","Fixed","GD-A80V Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["n-Butyl acrylate","C7H12O2","141-32-2","C7H12O2","SG","SG-8521","Fixed","GD-D58・GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["n-Butyl acrylate","C7H12O2","141-32-2","C7H12O2","SG","SG-8521","Fixed","SD-1GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["n-Butyl acrylate","C7H12O2","141-32-2","C7H12O2","SG","SG-8521","Fixed","SD-D58・GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["n-Butylamine","C4H9NH2","109-73-9","C4H11N","SG","SG-8521","Fixed","GD-A80V Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["n-Butylamine","C4H9NH2","109-73-9","C4H11N","SG","SG-8521","Fixed","GD-D58・GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["n-Butylamine","C4H9NH2","109-73-9","C4H11N","SG","SG-8521","Fixed","SD-1GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["n-Butylamine","C4H9NH2","109-73-9","C4H11N","SG","SG-8521","Fixed","SD-D58・GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["n-Butyraldehyde","C4H8O","123-72-8","C4H8O","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["n-Butyraldehyde","C4H8O","123-72-8","C4H8O","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["n-Butyraldehyde","C4H8O","123-72-8","C4H8O","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～25000ppm"]
["n-Butyraldehyde","C4H8O","123-72-8","C4H8O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～25000ppm"]
["n-Butyraldehyde","C4H8O","123-72-8","C4H8O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～25000ppm"]
["n-Butyraldehyde","C4H8O","123-72-8","C4H8O","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～25000ppm"]
["n-Butyraldehyde","C4H8O","123-72-8","C4H8O","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～25000ppm"]
["n-Butyraldehyde","C4H8O","123-72-8","C4H8O","SG","SG-8511","Fixed","GD-A80V Series","0～2000ppm/0～3000ppm/0～5000ppm"]
["n-Butyraldehyde","C4H8O","123-72-8","C4H8O","SG","SG-8511","Fixed","GD-D58・GH Series","0～2000ppm/0～3000ppm/0～5000ppm"]
["n-Butyraldehyde","C4H8O","123-72-8","C4H8O","SG","SG-8511","Fixed","SD-1GH Series","0～2000ppm/0～3000ppm/0～5000ppm"]
["n-Butyraldehyde","C4H8O","123-72-8","C4H8O","SG","SG-8511","Fixed","SD-D58・GH Series","0～2000ppm/0～3000ppm/0～5000ppm"]
["n-Butyraldehyde","C4H8O","123-72-8","C4H8O","SG","SG-8521","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["n-Butyraldehyde","C4H8O","123-72-8","C4H8O","SG","SG-8521","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["n-Butyraldehyde","C4H8O","123-72-8","C4H8O","SG","SG-8521","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["n-Butyraldehyde","C4H8O","123-72-8","C4H8O","SG","SG-8521","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["n-Decane","C10H22","124-18-5","C10H22","SG","SGU-8521","Fixed","GD-70D Series","0～2000ppm"]
["n-Decane","C10H22","124-18-5","C10H22","SG","SGU-8521","Fixed","TP-70D","0～2000ppm"]
["n-Decane","C10H22","124-18-5","C10H22","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～80%LEL/～5600ppm"]
["n-Decane","C10H22","124-18-5","C10H22","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～80%LEL/～5600ppm"]
["n-Decane","C10H22","124-18-5","C10H22","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～80%LEL/～5600ppm"]
["n-Decane","C10H22","124-18-5","C10H22","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～80%LEL/～5600ppm"]
["n-Decane","C10H22","124-18-5","C10H22","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～80%LEL/～5600ppm"]
["n-Decane","C10H22","124-18-5","C10H22","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["n-Decane","C10H22","124-18-5","C10H22","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["n-Decane","C10H22","124-18-5","C10H22","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["n-Decane","C10H22","124-18-5","C10H22","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["n-Decane","C10H22","124-18-5","C10H22","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["n-Decane","C10H22","124-18-5","C10H22","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["n-Decane","C10H22","124-18-5","C10H22","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["n-Decane","C10H22","124-18-5","C10H22","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["n-Decane","C10H22","124-18-5","C10H22","SG","SG-8521","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["n-Decane","C10H22","124-18-5","C10H22","SG","SG-8521","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["n-Decane","C10H22","124-18-5","C10H22","SG","SG-8521","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["n-Decane","C10H22","124-18-5","C10H22","SG","SG-8521","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["n-Heptane","n-C7H16","142-82-5","C7H16","HW","NC-6215","Portable","GP-1000(HC/CH4)","0～100%LEL"]
["n-Heptane","n-C7H16","142-82-5","C7H16","HW","NC-6307","Portable","NC-1000(HC/CH4)","0～10000ppm"]
["n-Heptane","n-C7H16","142-82-5","C7H16","RI","DE-3315-2","Fixed","SD-1RI Series","0～100%LEL"]
["n-Heptane","n-C7H16","142-82-5","C7H16","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["n-Heptane","n-C7H16","142-82-5","C7H16","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["n-Heptane","n-C7H16","142-82-5","C7H16","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～11000ppm"]
["n-Heptane","n-C7H16","142-82-5","C7H16","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～11000ppm"]
["n-Heptane","n-C7H16","142-82-5","C7H16","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～11000ppm"]
["n-Heptane","n-C7H16","142-82-5","C7H16","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～11000ppm"]
["n-Heptane","n-C7H16","142-82-5","C7H16","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～11000ppm"]
["n-Heptane","n-C7H16","142-82-5","C7H16","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["n-Heptane","n-C7H16","142-82-5","C7H16","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["n-Heptane","n-C7H16","142-82-5","C7H16","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["n-Heptane","n-C7H16","142-82-5","C7H16","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["n-Heptane","n-C7H16","142-82-5","C7H16","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["n-Heptane","n-C7H16","142-82-5","C7H16","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["n-Heptane","n-C7H16","142-82-5","C7H16","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["n-Heptane","n-C7H16","142-82-5","C7H16","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["n-Heptane","n-C7H16","142-82-5","C7H16","SG","SG-8521","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["n-Heptane","n-C7H16","142-82-5","C7H16","SG","SG-8521","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["n-Heptane","n-C7H16","142-82-5","C7H16","SG","SG-8521","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["n-Heptane","n-C7H16","142-82-5","C7H16","SG","SG-8521","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["n-Hexane","n-C6H14","110-54-3","C6H14","HW","NC-6215","Portable","GX-8000(TYPE LEL)","0～100%LEL"]
["n-Hexane","n-C6H14","110-54-3","C6H14","HW","NC-6215","Portable","GP-1000(HC/CH4)","0～100%LEL"]
["n-Hexane","n-C6H14","110-54-3","C6H14","HW","NC-6307","Portable","NC-1000(HC/CH4)","0～10000ppm"]
["n-Hexane","n-C6H14","110-54-3","C6H14","SH","SH-8662","Portable","SP-220(TYPE SC)","0～50ppm"]
["n-Hexane","n-C6H14","110-54-3","C6H14","SH","SH-8661","Portable","SP-220(TYPE H2)","0～10000ppm"]
["n-Hexane","n-C6H14","110-54-3","C6H14","SG","SGU-8521","Fixed","GD-70D Series","0～200ppm"]
["n-Hexane","n-C6H14","110-54-3","C6H14","SG","SGU-8521","Fixed","TP-70D","0～200ppm"]
["n-Hexane","n-C6H14","110-54-3","C6H14","SG","SGU-8521","Fixed","GD-70D Series","0～2000ppm"]
["n-Hexane","n-C6H14","110-54-3","C6H14","SG","SGU-8521","Fixed","TP-70D","0～2000ppm"]
["n-Hexane","n-C6H14","110-54-3","C6H14","HW","NCU-6211","Fixed","GD-70D Series","0～2000ppm"]
["n-Hexane","n-C6H14","110-54-3","C6H14","HW","NCU-6211","Fixed","TP-70D","0～2000ppm"]
["n-Hexane","n-C6H14","110-54-3","C6H14","RI","DE-3315-2","Fixed","SD-1RI Series","0～100%LEL"]
["n-Hexane","n-C6H14","110-54-3","C6H14","RI","DE-3315-2","Fixed","SD-1RI Series","0～5vol%"]
["n-Hexane","n-C6H14","110-54-3","C6H14","RI","DE-3315-2","Fixed","SD-1RI Series","0～10vol%"]
["n-Hexane","n-C6H14","110-54-3","C6H14","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["n-Hexane","n-C6H14","110-54-3","C6H14","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["n-Hexane","n-C6H14","110-54-3","C6H14","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～12000ppm"]
["n-Hexane","n-C6H14","110-54-3","C6H14","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～12000ppm"]
["n-Hexane","n-C6H14","110-54-3","C6H14","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～12000ppm"]
["n-Hexane","n-C6H14","110-54-3","C6H14","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～12000ppm"]
["n-Hexane","n-C6H14","110-54-3","C6H14","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～12000ppm"]
["n-Hexane","n-C6H14","110-54-3","C6H14","HW","NC-6240A","Fixed","GD-A80 Series","0～100%LEL/0～12000ppm"]
["n-Hexane","n-C6H14","110-54-3","C6H14","HW","NC-6240A","Fixed","GD-D58(TYPE NC) Series","0～100%LEL/0～12000ppm"]
["n-Hexane","n-C6H14","110-54-3","C6H14","HW","NC-6240A","Fixed","SD-1(TYPE NC) Series","0～100%LEL/0～12000ppm"]
["n-Hexane","n-C6H14","110-54-3","C6H14","HW","NC-6240A","Fixed","SD-D58(TYPE NC) Series","0～100%LEL/0～12000ppm"]
["n-Hexane","n-C6H14","110-54-3","C6H14","HW","NC-6245","Fixed","GD-A80 Series","0～100%LEL"]
["n-Hexane","n-C6H14","110-54-3","C6H14","HW","NC-6245","Fixed","GD-D58(TYPE NC) Series","0～100%LEL"]
["n-Hexane","n-C6H14","110-54-3","C6H14","HW","NC-6245","Fixed","SD-1(TYPE NC) Series","0～100%LEL"]
["n-Hexane","n-C6H14","110-54-3","C6H14","HW","NC-6245","Fixed","SD-D58(TYPE NC) Series","0～100%LEL"]
["n-Hexane","n-C6H14","110-54-3","C6H14","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["n-Hexane","n-C6H14","110-54-3","C6H14","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["n-Hexane","n-C6H14","110-54-3","C6H14","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["n-Hexane","n-C6H14","110-54-3","C6H14","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["n-Hexane","n-C6H14","110-54-3","C6H14","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["n-Hexane","n-C6H14","110-54-3","C6H14","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["n-Hexane","n-C6H14","110-54-3","C6H14","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["n-Hexane","n-C6H14","110-54-3","C6H14","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["n-Hexane","n-C6H14","110-54-3","C6H14","SG","SG-8511","Fixed","GD-A80V Series","0～3000ppm/0～5000ppm/0～10000ppm"]
["n-Hexane","n-C6H14","110-54-3","C6H14","SG","SG-8511","Fixed","GD-D58・GH Series","0～3000ppm/0～5000ppm/0～10000ppm"]
["n-Hexane","n-C6H14","110-54-3","C6H14","SG","SG-8511","Fixed","SD-1GH Series","0～3000ppm/0～5000ppm/0～10000ppm"]
["n-Hexane","n-C6H14","110-54-3","C6H14","SG","SG-8511","Fixed","SD-D58・GH Series","0～3000ppm/0～5000ppm/0～10000ppm"]
["n-Hexane","n-C6H14","110-54-3","C6H14","SG","SG-8521","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["n-Hexane","n-C6H14","110-54-3","C6H14","SG","SG-8521","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["n-Hexane","n-C6H14","110-54-3","C6H14","SG","SG-8521","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["n-Hexane","n-C6H14","110-54-3","C6H14","SG","SG-8521","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Nitric Acid","HNO3","7697-37-2","HNO3","ES","ESM-K233","Portable","SC-8000","0～20ppm"]
["Nitric Acid","HNO3","7697-37-2","HNO3","ES","ESU-K233","Fixed","GD-70D Series","0～20ppm"]
["Nitric Acid","HNO3","7697-37-2","HNO3","ES","ESU-K233","Fixed","TP-70D","0～20ppm"]
["Nitric Acid","HNO3","7697-37-2","HNO3","ES","ESM-K233","Fixed","GD-K88Ai Series","0～20ppm"]
["Nitric Acid","HNO3","7697-37-2","HNO3","ES","ESM-K233","Fixed","GD-K88Di Series","0～20ppm"]
["Nitrobenzene","C6H5NO2","98-95-3","C6H5NO2","SG","SG-8562","Fixed","GD-A80V Series","0～200ppm"]
["Nitrobenzene","C6H5NO2","98-95-3","C6H5NO2","SG","SG-8562","Fixed","GD-D58・GH Series","0～200ppm"]
["Nitrobenzene","C6H5NO2","98-95-3","C6H5NO2","SG","SG-8562","Fixed","SD-1GH Series","0～200ppm"]
["Nitrobenzene","C6H5NO2","98-95-3","C6H5NO2","SG","SG-8562","Fixed","SD-D58・GH Series","0～200ppm"]
["Nitrogen Dioxide","NO2","10102-44-0","NO2","ES","ESS-03DH","Portable","GX-6000","0～20ppm"]
["Nitrogen Dioxide","NO2","10102-44-0","NO2","ES","ESM-23AR","Portable","SC-8000","0～15ppm"]
["Nitrogen Dioxide","NO2","10102-44-0","NO2","ES","ESU-23AH","Fixed","GD-70D Series","0～9ppm"]
["Nitrogen Dioxide","NO2","10102-44-0","NO2","ES","ESU-23AH","Fixed","TP-70D","0～9ppm"]
["Nitrogen Dioxide","NO2","10102-44-0","NO2","ES","ESU-23AH","Fixed","GD-70D Series","0～15ppm"]
["Nitrogen Dioxide","NO2","10102-44-0","NO2","ES","ESU-23AH","Fixed","TP-70D","0～15ppm"]
["Nitrogen Dioxide","NO2","10102-44-0","NO2","ES","ESM-23AH","Fixed","GD-K88Ai Series","0～9ppm"]
["Nitrogen Dioxide","NO2","10102-44-0","NO2","ES","ESM-23AH","Fixed","GD-K88Di Series","0～9ppm"]
["Nitrogen Dioxide","NO2","10102-44-0","NO2","ES","ESM-23AH","Fixed","GD-K88Ai Series","0～15ppm"]
["Nitrogen Dioxide","NO2","10102-44-0","NO2","ES","ESM-23AH","Fixed","GD-K88Di Series","0～15ppm"]
["Nitrogen Dioxide","NO2","10102-44-0","NO2","ES","ESM-23AR","Fixed","GD-K88Ai Series","0～9ppm"]
["Nitrogen Dioxide","NO2","10102-44-0","NO2","ES","ESM-23AR","Fixed","GD-K88Di Series","0～9ppm"]
["Nitrogen Dioxide","NO2","10102-44-0","NO2","ES","ESM-23AR","Fixed","GD-K88Ai Series","0～15ppm"]
["Nitrogen Dioxide","NO2","10102-44-0","NO2","ES","ESM-23AR","Fixed","GD-K88Di Series","0～15ppm"]
["Nitrogen Monoxide","NO","10102-43-9","NO","ES","ESM-23A","Portable","SC-8000","0～100ppm"]
["Nitrogen Monoxide","NO","10102-43-9","NO","ES","ESU-23A","Fixed","GD-70D Series","0～100ppm"]
["Nitrogen Monoxide","NO","10102-43-9","NO","ES","ESU-23A","Fixed","TP-70D","0～100ppm"]
["Nitrogen Monoxide","NO","10102-43-9","NO","ES","ESM-23A","Fixed","GD-K88Ai Series","0～100ppm"]
["Nitrogen Monoxide","NO","10102-43-9","NO","ES","ESM-23A","Fixed","GD-K88Di Series","0～100ppm"]
["Nitrogen Tetraoxide","N2O4","10544-72-6","N2O4","ES","ESM-23AR","Fixed","GD-K88Ai Series","0～5ppm"]
["Nitrogen Tetraoxide","N2O4","10544-72-6","N2O4","ES","ESM-23AR","Fixed","GD-K88Di Series","0～5ppm"]
["Nitrogen Tetraoxide","N2O4","10544-72-6","N2O4","ES","ESM-23AR","Fixed","GD-K88Ai Series","0～30ppm"]
["Nitrogen Tetraoxide","N2O4","10544-72-6","N2O4","ES","ESM-23AR","Fixed","GD-K88Di Series","0～30ppm"]
["Nitrogen Trifluoride","NF3","7783-54-2","NF3","ES","ESU-23AH-D","Fixed","GD-70D+PLU Series","0～30ppm","PLU-70 required"]
["Nitrogen Trifluoride","NF3","7783-54-2","NF3","ES","ESU-23AH-D","Fixed","GD-70DG","0～30ppm","PLU-70 required"]
["Nitrogen Trifluoride","NF3","7783-54-2","NF3","ES","ESU-23AH-D","Fixed","TP-70DG","0～30ppm","PLU-70 required"]
["Nitrous oxide","N2O","10024-97-2","N2O","RI","IRU-2428","Fixed","GD-70D(RI) Series","0～500ppm","Only for GD-70D(IRU)"]
["N-Methyl-2-pyrrolidone","NMP","872-50-4","C5H9NO","SG","SGU-8521","Fixed","GD-70D Series","0～1000ppm"]
["N-Methyl-2-pyrrolidone","NMP","872-50-4","C5H9NO","SG","SGU-8521","Fixed","TP-70D","0～1000ppm"]
["N-Methyl-2-pyrrolidone","NMP","872-50-4","C5H9NO","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["N-Methyl-2-pyrrolidone","NMP","872-50-4","C5H9NO","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["N-Methyl-2-pyrrolidone","NMP","872-50-4","C5H9NO","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["N-Methyl-2-pyrrolidone","NMP","872-50-4","C5H9NO","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["N-Methyl-2-pyrrolidone","NMP","872-50-4","C5H9NO","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["N-Methyl-2-pyrrolidone","NMP","872-50-4","C5H9NO","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["N-Methyl-2-pyrrolidone","NMP","872-50-4","C5H9NO","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["N-Methyl-2-pyrrolidone","NMP","872-50-4","C5H9NO","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["N-Methyl-2-pyrrolidone","NMP","872-50-4","C5H9NO","SG","SG-8521","Fixed","GD-A80V Series","0～1000ppm"]
["N-Methyl-2-pyrrolidone","NMP","872-50-4","C5H9NO","SG","SG-8521","Fixed","GD-D58・GH Series","0～1000ppm"]
["N-Methyl-2-pyrrolidone","NMP","872-50-4","C5H9NO","SG","SG-8521","Fixed","SD-1GH Series","0～1000ppm"]
["N-Methyl-2-pyrrolidone","NMP","872-50-4","C5H9NO","SG","SG-8521","Fixed","SD-D58・GH Series","0～1000ppm"]
["N-Methyl-2-pyrrolidone","NMP","872-50-4","C5H9NO","SG","SG-8562","Fixed","GD-A80V Series","0～100ppm/0～150ppm/0～200ppm/0～300ppm/0～500ppm"]
["N-Methyl-2-pyrrolidone","NMP","872-50-4","C5H9NO","SG","SG-8562","Fixed","GD-D58・GH Series","0～100ppm/0～150ppm/0～200ppm/0～300ppm/0～500ppm"]
["N-Methyl-2-pyrrolidone","NMP","872-50-4","C5H9NO","SG","SG-8562","Fixed","SD-1GH Series","0～100ppm/0～150ppm/0～200ppm/0～300ppm/0～500ppm"]
["N-Methyl-2-pyrrolidone","NMP","872-50-4","C5H9NO","SG","SG-8562","Fixed","SD-D58・GH Series","0～100ppm/0～150ppm/0～200ppm/0～300ppm/0～500ppm"]
["n-Octane","C8H18","111-65-9","C8H18","SG","SGU-8511","Fixed","GD-70D Series","0～3000ppm"]
["n-Octane","C8H18","111-65-9","C8H18","SG","SGU-8511","Fixed","TP-70D","0～3000ppm"]
["n-Octane","C8H18","111-65-9","C8H18","SG","SGU-8521","Fixed","GD-70D Series","0～2000ppm"]
["n-Octane","C8H18","111-65-9","C8H18","SG","SGU-8521","Fixed","TP-70D","0～2000ppm"]
["n-Octane","C8H18","111-65-9","C8H18","HW","NCU-6211","Fixed","GD-70D Series","0～100%LEL","Confirm that GD-70D is non-explosion proof"]
["n-Octane","C8H18","111-65-9","C8H18","HW","NCU-6211","Fixed","TP-70D","0～100%LEL","Confirm that GD-70D is non-explosion proof"]
["n-Octane","C8H18","111-65-9","C8H18","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["n-Octane","C8H18","111-65-9","C8H18","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["n-Octane","C8H18","111-65-9","C8H18","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～8000ppm"]
["n-Octane","C8H18","111-65-9","C8H18","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～8000ppm"]
["n-Octane","C8H18","111-65-9","C8H18","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～8000ppm"]
["n-Octane","C8H18","111-65-9","C8H18","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～8000ppm"]
["n-Octane","C8H18","111-65-9","C8H18","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～8000ppm"]
["n-Octane","C8H18","111-65-9","C8H18","HW","NC-6240A","Fixed","GD-A80 Series","0～100%LEL/0～8000ppm"]
["n-Octane","C8H18","111-65-9","C8H18","HW","NC-6240A","Fixed","GD-D58(TYPE NC) Series","0～100%LEL/0～8000ppm"]
["n-Octane","C8H18","111-65-9","C8H18","HW","NC-6240A","Fixed","SD-1(TYPE NC) Series","0～100%LEL/0～8000ppm"]
["n-Octane","C8H18","111-65-9","C8H18","HW","NC-6240A","Fixed","SD-D58(TYPE NC) Series","0～100%LEL/0～8000ppm"]
["n-Octane","C8H18","111-65-9","C8H18","HW","NC-6245","Fixed","GD-A80 Series","0～100%LEL"]
["n-Octane","C8H18","111-65-9","C8H18","HW","NC-6245","Fixed","GD-D58(TYPE NC) Series","0～100%LEL"]
["n-Octane","C8H18","111-65-9","C8H18","HW","NC-6245","Fixed","SD-1(TYPE NC) Series","0～100%LEL"]
["n-Octane","C8H18","111-65-9","C8H18","HW","NC-6245","Fixed","SD-D58(TYPE NC) Series","0～100%LEL"]
["n-Octane","C8H18","111-65-9","C8H18","HW","NC-6250","Fixed","GD-A80 Series","0～100%LEL/0～8000ppm"]
["n-Octane","C8H18","111-65-9","C8H18","HW","NC-6250","Fixed","GD-D58(TYPE NC) Series","0～100%LEL/0～8000ppm"]
["n-Octane","C8H18","111-65-9","C8H18","SG","SG-8511","Fixed","GD-A80V Series","0～3000ppm/0～5000ppm"]
["n-Octane","C8H18","111-65-9","C8H18","SG","SG-8511","Fixed","GD-D58・GH Series","0～3000ppm/0～5000ppm"]
["n-Octane","C8H18","111-65-9","C8H18","SG","SG-8511","Fixed","SD-1GH Series","0～3000ppm/0～5000ppm"]
["n-Octane","C8H18","111-65-9","C8H18","SG","SG-8511","Fixed","SD-D58・GH Series","0～3000ppm/0～5000ppm"]
["n-Octane","C8H18","111-65-9","C8H18","SG","SG-8521","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["n-Octane","C8H18","111-65-9","C8H18","SG","SG-8521","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["n-Octane","C8H18","111-65-9","C8H18","SG","SG-8521","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["n-Octane","C8H18","111-65-9","C8H18","SG","SG-8521","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["n-Octyl Acetate","OCTYLAc","112-14-1","C10H20O2","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["n-Octyl Acetate","OCTYLAc","112-14-1","C10H20O2","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["n-Octyl Acetate","OCTYLAc","112-14-1","C10H20O2","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["n-Octyl Acetate","OCTYLAc","112-14-1","C10H20O2","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["n-Octyl Acetate","OCTYLAc","112-14-1","C10H20O2","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["n-Octyl Acetate","OCTYLAc","112-14-1","C10H20O2","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["n-Octyl Acetate","OCTYLAc","112-14-1","C10H20O2","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["n-Octyl Acetate","OCTYLAc","112-14-1","C10H20O2","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["Nonane","C9H20","111-84-2","C9H20","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Nonane","C9H20","111-84-2","C9H20","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Nonane","C9H20","111-84-2","C9H20","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～7000ppm"]
["Nonane","C9H20","111-84-2","C9H20","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～7000ppm"]
["Nonane","C9H20","111-84-2","C9H20","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～7000ppm"]
["Nonane","C9H20","111-84-2","C9H20","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～7000ppm"]
["Nonane","C9H20","111-84-2","C9H20","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～7000ppm"]
["Nonane","C9H20","111-84-2","C9H20","SG","SG-8521","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Nonane","C9H20","111-84-2","C9H20","SG","SG-8521","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Nonane","C9H20","111-84-2","C9H20","SG","SG-8521","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Nonane","C9H20","111-84-2","C9H20","SG","SG-8521","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["n-Propanol","C3H8O","71-23-8","C3H8O","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["n-Propanol","C3H8O","71-23-8","C3H8O","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["n-Propanol","C3H8O","71-23-8","C3H8O","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～21000ppm"]
["n-Propanol","C3H8O","71-23-8","C3H8O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～21000ppm"]
["n-Propanol","C3H8O","71-23-8","C3H8O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～21000ppm"]
["n-Propanol","C3H8O","71-23-8","C3H8O","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～21000ppm"]
["n-Propanol","C3H8O","71-23-8","C3H8O","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～21000ppm"]
["n-Propanol","C3H8O","71-23-8","C3H8O","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["n-Propanol","C3H8O","71-23-8","C3H8O","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["n-Propanol","C3H8O","71-23-8","C3H8O","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["n-Propanol","C3H8O","71-23-8","C3H8O","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["n-Propanol","C3H8O","71-23-8","C3H8O","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["n-Propanol","C3H8O","71-23-8","C3H8O","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["n-Propanol","C3H8O","71-23-8","C3H8O","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["n-Propanol","C3H8O","71-23-8","C3H8O","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["n-Propanol","C3H8O","71-23-8","C3H8O","SG","SG-8521","Fixed","GD-A80V Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["n-Propanol","C3H8O","71-23-8","C3H8O","SG","SG-8521","Fixed","GD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["n-Propanol","C3H8O","71-23-8","C3H8O","SG","SG-8521","Fixed","SD-1GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["n-Propanol","C3H8O","71-23-8","C3H8O","SG","SG-8521","Fixed","SD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["n-Propyl acetate","ｎPAc","109-60-4","C5H10O2","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["n-Propyl acetate","ｎPAc","109-60-4","C5H10O2","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["n-Propyl acetate","ｎPAc","109-60-4","C5H10O2","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～17000ppm"]
["n-Propyl acetate","ｎPAc","109-60-4","C5H10O2","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～17000ppm"]
["n-Propyl acetate","ｎPAc","109-60-4","C5H10O2","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～17000ppm"]
["n-Propyl acetate","ｎPAc","109-60-4","C5H10O2","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～17000ppm"]
["n-Propyl acetate","ｎPAc","109-60-4","C5H10O2","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～17000ppm"]
["N-Vinyl-2-pyrrolidone","C6H9NO","88-12-0","C6H9NO","SG","SG-8562","Fixed","GD-A80V Series","0～100ppm"]
["N-Vinyl-2-pyrrolidone","C6H9NO","88-12-0","C6H9NO","SG","SG-8562","Fixed","GD-D58・GH Series","0～100ppm"]
["N-Vinyl-2-pyrrolidone","C6H9NO","88-12-0","C6H9NO","SG","SG-8562","Fixed","SD-1GH Series","0～100ppm"]
["N-Vinyl-2-pyrrolidone","C6H9NO","88-12-0","C6H9NO","SG","SG-8562","Fixed","SD-D58・GH Series","0～100ppm"]
["Octa-fluorocyclobutane","FC-C318","115-25-3","C4F8","RI","DE-2113-37","Fixed","RI-257","0～5000ppm"]
["Octafluorocyclopentene","C5F8","559-40-0","C5F8","ES","ESU-K235L","Fixed","TP-70DGⅡ Series","0～5ppm","Only for TP-70DGⅡ"]
["Octafluorocyclopentene","C5F8","559-40-0","C5F8","SG","SGU-8521","Fixed","GD-70D Series","0～2000ppm"]
["Octafluorocyclopentene","C5F8","559-40-0","C5F8","SG","SGU-8521","Fixed","TP-70D","0～2000ppm"]
["Octafluorocyclopentene","C5F8","559-40-0","C5F8","SG","SG-8521","Fixed","GD-A80V Series","0～2000ppm/0～3000ppm/0～5000ppm"]
["Octafluorocyclopentene","C5F8","559-40-0","C5F8","SG","SG-8521","Fixed","GD-D58・GH Series","0～2000ppm/0～3000ppm/0～5000ppm"]
["Octafluorocyclopentene","C5F8","559-40-0","C5F8","SG","SG-8521","Fixed","SD-1GH Series","0～2000ppm/0～3000ppm/0～5000ppm"]
["Octafluorocyclopentene","C5F8","559-40-0","C5F8","SG","SG-8521","Fixed","SD-D58・GH Series","0～2000ppm/0～3000ppm/0～5000ppm"]
["Octafluoropropane","C3F8","76-19-7","C3F8","RI","DE-2113-37","Fixed","RI-257","0～5000ppm"]
["Octamethylcyclotetrasiloxane","OMCTS","556-67-2","C8H24O4Si4","SS","SSU-1925","Fixed","GD-70D+PLU Series","0～3ppm","PLU-70 required"]
["Octamethylcyclotetrasiloxane","OMCTS","556-67-2","C8H24O4Si4","SS","SSU-1925","Fixed","GD-70DG","0～3ppm","PLU-70 required"]
["Octamethylcyclotetrasiloxane","OMCTS","556-67-2","C8H24O4Si4","RI","DE-2113-35","Fixed","RI-257","0～1000ppm"]
["OK73 thinner","OK-73","-","-","SG","SGU-8521","Fixed","GD-70D Series","0～1000ppm"]
["OK73 thinner","OK-73","-","-","SG","SGU-8521","Fixed","TP-70D","0～1000ppm"]
["Oxygen","O2","7782-44-7","O2","OS","OS-BM2C","Portable","GX-2009","0～25vol%"]
["Oxygen","O2","7782-44-7","O2","OS","OS-BM2C","Portable","GX-2012","0～25vol%"]
["Oxygen","O2","7782-44-7","O2","OS","OS-BM2C","Portable","GX-2012GT","0～25vol%"]
["Oxygen","O2","7782-44-7","O2","OS","OS-BM2C","Portable","GX-6000","0～25vol%"]
["Oxygen","O2","7782-44-7","O2","OS","OS-BM2C","Portable","OX-03","0～25vol%"]
["Oxygen","O2","7782-44-7","O2","OS","OS-BM1","Portable","GX-8000","0～25vol%"]
["Oxygen","O2","7782-44-7","O2","OS","OS-BM1","Portable","GX-8000(TYPE O2)","0～25vol%"]
["Oxygen","O2","7782-44-7","O2","OS","OS-BM1","Portable","RX-8000","0～25vol%"]
["Oxygen","O2","7782-44-7","O2","OS","OS-BM1","Portable","RX-8500","0～25vol%"]
["Oxygen","O2","7782-44-7","O2","OS","OS-BM1","Portable","RX-8700","0～25vol%"]
["Oxygen","O2","7782-44-7","O2","OS","OS-BM1","Portable","CX-5","0～25vol%"]
["Oxygen","O2","7782-44-7","O2","ES","ESU-X23","Fixed","GD-70D Series","0～25vol%"]
["Oxygen","O2","7782-44-7","O2","ES","ESU-X23","Fixed","TP-70D","0～25vol%"]
["Oxygen","O2","7782-44-7","O2","OS","OSU-8078","Fixed","GD-70D Series","0～5vol%","H-HH(standard)、L-LL、L-H"]
["Oxygen","O2","7782-44-7","O2","OS","OSU-8078","Fixed","TP-70D","0～5vol%","H-HH(standard)、L-LL、L-H"]
["Oxygen","O2","7782-44-7","O2","OS","OSU-8078","Fixed","GD-70D Series","0‐25vol%","L-LL(standard)、L-H/Suppress：20.9±0.5"]
["Oxygen","O2","7782-44-7","O2","OS","OSU-8078","Fixed","TP-70D","0‐25vol%","L-LL(standard)、L-H/Suppress：20.9±0.5"]
["Oxygen","O2","7782-44-7","O2","OS","OSU-8078","Fixed","GD-70D Series","0～50vol%","H-HH"]
["Oxygen","O2","7782-44-7","O2","OS","OSU-8078","Fixed","TP-70D","0～50vol%","H-HH"]
["Oxygen","O2","7782-44-7","O2","OS","OSU-8078","Fixed","GD-70D Series","0～100vol%","H-HH"]
["Oxygen","O2","7782-44-7","O2","OS","OSU-8078","Fixed","TP-70D","0～100vol%","H-HH"]
["Oxygen","O2","7782-44-7","O2","OS","OSU-8078TF-A","Fixed","GD-70D Series","0‐25vol%","Against solvent"]
["Oxygen","O2","7782-44-7","O2","OS","OSU-8078TF-A","Fixed","TP-70D","0‐25vol%","Against solvent"]
["Oxygen","O2","7782-44-7","O2","OS","OS-B11-A","Fixed","GD-F3A-A Series","0～5vol%/0～10vol%/0～25vol%"]
["Oxygen","O2","7782-44-7","O2","OS","OS-B11-A","Fixed","GD-F4A-A Series","0～5vol%/0～10vol%/0～25vol%"]
["Oxygen","O2","7782-44-7","O2","OS","OS-B11-A","Fixed","GD-F88Ai Series","0～5vol%/0～10vol%/0～25vol%"]
["Oxygen","O2","7782-44-7","O2","OS","OS-B11-A","Fixed","GD-F88Di Series","0～5vol%/0～10vol%/0～25vol%"]
["Oxygen","O2","7782-44-7","O2","OS","OS-B11TF-A","Fixed","GD-F3A-A Series","0～5vol%/0～10vol%/0～25vol%","Against solvent"]
["Oxygen","O2","7782-44-7","O2","OS","OS-B11TF-A","Fixed","GD-F4A-A Series","0～5vol%/0～10vol%/0～25vol%","Against solvent"]
["Oxygen","O2","7782-44-7","O2","OS","OS-B11TF-A","Fixed","GD-F88Ai Series","0～5vol%/0～10vol%/0～25vol%","Against solvent"]
["Oxygen","O2","7782-44-7","O2","OS","OS-B11TF-A","Fixed","GD-F88Di Series","0～5vol%/0～10vol%/0～25vol%","Against solvent"]
["Oxygen","O2","7782-44-7","O2","OS","OS-B11TFX-A","Fixed","GD-F3A-A Series","0～5vol%/0～10vol%/0～25vol%","Against solvent"]
["Oxygen","O2","7782-44-7","O2","OS","OS-B11TFX-A","Fixed","GD-F4A-A Series","0～5vol%/0～10vol%/0～25vol%","Against solvent"]
["Oxygen","O2","7782-44-7","O2","OS","OS-B11TFX-A","Fixed","GD-F88Ai Series","0～5vol%/0～10vol%/0～25vol%","Against solvent"]
["Oxygen","O2","7782-44-7","O2","OS","OS-B11TFX-A","Fixed","GD-F88Di Series","0～5vol%/0～10vol%/0～25vol%","Against solvent"]
["Oxygen","O2","7782-44-7","O2","OS","OS-B11E-A","Fixed","SD-1OX Series","0～5vol%/0～10vol%/0～25vol%"]
["Oxygen","O2","7782-44-7","O2","OS","OS-B11E-A","Fixed","SDWL-1OX Series","0～5vol%/0～10vol%/0～25vol%"]
["Oxygen","O2","7782-44-7","O2","OS","OS-B11TFE-A","Fixed","SD-1OX Series","0～5vol%/0～10vol%/0～25vol%","Against solvent"]
["Oxygen","O2","7782-44-7","O2","OS","OS-B11TFE-A","Fixed","SDWL-1OX Series","0～5vol%/0～10vol%/0～25vol%","Against solvent"]
["Oxygen","O2","7782-44-7","O2","OS","OS-B11TFXE-A","Fixed","SD-1OX Series","0～5vol%/0～10vol%/0～25vol%","Against solvent"]
["Oxygen","O2","7782-44-7","O2","OS","OS-B11TFXE-A","Fixed","SDWL-1OX Series","0～5vol%/0～10vol%/0～25vol%","Against solvent"]
["Ozone","O3","10028-15-6","O3","ES","ESM-K239C","Portable","SC-8000","0～1ppm"]
["Ozone","O3","10028-15-6","O3","ES","ESU-K239C","Fixed","GD-70D Series","0～1ppm"]
["Ozone","O3","10028-15-6","O3","ES","ESU-K239C","Fixed","TP-70D","0～1ppm"]
["Ozone","O3","10028-15-6","O3","ES","ESU-K239C-S","Fixed","GD-70D Series","0～0.6ppm"]
["Ozone","O3","10028-15-6","O3","ES","ESU-K239C-S","Fixed","TP-70D","0～0.6ppm"]
["Ozone","O3","10028-15-6","O3","ES","ESU-K239CL-S","Fixed","GD-70D Series","0～0.6ppm","Sensor for low humidity/Range: ～62%RH"]
["Ozone","O3","10028-15-6","O3","ES","ESU-K239CL-S","Fixed","TP-70D","0～0.6ppm","Sensor for low humidity/Range: ～62%RH"]
["Ozone","O3","10028-15-6","O3","ES","ESM-K239C","Fixed","GD-K88Ai Series","0～1ppm"]
["Ozone","O3","10028-15-6","O3","ES","ESM-K239C","Fixed","GD-K88Di Series","0～1ppm"]
["Ozone","O3","10028-15-6","O3","ES","ESM-K239C-S","Fixed","GD-K88Ai Series","0～0.6ppm"]
["Ozone","O3","10028-15-6","O3","ES","ESM-K239C-S","Fixed","GD-K88Di Series","0～0.6ppm"]
["Ozone","O3","10028-15-6","O3","ES","ESM-K239CL","Fixed","GD-K88Ai Series","0～1ppm"]
["Ozone","O3","10028-15-6","O3","ES","ESM-K239CL","Fixed","GD-K88Di Series","0～1ppm"]
["Ozone","O3","10028-15-6","O3","ES","ESM-K239CL-S","Fixed","GD-K88Ai Series","0～0.6ppm","Sensor for low humidity/Range: ～62%RH"]
["Ozone","O3","10028-15-6","O3","ES","ESM-K239CL-S","Fixed","GD-K88Di Series","0～0.6ppm","Sensor for low humidity/Range: ～62%RH"]
["Pentane","n-C5H12","109-66-0","C5H12","HW","NC-6215","Portable","GP-1000(Specified cal.gas)","0～100%LEL"]
["Pentane","n-C5H12","109-66-0","C5H12","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Pentane","n-C5H12","109-66-0","C5H12","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Pentane","n-C5H12","109-66-0","C5H12","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～15000ppm"]
["Pentane","n-C5H12","109-66-0","C5H12","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～15000ppm"]
["Pentane","n-C5H12","109-66-0","C5H12","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～15000ppm"]
["Pentane","n-C5H12","109-66-0","C5H12","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～15000ppm"]
["Pentane","n-C5H12","109-66-0","C5H12","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～15000ppm"]
["Pentane","n-C5H12","109-66-0","C5H12","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Pentane","n-C5H12","109-66-0","C5H12","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Pentane","n-C5H12","109-66-0","C5H12","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Pentane","n-C5H12","109-66-0","C5H12","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Pentane","n-C5H12","109-66-0","C5H12","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Pentane","n-C5H12","109-66-0","C5H12","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Pentane","n-C5H12","109-66-0","C5H12","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Pentane","n-C5H12","109-66-0","C5H12","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["Pentane","n-C5H12","109-66-0","C5H12","SG","SG-8511","Fixed","GD-A80V Series","0～3000ppm/0～5000ppm"]
["Pentane","n-C5H12","109-66-0","C5H12","SG","SG-8511","Fixed","GD-D58・GH Series","0～3000ppm/0～5000ppm"]
["Pentane","n-C5H12","109-66-0","C5H12","SG","SG-8511","Fixed","SD-1GH Series","0～3000ppm/0～5000ppm"]
["Pentane","n-C5H12","109-66-0","C5H12","SG","SG-8511","Fixed","SD-D58・GH Series","0～3000ppm/0～5000ppm"]
["Pentane","n-C5H12","109-66-0","C5H12","SG","SG-8521","Fixed","GD-A80V Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Pentane","n-C5H12","109-66-0","C5H12","SG","SG-8521","Fixed","GD-D58・GH Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Pentane","n-C5H12","109-66-0","C5H12","SG","SG-8521","Fixed","SD-1GH Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Pentane","n-C5H12","109-66-0","C5H12","SG","SG-8521","Fixed","SD-D58・GH Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Perfluoro(methyl vinyl ether)","PMVE","1187-93-5","C3OF6","SG","SG-8511","Fixed","GD-A80V Series","0～10000ppm"]
["Perfluoro(methyl vinyl ether)","PMVE","1187-93-5","C3OF6","SG","SG-8511","Fixed","GD-D58・GH Series","0～10000ppm"]
["Perfluoro(methyl vinyl ether)","PMVE","1187-93-5","C3OF6","SG","SG-8511","Fixed","SD-1GH Series","0～10000ppm"]
["Perfluoro(methyl vinyl ether)","PMVE","1187-93-5","C3OF6","SG","SG-8511","Fixed","SD-D58・GH Series","0～10000ppm"]
["Phenol","C6H5OH","108-95-2","C6H6O","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Phenol","C6H5OH","108-95-2","C6H6O","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Phenol","C6H5OH","108-95-2","C6H6O","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Phenol","C6H5OH","108-95-2","C6H6O","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Phenol","C6H5OH","108-95-2","C6H6O","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Phenol","C6H5OH","108-95-2","C6H6O","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Phenol","C6H5OH","108-95-2","C6H6O","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Phenol","C6H5OH","108-95-2","C6H6O","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["Phenol","C6H5OH","108-95-2","C6H6O","SG","SG-8521","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Phenol","C6H5OH","108-95-2","C6H6O","SG","SG-8521","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Phenol","C6H5OH","108-95-2","C6H6O","SG","SG-8521","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Phenol","C6H5OH","108-95-2","C6H6O","SG","SG-8521","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Phosgene","COCL2","75-44-5","COCL2","ES","ESM-D25BY","Fixed","GD-K88Ai Series","0～0.3ppm"]
["Phosphine","PH3","7803-51-2","PH3","SH","SH-8662","Portable","SP-220(TYPE FUM)","0～4.5ppm"]
["Phosphine","PH3","7803-51-2","PH3","SH","SH-8662","Portable","SP-220(TYPE SC)","0～2ppm"]
["Phosphine","PH3","7803-51-2","PH3","ES","ESM-01DH","Portable","SC-01","0～1ppm"]
["Phosphine","PH3","7803-51-2","PH3","ES","ESM-23DH","Portable","SC-8000","0～1ppm"]
["Phosphine","PH3","7803-51-2","PH3","ES","ESM-23DH","Portable","SC-8000","0～10ppm"]
["Phosphine","PH3","7803-51-2","PH3","ES","ESU-23DH","Fixed","GD-70D Series","0～1ppm"]
["Phosphine","PH3","7803-51-2","PH3","ES","ESU-23DH","Fixed","TP-70D","0～1ppm"]
["Phosphine","PH3","7803-51-2","PH3","ES","ESU-23AH","Fixed","GD-70D Series","0～1ppm"]
["Phosphine","PH3","7803-51-2","PH3","ES","ESU-23AH","Fixed","TP-70D","0～1ppm"]
["Phosphine","PH3","7803-51-2","PH3","ES","ESM-23AH","Fixed","GD-K88Ai Series","0～1ppm"]
["Phosphine","PH3","7803-51-2","PH3","ES","ESM-23AH","Fixed","GD-K88Di Series","0～1ppm"]
["Phosphine","PH3","7803-51-2","PH3","ES","ESM-23DH","Fixed","GD-K88Ai Series","0～1ppm"]
["Phosphine","PH3","7803-51-2","PH3","ES","ESM-23DH","Fixed","GD-K88Di Series","0～1ppm"]
["Phosphorus Trifluoride","PF3","7783-55-3","PF3","ES","ESU-23DH","Fixed","GD-70D Series","0～10ppm"]
["Phosphorus Trifluoride","PF3","7783-55-3","PF3","ES","ESU-23DH","Fixed","TP-70D","0～10ppm"]
["Phosphorus Trifluoride","PF3","7783-55-3","PF3","ES","ESM-23DH","Fixed","GD-K88Ai Series","0～10ppm"]
["Phosphorus Trifluoride","PF3","7783-55-3","PF3","ES","ESM-23DH","Fixed","GD-K88Di Series","0～10ppm"]
["Propane","C3H8","74-98-6","C3H8","HW","NC-6215","Portable","GP-1000(CH4)","0～100%LEL"]
["Propane","C3H8","74-98-6","C3H8","HW","NC-6307","Portable","NC-1000(CH4)","0～10000ppm"]
["Propane","C3H8","74-98-6","C3H8","TE","TE-7515W","Portable","NP-1000(CH4)","0～100vol%"]
["Propane","C3H8","74-98-6","C3H8","SH","SH-8662","Portable","SP-220(TYPE SC)","0～20ppm"]
["Propane","C3H8","74-98-6","C3H8","SH","SH-8661","Portable","SP-220(TYPE F)","0～10000ppm"]
["Propane","C3H8","74-98-6","C3H8","SH","SH-8661","Portable","SP-220(TYPE H2)","0～10000ppm"]
["Propane","C3H8","74-98-6","C3H8","SG","SGU-8511","Fixed","GD-70D Series","0～2000ppm"]
["Propane","C3H8","74-98-6","C3H8","SG","SGU-8511","Fixed","TP-70D","0～2000ppm"]
["Propane","C3H8","74-98-6","C3H8","SG","SGU-8511","Fixed","GD-70D Series","0～5000ppm"]
["Propane","C3H8","74-98-6","C3H8","SG","SGU-8511","Fixed","TP-70D","0～5000ppm"]
["Propane","C3H8","74-98-6","C3H8","SG","SGU-8582","Fixed","GD-70D Series","0～2000ppm"]
["Propane","C3H8","74-98-6","C3H8","SG","SGU-8582","Fixed","TP-70D","0～2000ppm"]
["Propane","C3H8","74-98-6","C3H8","HW","NCU-6211","Fixed","GD-70D Series","0～100%LEL","Confirm that GD-70D is non-explosion proof"]
["Propane","C3H8","74-98-6","C3H8","HW","NCU-6211","Fixed","TP-70D","0～100%LEL","Confirm that GD-70D is non-explosion proof"]
["Propane","C3H8","74-98-6","C3H8","RI","DE-2113-60","Fixed","RI-557","0～20vol%"]
["Propane","C3H8","74-98-6","C3H8","RI","DE-3315-2","Fixed","SD-1RI Series","0～100%LEL"]
["Propane","C3H8","74-98-6","C3H8","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Propane","C3H8","74-98-6","C3H8","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Propane","C3H8","74-98-6","C3H8","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～20000ppm"]
["Propane","C3H8","74-98-6","C3H8","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～20000ppm"]
["Propane","C3H8","74-98-6","C3H8","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～20000ppm"]
["Propane","C3H8","74-98-6","C3H8","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～20000ppm"]
["Propane","C3H8","74-98-6","C3H8","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～20000ppm"]
["Propane","C3H8","74-98-6","C3H8","HW","HW-6213/NC-6213","Fixed","GD-A80 Series","0～100%LEL/0～20000ppm"]
["Propane","C3H8","74-98-6","C3H8","HW","HW-6213/NC-6213","Fixed","GD-D58(TYPE GP) Series","0～100%LEL/0～20000ppm"]
["Propane","C3H8","74-98-6","C3H8","HW","HW-6213/NC-6213","Fixed","GD-D58(TYPE NC) Series","0～100%LEL/0～20000ppm"]
["Propane","C3H8","74-98-6","C3H8","HW","HW-6239","Fixed","GD-A80-70 Series","0～100%LEL"]
["Propane","C3H8","74-98-6","C3H8","HW","HW-6239","Fixed","SD-1(TYPE GP) Series","0～100%LEL"]
["Propane","C3H8","74-98-6","C3H8","HW","HW-6239","Fixed","SD-D58(TYPE GP) Series","0～100%LEL"]
["Propane","C3H8","74-98-6","C3H8","HW","HW-6239/NC-6239","Fixed","GD-A80 Series","0～100%LEL/0～20000ppm"]
["Propane","C3H8","74-98-6","C3H8","HW","HW-6239/NC-6239","Fixed","GD-D58(TYPE GP) Series","0～100%LEL/0～20000ppm"]
["Propane","C3H8","74-98-6","C3H8","HW","HW-6239/NC-6239","Fixed","GD-D58(TYPE NC) Series","0～100%LEL/0～20000ppm"]
["Propane","C3H8","74-98-6","C3H8","HW","HW-6239/NC-6239","Fixed","SD-1(TYPE NC) Series","0～100%LEL/0～20000ppm"]
["Propane","C3H8","74-98-6","C3H8","HW","HW-6239/NC-6239","Fixed","SD-D58(TYPE NC) Series","0～100%LEL/0～20000ppm"]
["Propane","C3H8","74-98-6","C3H8","HW","NC-6240A","Fixed","GD-A80 Series","0～100%LEL/0～20000ppm"]
["Propane","C3H8","74-98-6","C3H8","HW","NC-6240A","Fixed","GD-D58(TYPE NC) Series","0～100%LEL/0～20000ppm"]
["Propane","C3H8","74-98-6","C3H8","HW","NC-6240A","Fixed","SD-1(TYPE NC) Series","0～100%LEL/0～20000ppm"]
["Propane","C3H8","74-98-6","C3H8","HW","NC-6240A","Fixed","SD-D58(TYPE NC) Series","0～100%LEL/0～20000ppm"]
["Propane","C3H8","74-98-6","C3H8","HW","NC-6245","Fixed","GD-A80 Series","0～100%LEL"]
["Propane","C3H8","74-98-6","C3H8","HW","NC-6245","Fixed","GD-D58(TYPE NC) Series","0～100%LEL"]
["Propane","C3H8","74-98-6","C3H8","HW","NC-6245","Fixed","SD-1(TYPE NC) Series","0～100%LEL"]
["Propane","C3H8","74-98-6","C3H8","HW","NC-6245","Fixed","SD-D58(TYPE NC) Series","0～100%LEL"]
["Propane","C3H8","74-98-6","C3H8","HW","NC-6250","Fixed","GD-A80 Series","0～100%LEL/0～20000ppm"]
["Propane","C3H8","74-98-6","C3H8","HW","NC-6250","Fixed","GD-D58(TYPE NC) Series","0～100%LEL/0～20000ppm"]
["Propane","C3H8","74-98-6","C3H8","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Propane","C3H8","74-98-6","C3H8","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Propane","C3H8","74-98-6","C3H8","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Propane","C3H8","74-98-6","C3H8","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Propane","C3H8","74-98-6","C3H8","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Propane","C3H8","74-98-6","C3H8","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Propane","C3H8","74-98-6","C3H8","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Propane","C3H8","74-98-6","C3H8","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["Propane","C3H8","74-98-6","C3H8","SG","SG-8511","Fixed","GD-A80V Series","0～2000ppm/0～3000ppm/0～5000ppm/0～10000ppm/0～20000ppm/0～50%LEL/0～100%LEL"]
["Propane","C3H8","74-98-6","C3H8","SG","SG-8511","Fixed","GD-D58・GH Series","0～2000ppm/0～3000ppm/0～5000ppm/0～10000ppm/0～20000ppm/0～50%LEL/0～100%LEL"]
["Propane","C3H8","74-98-6","C3H8","SG","SG-8511","Fixed","SD-1GH Series","0～2000ppm/0～3000ppm/0～5000ppm/0～10000ppm/0～20000ppm/0～50%LEL/0～100%LEL"]
["Propane","C3H8","74-98-6","C3H8","SG","SG-8511","Fixed","SD-D58・GH Series","0～2000ppm/0～3000ppm/0～5000ppm/0～10000ppm/0～20000ppm/0～50%LEL/0～100%LEL"]
["Propane","C3H8","74-98-6","C3H8","SG","SG-8521","Fixed","GD-A80V Series","★0～500ppm/★0～1000ppm","★Range easily affected by environmental conditions and other"]
["Propane","C3H8","74-98-6","C3H8","SG","SG-8521","Fixed","GD-D58・GH Series","★0～500ppm/★0～1000ppm","★Range easily affected by environmental conditions and other"]
["Propane","C3H8","74-98-6","C3H8","SG","SG-8521","Fixed","SD-1GH Series","★0～500ppm/★0～1000ppm","★Range easily affected by environmental conditions and other"]
["Propane","C3H8","74-98-6","C3H8","SG","SG-8521","Fixed","SD-D58・GH Series","★0～500ppm/★0～1000ppm","★Range easily affected by environmental conditions and other"]
["Propane","C3H8","74-98-6","C3H8","SG","SG-8582","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Propane","C3H8","74-98-6","C3H8","SG","SG-8582","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Propane","C3H8","74-98-6","C3H8","SG","SG-8582","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Propane","C3H8","74-98-6","C3H8","SG","SG-8582","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Propionaldehyde","C2H5CHO","123-38-6","C3H6O","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Propionaldehyde","C2H5CHO","123-38-6","C3H6O","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Propionaldehyde","C2H5CHO","123-38-6","C3H6O","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～23000ppm"]
["Propionaldehyde","C2H5CHO","123-38-6","C3H6O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～23000ppm"]
["Propionaldehyde","C2H5CHO","123-38-6","C3H6O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～23000ppm"]
["Propionaldehyde","C2H5CHO","123-38-6","C3H6O","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～23000ppm"]
["Propionaldehyde","C2H5CHO","123-38-6","C3H6O","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～23000ppm"]
["Propionic acid","Pacid","79-09-4","C3H6O2","SG","SG-8562","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Propionic acid","Pacid","79-09-4","C3H6O2","SG","SG-8562","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Propionic acid","Pacid","79-09-4","C3H6O2","SG","SG-8562","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Propionic acid","Pacid","79-09-4","C3H6O2","SG","SG-8562","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Propionitrile","C3H5N","107-12-0","C3H5N","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Propionitrile","C3H5N","107-12-0","C3H5N","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Propionitrile","C3H5N","107-12-0","C3H5N","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～31000ppm"]
["Propionitrile","C3H5N","107-12-0","C3H5N","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～31000ppm"]
["Propionitrile","C3H5N","107-12-0","C3H5N","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～31000ppm"]
["Propionitrile","C3H5N","107-12-0","C3H5N","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～31000ppm"]
["Propionitrile","C3H5N","107-12-0","C3H5N","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～31000ppm"]
["Propylamine","nPA","107-10-8","C3H9N","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Propylamine","nPA","107-10-8","C3H9N","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Propylamine","nPA","107-10-8","C3H9N","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～20000ppm"]
["Propylamine","nPA","107-10-8","C3H9N","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～20000ppm"]
["Propylamine","nPA","107-10-8","C3H9N","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～20000ppm"]
["Propylamine","nPA","107-10-8","C3H9N","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～20000ppm"]
["Propylamine","nPA","107-10-8","C3H9N","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～20000ppm"]
["Propylene","C3H6","115-07-1","C3H6","HW","NC-6215","Portable","GP-1000(HC/CH4)","0～100%LEL"]
["Propylene","C3H6","115-07-1","C3H6","HW","NC-6307","Portable","NC-1000(HC/CH4)","0～10000ppm"]
["Propylene","C3H6","115-07-1","C3H6","SH","SH-8661","Portable","SP-220(TYPE H2)","0～10000ppm"]
["Propylene","C3H6","115-07-1","C3H6","SG","SGU-8511","Fixed","GD-70D Series","0～2000ppm"]
["Propylene","C3H6","115-07-1","C3H6","SG","SGU-8511","Fixed","TP-70D","0～2000ppm"]
["Propylene","C3H6","115-07-1","C3H6","SG","SGU-8521","Fixed","GD-70D Series","0～2000ppm"]
["Propylene","C3H6","115-07-1","C3H6","SG","SGU-8521","Fixed","TP-70D","0～2000ppm"]
["Propylene","C3H6","115-07-1","C3H6","SG","SGU-8511","Fixed","GD-70D Series","0～5000ppm"]
["Propylene","C3H6","115-07-1","C3H6","SG","SGU-8511","Fixed","TP-70D","0～5000ppm"]
["Propylene","C3H6","115-07-1","C3H6","HW","NCU-6211","Fixed","GD-70D Series","0～100%LEL","Confirm that GD-70D is non-explosion proof"]
["Propylene","C3H6","115-07-1","C3H6","HW","NCU-6211","Fixed","TP-70D","0～100%LEL","Confirm that GD-70D is non-explosion proof"]
["Propylene","C3H6","115-07-1","C3H6","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Propylene","C3H6","115-07-1","C3H6","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Propylene","C3H6","115-07-1","C3H6","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～20000ppm"]
["Propylene","C3H6","115-07-1","C3H6","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～20000ppm"]
["Propylene","C3H6","115-07-1","C3H6","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～20000ppm"]
["Propylene","C3H6","115-07-1","C3H6","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～20000ppm"]
["Propylene","C3H6","115-07-1","C3H6","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～20000ppm"]
["Propylene","C3H6","115-07-1","C3H6","HW","HW-6239","Fixed","GD-A80-70 Series","0～100%LEL"]
["Propylene","C3H6","115-07-1","C3H6","HW","HW-6239","Fixed","SD-1(TYPE GP) Series","0～100%LEL"]
["Propylene","C3H6","115-07-1","C3H6","HW","HW-6239","Fixed","SD-D58(TYPE GP) Series","0～100%LEL"]
["Propylene","C3H6","115-07-1","C3H6","HW","HW-6239/NC-6239","Fixed","GD-A80 Series","0～100%LEL/0～20000ppm"]
["Propylene","C3H6","115-07-1","C3H6","HW","HW-6239/NC-6239","Fixed","GD-D58(TYPE GP) Series","0～100%LEL/0～20000ppm"]
["Propylene","C3H6","115-07-1","C3H6","HW","HW-6239/NC-6239","Fixed","GD-D58(TYPE NC) Series","0～100%LEL/0～20000ppm"]
["Propylene","C3H6","115-07-1","C3H6","HW","HW-6239/NC-6239","Fixed","SD-1(TYPE NC) Series","0～100%LEL/0～20000ppm"]
["Propylene","C3H6","115-07-1","C3H6","HW","HW-6239/NC-6239","Fixed","SD-D58(TYPE NC) Series","0～100%LEL/0～20000ppm"]
["Propylene","C3H6","115-07-1","C3H6","SG","SG-8511","Fixed","GD-A80V Series","0～2000ppm/0～3000ppm/0～5000ppm/0～100%LEL"]
["Propylene","C3H6","115-07-1","C3H6","SG","SG-8511","Fixed","GD-D58・GH Series","0～2000ppm/0～3000ppm/0～5000ppm/0～100%LEL"]
["Propylene","C3H6","115-07-1","C3H6","SG","SG-8511","Fixed","SD-1GH Series","0～2000ppm/0～3000ppm/0～5000ppm/0～100%LEL"]
["Propylene","C3H6","115-07-1","C3H6","SG","SG-8511","Fixed","SD-D58・GH Series","0～2000ppm/0～3000ppm/0～5000ppm/0～100%LEL"]
["Propylene","C3H6","115-07-1","C3H6","SG","SG-8521","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Propylene","C3H6","115-07-1","C3H6","SG","SG-8521","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Propylene","C3H6","115-07-1","C3H6","SG","SG-8521","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Propylene","C3H6","115-07-1","C3H6","SG","SG-8521","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Propylene carbonate","PC","108-32-7","C4H6O3","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Propylene carbonate","PC","108-32-7","C4H6O3","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Propylene carbonate","PC","108-32-7","C4H6O3","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Propylene carbonate","PC","108-32-7","C4H6O3","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Propylene carbonate","PC","108-32-7","C4H6O3","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Propylene carbonate","PC","108-32-7","C4H6O3","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Propylene carbonate","PC","108-32-7","C4H6O3","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Propylene Glycol","PGLY","57-55-6","C3H8O2","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Propylene Glycol","PGLY","57-55-6","C3H8O2","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Propylene Glycol","PGLY","57-55-6","C3H8O2","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Propylene Glycol","PGLY","57-55-6","C3H8O2","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Propylene Glycol","PGLY","57-55-6","C3H8O2","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Propylene Glycol","PGLY","57-55-6","C3H8O2","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Propylene Glycol","PGLY","57-55-6","C3H8O2","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Propylene Glycol","PGLY","57-55-6","C3H8O2","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["Propylene Glycol","PGLY","57-55-6","C3H8O2","SG","SG-8521","Fixed","GD-A80V Series","0～200ppm"]
["Propylene Glycol","PGLY","57-55-6","C3H8O2","SG","SG-8521","Fixed","GD-D58・GH Series","0～200ppm"]
["Propylene Glycol","PGLY","57-55-6","C3H8O2","SG","SG-8521","Fixed","SD-1GH Series","0～200ppm"]
["Propylene Glycol","PGLY","57-55-6","C3H8O2","SG","SG-8521","Fixed","SD-D58・GH Series","0～200ppm"]
["Propylene Glycol Butyl Ether ","C7H16O2","29387-86-8","C7H16O2","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Propylene Glycol Butyl Ether ","C7H16O2","29387-86-8","C7H16O2","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Propylene Glycol Butyl Ether ","C7H16O2","29387-86-8","C7H16O2","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Propylene Glycol Butyl Ether ","C7H16O2","29387-86-8","C7H16O2","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Propylene Glycol Butyl Ether ","C7H16O2","29387-86-8","C7H16O2","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Propylene Glycol Butyl Ether ","C7H16O2","29387-86-8","C7H16O2","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Propylene Glycol Butyl Ether ","C7H16O2","29387-86-8","C7H16O2","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Propylene Glycol Butyl Ether ","C7H16O2","29387-86-8","C7H16O2","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["Propylene Glycol Butyl Ether ","C7H16O2","29387-86-8","C7H16O2","SG","SG-8521","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Propylene Glycol Butyl Ether ","C7H16O2","29387-86-8","C7H16O2","SG","SG-8521","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Propylene Glycol Butyl Ether ","C7H16O2","29387-86-8","C7H16O2","SG","SG-8521","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Propylene Glycol Butyl Ether ","C7H16O2","29387-86-8","C7H16O2","SG","SG-8521","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Propylene Glycol Monoethyl Ether","PGMEE","1569-02-4","C5H12O2","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Propylene Glycol Monoethyl Ether","PGMEE","1569-02-4","C5H12O2","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Propylene Glycol Monoethyl Ether","PGMEE","1569-02-4","C5H12O2","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～13000ppm"]
["Propylene Glycol Monoethyl Ether","PGMEE","1569-02-4","C5H12O2","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～13000ppm"]
["Propylene Glycol Monoethyl Ether","PGMEE","1569-02-4","C5H12O2","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～13000ppm"]
["Propylene Glycol Monoethyl Ether","PGMEE","1569-02-4","C5H12O2","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～13000ppm"]
["Propylene Glycol Monoethyl Ether","PGMEE","1569-02-4","C5H12O2","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～13000ppm"]
["Propylene Glycol Monoethyl Ether","PGMEE","1569-02-4","C5H12O2","SG","SG-8521","Fixed","GD-A80V Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Propylene Glycol Monoethyl Ether","PGMEE","1569-02-4","C5H12O2","SG","SG-8521","Fixed","GD-D58・GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Propylene Glycol Monoethyl Ether","PGMEE","1569-02-4","C5H12O2","SG","SG-8521","Fixed","SD-1GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Propylene Glycol Monoethyl Ether","PGMEE","1569-02-4","C5H12O2","SG","SG-8521","Fixed","SD-D58・GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Propylene Glycol Monomethyl Ether ","PGMME","107-98-2","C4H10O2","SG","SGU-8511","Fixed","GD-70D Series","0～2000ppm"]
["Propylene Glycol Monomethyl Ether ","PGMME","107-98-2","C4H10O2","SG","SGU-8511","Fixed","TP-70D","0～2000ppm"]
["Propylene Glycol Monomethyl Ether ","PGMME","107-98-2","C4H10O2","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Propylene Glycol Monomethyl Ether ","PGMME","107-98-2","C4H10O2","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Propylene Glycol Monomethyl Ether ","PGMME","107-98-2","C4H10O2","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～16000ppm"]
["Propylene Glycol Monomethyl Ether ","PGMME","107-98-2","C4H10O2","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～16000ppm"]
["Propylene Glycol Monomethyl Ether ","PGMME","107-98-2","C4H10O2","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～16000ppm"]
["Propylene Glycol Monomethyl Ether ","PGMME","107-98-2","C4H10O2","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～16000ppm"]
["Propylene Glycol Monomethyl Ether ","PGMME","107-98-2","C4H10O2","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～16000ppm"]
["Propylene Glycol Monomethyl Ether ","PGMME","107-98-2","C4H10O2","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Propylene Glycol Monomethyl Ether ","PGMME","107-98-2","C4H10O2","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Propylene Glycol Monomethyl Ether ","PGMME","107-98-2","C4H10O2","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Propylene Glycol Monomethyl Ether ","PGMME","107-98-2","C4H10O2","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Propylene Glycol Monomethyl Ether ","PGMME","107-98-2","C4H10O2","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Propylene Glycol Monomethyl Ether ","PGMME","107-98-2","C4H10O2","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Propylene Glycol Monomethyl Ether ","PGMME","107-98-2","C4H10O2","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Propylene Glycol Monomethyl Ether ","PGMME","107-98-2","C4H10O2","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["Propylene Glycol Monomethyl Ether ","PGMME","107-98-2","C4H10O2","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Propylene Glycol Monomethyl Ether ","PGMME","107-98-2","C4H10O2","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Propylene Glycol Monomethyl Ether ","PGMME","107-98-2","C4H10O2","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Propylene Glycol Monomethyl Ether ","PGMME","107-98-2","C4H10O2","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Propylene Glycol Monomethyl Ether ","PGMME","107-98-2","C4H10O2","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Propylene Glycol Monomethyl Ether ","PGMME","107-98-2","C4H10O2","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Propylene Glycol Monomethyl Ether ","PGMME","107-98-2","C4H10O2","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Propylene Glycol Monomethyl Ether ","PGMME","107-98-2","C4H10O2","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["Propylene Glycol Monomethyl Ether ","PGMME","107-98-2","C4H10O2","SG","SG-8511","Fixed","GD-A80V Series","0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Propylene Glycol Monomethyl Ether ","PGMME","107-98-2","C4H10O2","SG","SG-8511","Fixed","GD-D58・GH Series","0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Propylene Glycol Monomethyl Ether ","PGMME","107-98-2","C4H10O2","SG","SG-8511","Fixed","SD-1GH Series","0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Propylene Glycol Monomethyl Ether ","PGMME","107-98-2","C4H10O2","SG","SG-8511","Fixed","SD-D58・GH Series","0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Propylene Glycol Monomethyl Ether ","PGMME","107-98-2","C4H10O2","SG","SG-8521","Fixed","GD-A80V Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["Propylene Glycol Monomethyl Ether ","PGMME","107-98-2","C4H10O2","SG","SG-8521","Fixed","GD-D58・GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["Propylene Glycol Monomethyl Ether ","PGMME","107-98-2","C4H10O2","SG","SG-8521","Fixed","SD-1GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["Propylene Glycol Monomethyl Ether ","PGMME","107-98-2","C4H10O2","SG","SG-8521","Fixed","SD-D58・GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["Propylene Glycol Monomethyl Ether Acetate","PGMMEAc","108-65-6","C6H12O3","SG","SGU-8521","Fixed","GD-70D Series","0～2000ppm"]
["Propylene Glycol Monomethyl Ether Acetate","PGMMEAc","108-65-6","C6H12O3","SG","SGU-8521","Fixed","TP-70D","0～2000ppm"]
["Propylene Glycol Monomethyl Ether Acetate","PGMMEAc","108-65-6","C6H12O3","RI","DE-3315-2","Fixed","SD-1RI Series","0～100%LEL"]
["Propylene Glycol Monomethyl Ether Acetate","PGMMEAc","108-65-6","C6H12O3","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Propylene Glycol Monomethyl Ether Acetate","PGMMEAc","108-65-6","C6H12O3","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Propylene Glycol Monomethyl Ether Acetate","PGMMEAc","108-65-6","C6H12O3","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～15000ppm"]
["Propylene Glycol Monomethyl Ether Acetate","PGMMEAc","108-65-6","C6H12O3","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～15000ppm"]
["Propylene Glycol Monomethyl Ether Acetate","PGMMEAc","108-65-6","C6H12O3","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～15000ppm"]
["Propylene Glycol Monomethyl Ether Acetate","PGMMEAc","108-65-6","C6H12O3","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～15000ppm"]
["Propylene Glycol Monomethyl Ether Acetate","PGMMEAc","108-65-6","C6H12O3","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～15000ppm"]
["Propylene Glycol Monomethyl Ether Acetate","PGMMEAc","108-65-6","C6H12O3","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Propylene Glycol Monomethyl Ether Acetate","PGMMEAc","108-65-6","C6H12O3","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Propylene Glycol Monomethyl Ether Acetate","PGMMEAc","108-65-6","C6H12O3","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Propylene Glycol Monomethyl Ether Acetate","PGMMEAc","108-65-6","C6H12O3","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Propylene Glycol Monomethyl Ether Acetate","PGMMEAc","108-65-6","C6H12O3","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Propylene Glycol Monomethyl Ether Acetate","PGMMEAc","108-65-6","C6H12O3","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Propylene Glycol Monomethyl Ether Acetate","PGMMEAc","108-65-6","C6H12O3","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Propylene Glycol Monomethyl Ether Acetate","PGMMEAc","108-65-6","C6H12O3","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["Propylene Glycol Monomethyl Ether Acetate","PGMMEAc","108-65-6","C6H12O3","SG","SG-8521","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Propylene Glycol Monomethyl Ether Acetate","PGMMEAc","108-65-6","C6H12O3","SG","SG-8521","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Propylene Glycol Monomethyl Ether Acetate","PGMMEAc","108-65-6","C6H12O3","SG","SG-8521","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Propylene Glycol Monomethyl Ether Acetate","PGMMEAc","108-65-6","C6H12O3","SG","SG-8521","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Propylene oxide","PO","75-56-9","C3H6O","HW","NC-6215","Portable","GP-1000(Specified cal.gas)","0～100%LEL"]
["Propylene oxide","PO","75-56-9","C3H6O","RI","DE-3315-2","Fixed","SD-1RI Series","0～100%LEL"]
["Propylene oxide","PO","75-56-9","C3H6O","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Propylene oxide","PO","75-56-9","C3H6O","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Propylene oxide","PO","75-56-9","C3H6O","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～28000ppm"]
["Propylene oxide","PO","75-56-9","C3H6O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～28000ppm"]
["Propylene oxide","PO","75-56-9","C3H6O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～28000ppm"]
["Propylene oxide","PO","75-56-9","C3H6O","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～28000ppm"]
["Propylene oxide","PO","75-56-9","C3H6O","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～28000ppm"]
["Propylene oxide","PO","75-56-9","C3H6O","HW","NC-6240A","Fixed","GD-A80 Series","0～100%LEL/0～28000ppm"]
["Propylene oxide","PO","75-56-9","C3H6O","HW","NC-6240A","Fixed","GD-D58(TYPE NC) Series","0～100%LEL/0～28000ppm"]
["Propylene oxide","PO","75-56-9","C3H6O","HW","NC-6240A","Fixed","SD-1(TYPE NC) Series","0～100%LEL/0～28000ppm"]
["Propylene oxide","PO","75-56-9","C3H6O","HW","NC-6240A","Fixed","SD-D58(TYPE NC) Series","0～100%LEL/0～28000ppm"]
["Propylene oxide","PO","75-56-9","C3H6O","HW","NC-6245","Fixed","GD-A80 Series","0～100%LEL"]
["Propylene oxide","PO","75-56-9","C3H6O","HW","NC-6245","Fixed","GD-D58(TYPE NC) Series","0～100%LEL"]
["Propylene oxide","PO","75-56-9","C3H6O","HW","NC-6245","Fixed","SD-1(TYPE NC) Series","0～100%LEL"]
["Propylene oxide","PO","75-56-9","C3H6O","HW","NC-6245","Fixed","SD-D58(TYPE NC) Series","0～100%LEL"]
["Propylene oxide","PO","75-56-9","C3H6O","SG","SG-8511","Fixed","GD-A80V Series","0～2000ppm/0～3000ppm/0～5000ppm/0～10000ppm/0～20000ppm/0～50%LEL/0～100%LEL"]
["Propylene oxide","PO","75-56-9","C3H6O","SG","SG-8511","Fixed","GD-D58・GH Series","0～2000ppm/0～3000ppm/0～5000ppm/0～10000ppm/0～20000ppm/0～50%LEL/0～100%LEL"]
["Propylene oxide","PO","75-56-9","C3H6O","SG","SG-8511","Fixed","SD-1GH Series","0～2000ppm/0～3000ppm/0～5000ppm/0～10000ppm/0～20000ppm/0～50%LEL/0～100%LEL"]
["Propylene oxide","PO","75-56-9","C3H6O","SG","SG-8511","Fixed","SD-D58・GH Series","0～2000ppm/0～3000ppm/0～5000ppm/0～10000ppm/0～20000ppm/0～50%LEL/0～100%LEL"]
["Propylene oxide","PO","75-56-9","C3H6O","SG","SG-8521","Fixed","GD-A80V Series","0～180ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Propylene oxide","PO","75-56-9","C3H6O","SG","SG-8521","Fixed","GD-D58・GH Series","0～180ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Propylene oxide","PO","75-56-9","C3H6O","SG","SG-8521","Fixed","SD-1GH Series","0～180ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Propylene oxide","PO","75-56-9","C3H6O","SG","SG-8521","Fixed","SD-D58・GH Series","0～180ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Propylene oxide","PO","75-56-9","C3H6O","SG","SG-8521","Fixed","GD-A80V Series","0～100ppm/0～200ppm"]
["Propylene oxide","PO","75-56-9","C3H6O","SG","SG-8521","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm"]
["Propylene oxide","PO","75-56-9","C3H6O","SG","SG-8521","Fixed","SD-1GH Series","0～100ppm/0～200ppm"]
["Propylene oxide","PO","75-56-9","C3H6O","SG","SG-8521","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm"]
["Propylene oxide","PO","75-56-9","C3H6O","SG","SG-8563","Fixed","GD-A80V Series","0～10ppm/0～20ppm/0～30ppm/0～50ppm/0～100ppm/0～150ppm/0～200ppm"]
["Propylene oxide","PO","75-56-9","C3H6O","SG","SG-8563","Fixed","GD-D58・GH Series","0～10ppm/0～20ppm/0～30ppm/0～50ppm/0～100ppm/0～150ppm/0～200ppm"]
["Propylene oxide","PO","75-56-9","C3H6O","SG","SG-8563","Fixed","SD-1GH Series","0～10ppm/0～20ppm/0～30ppm/0～50ppm/0～100ppm/0～150ppm/0～200ppm"]
["Propylene oxide","PO","75-56-9","C3H6O","SG","SG-8563","Fixed","SD-D58・GH Series","0～10ppm/0～20ppm/0～30ppm/0～50ppm/0～100ppm/0～150ppm/0～200ppm"]
["Pyridine","C5H5N","110-86-1","C5H5N","SG","SGU-8521","Fixed","GD-70D Series","0～50ppm"]
["Pyridine","C5H5N","110-86-1","C5H5N","SG","SGU-8521","Fixed","TP-70D","0～50ppm"]
["Pyridine","C5H5N","110-86-1","C5H5N","SG","SGU-8521","Fixed","GD-70D Series","0～500ppm"]
["Pyridine","C5H5N","110-86-1","C5H5N","SG","SGU-8521","Fixed","TP-70D","0～500ppm"]
["Pyridine","C5H5N","110-86-1","C5H5N","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Pyridine","C5H5N","110-86-1","C5H5N","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Pyridine","C5H5N","110-86-1","C5H5N","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～18000ppm"]
["Pyridine","C5H5N","110-86-1","C5H5N","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～18000ppm"]
["Pyridine","C5H5N","110-86-1","C5H5N","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～18000ppm"]
["Pyridine","C5H5N","110-86-1","C5H5N","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～18000ppm"]
["Pyridine","C5H5N","110-86-1","C5H5N","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～18000ppm"]
["Pyridine","C5H5N","110-86-1","C5H5N","SG","SG-8521","Fixed","GD-A80V Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["Pyridine","C5H5N","110-86-1","C5H5N","SG","SG-8521","Fixed","GD-D58・GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["Pyridine","C5H5N","110-86-1","C5H5N","SG","SG-8521","Fixed","SD-1GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["Pyridine","C5H5N","110-86-1","C5H5N","SG","SG-8521","Fixed","SD-D58・GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["R-113E","R-113E","-","-","SG","SG-8513","Fixed","GD-A80V Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["R-113E","R-113E","-","-","SG","SG-8513","Fixed","GD-D58・GH Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["R-113E","R-113E","-","-","SG","SG-8513","Fixed","SD-1GH Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["R-113E","R-113E","-","-","SG","SG-8513","Fixed","SD-D58・GH Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["R-318","R-318","-","C4F8CL2","RI","DE-2113-35","Fixed","RI-257","0～2vol%"]
["R-404A","R-404A","-","-","SH","SH-8662","Portable","SP-220(TYPE SC)","0～50ppm"]
["R-404A","R-404A","-","-","SH","SH-8661","Portable","SP-220(TYPE F)","0～5000ppm"]
["R-404A","R-404A","-","-","RI","DE-2113-35","Fixed","RI-257","0～5000ppm"]
["R-404A","R-404A","-","-","SG","SG-8521","Fixed","GD-A80V Series","0～2000ppm/0～3000ppm/0～5000ppm"]
["R-404A","R-404A","-","-","SG","SG-8521","Fixed","GD-D58・GH Series","0～2000ppm/0～3000ppm/0～5000ppm"]
["R-404A","R-404A","-","-","SG","SG-8521","Fixed","SD-1GH Series","0～2000ppm/0～3000ppm/0～5000ppm"]
["R-404A","R-404A","-","-","SG","SG-8521","Fixed","SD-D58・GH Series","0～2000ppm/0～3000ppm/0～5000ppm"]
["R-407A","R-407A","-","-","SH","SH-8661","Portable","SP-220(TYPE F)","0～5000ppm"]
["R-407C","R-407C","-","-","SH","SH-8662","Portable","SP-220(TYPE SC)","0～50ppm"]
["R-407C","R-407C","-","-","SH","SH-8661","Portable","SP-220(TYPE F)","0～10000ppm"]
["R-407C","R-407C","-","-","RI","DE-2113-35","Fixed","RI-257","0～5000ppm"]
["R-407C","R-407C","-","-","SG","SG-8521","Fixed","GD-A80V Series","0～2000ppm/0～3000ppm/0～5000ppm"]
["R-407C","R-407C","-","-","SG","SG-8521","Fixed","GD-D58・GH Series","0～2000ppm/0～3000ppm/0～5000ppm"]
["R-407C","R-407C","-","-","SG","SG-8521","Fixed","SD-1GH Series","0～2000ppm/0～3000ppm/0～5000ppm"]
["R-407C","R-407C","-","-","SG","SG-8521","Fixed","SD-D58・GH Series","0～2000ppm/0～3000ppm/0～5000ppm"]
["R-407E","R-407E","-","-","SG","SGU-8521","Fixed","GD-70D Series","0～5000ppm"]
["R-407E","R-407E","-","-","SG","SGU-8521","Fixed","TP-70D","0～5000ppm"]
["R-407E","R-407E","-","-","SG","SG-8521","Fixed","GD-A80V Series","0～2000ppm/0～3000ppm/0～5000ppm"]
["R-407E","R-407E","-","-","SG","SG-8521","Fixed","GD-D58・GH Series","0～2000ppm/0～3000ppm/0～5000ppm"]
["R-407E","R-407E","-","-","SG","SG-8521","Fixed","SD-1GH Series","0～2000ppm/0～3000ppm/0～5000ppm"]
["R-407E","R-407E","-","-","SG","SG-8521","Fixed","SD-D58・GH Series","0～2000ppm/0～3000ppm/0～5000ppm"]
["R-410A","R-410A","-","-","SH","SH-8662","Portable","SP-220(TYPE SC)","0～50ppm"]
["R-410A","R-410A","-","-","SH","SH-8661","Portable","SP-220(TYPE F)","0～10000ppm"]
["R-410A","R-410A","-","-","SG","SGU-8521","Fixed","GD-70D Series","0～5000ppm"]
["R-410A","R-410A","-","-","SG","SGU-8521","Fixed","TP-70D","0～5000ppm"]
["R-410A","R-410A","-","-","RI","DE-2113-35","Fixed","RI-257","0～5000ppm"]
["R-410A","R-410A","-","-","SG","SG-8521","Fixed","GD-A80V Series","0～5000ppm"]
["R-410A","R-410A","-","-","SG","SG-8521","Fixed","GD-D58・GH Series","0～5000ppm"]
["R-410A","R-410A","-","-","SG","SG-8521","Fixed","SD-1GH Series","0～5000ppm"]
["R-410A","R-410A","-","-","SG","SG-8521","Fixed","SD-D58・GH Series","0～5000ppm"]
["R-417A","R-417A","-","-","SG","SG-8521","Fixed","GD-A80V Series","0～20000ppm/0～30000ppm/0～50000ppm"]
["R-417A","R-417A","-","-","SG","SG-8521","Fixed","GD-D58・GH Series","0～20000ppm/0～30000ppm/0～50000ppm"]
["R-417A","R-417A","-","-","SG","SG-8521","Fixed","SD-1GH Series","0～20000ppm/0～30000ppm/0～50000ppm"]
["R-417A","R-417A","-","-","SG","SG-8521","Fixed","SD-D58・GH Series","0～20000ppm/0～30000ppm/0～50000ppm"]
["R-422A","R-422A","-","-","SG","SG-8521","Fixed","GD-A80V Series","0～30000ppm/0～50000ppm"]
["R-422A","R-422A","-","-","SG","SG-8521","Fixed","GD-D58・GH Series","0～30000ppm/0～50000ppm"]
["R-422A","R-422A","-","-","SG","SG-8521","Fixed","SD-1GH Series","0～30000ppm/0～50000ppm"]
["R-422A","R-422A","-","-","SG","SG-8521","Fixed","SD-D58・GH Series","0～30000ppm/0～50000ppm"]
["R-454C","R-454C","-","-","SG","SG-8511","Fixed","GD-A80V Series","0～3000ppm/0～5000ppm/0～10000ppm/0～20000ppm"]
["R-454C","R-454C","-","-","SG","SG-8511","Fixed","GD-D58・GH Series","0～3000ppm/0～5000ppm/0～10000ppm/0～20000ppm"]
["R-454C","R-454C","-","-","SG","SG-8511","Fixed","SD-1GH Series","0～3000ppm/0～5000ppm/0～10000ppm/0～20000ppm"]
["R-454C","R-454C","-","-","SG","SG-8511","Fixed","SD-D58・GH Series","0～3000ppm/0～5000ppm/0～10000ppm/0～20000ppm"]
["R-454C","R-454C","-","-","SG","SG-8521","Fixed","GD-A80V Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["R-454C","R-454C","-","-","SG","SG-8521","Fixed","GD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["R-454C","R-454C","-","-","SG","SG-8521","Fixed","SD-1GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["R-454C","R-454C","-","-","SG","SG-8521","Fixed","SD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["R-502","R-502","-","-","RI","DE-2113-35","Fixed","RI-257","0～5000ppm"]
["R-502","R-502","-","-","SG","SG-8513","Fixed","GD-A80V Series","0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm/0～10000ppm"]
["R-502","R-502","-","-","SG","SG-8513","Fixed","GD-D58・GH Series","0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm/0～10000ppm"]
["R-502","R-502","-","-","SG","SG-8513","Fixed","SD-1GH Series","0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm/0～10000ppm"]
["R-502","R-502","-","-","SG","SG-8513","Fixed","SD-D58・GH Series","0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm/0～10000ppm"]
["R-507A","R-507A","-","-","SH","SH-8661","Portable","SP-220(TYPE F)","0～2000ppm"]
["R-507A","R-507A","-","-","SG","SG-8562","Fixed","GD-A80V Series","0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["R-507A","R-507A","-","-","SG","SG-8562","Fixed","GD-D58・GH Series","0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["R-507A","R-507A","-","-","SG","SG-8562","Fixed","SD-1GH Series","0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["R-507A","R-507A","-","-","SG","SG-8562","Fixed","SD-D58・GH Series","0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Silane","SiH4","7803-62-5","SiH4","SH","SH-8662","Portable","SP-220(TYPE SC)","0～0.5ppm"]
["Silane","SiH4","7803-62-5","SiH4","ES","ESM-23DH","Portable","SC-8000","0～15ppm"]
["Silane","SiH4","7803-62-5","SiH4","ES","ESU-23DH","Fixed","GD-70D Series","0～15ppm"]
["Silane","SiH4","7803-62-5","SiH4","ES","ESU-23DH","Fixed","TP-70D","0～15ppm"]
["Silane","SiH4","7803-62-5","SiH4","ES","ESU-23AH","Fixed","GD-70D Series","0～15ppm"]
["Silane","SiH4","7803-62-5","SiH4","ES","ESU-23AH","Fixed","TP-70D","0～15ppm"]
["Silane","SiH4","7803-62-5","SiH4","ES","ESM-23AH","Fixed","GD-K88Ai Series","0～15ppm"]
["Silane","SiH4","7803-62-5","SiH4","ES","ESM-23AH","Fixed","GD-K88Di Series","0～15ppm"]
["Silane","SiH4","7803-62-5","SiH4","ES","ESM-23AH-S","Fixed","GD-K88Ai Series","0～15ppm"]
["Silane","SiH4","7803-62-5","SiH4","ES","ESM-23AH-S","Fixed","GD-K88Di Series","0～15ppm"]
["Silane","SiH4","7803-62-5","SiH4","ES","ESM-23DH","Fixed","GD-K88Ai Series","0～15ppm"]
["Silane","SiH4","7803-62-5","SiH4","ES","ESM-23DH","Fixed","GD-K88Di Series","0～15ppm"]
["Silicon Dioxide","SiO2","7631-86-9","SiO2","SS","SSU-1925","Fixed","GD-70D Series","0～10mg/m3","Only show if gas is existing or not(No concentratuion displayed)/Unavailable with dust filter "]
["Styrene","C8H8","100-42-5","C8H8","HW","NC-6307","Portable","NC-1000(Specified cal. Gas)","0～10000ppm"]
["Styrene","C8H8","100-42-5","C8H8","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Styrene","C8H8","100-42-5","C8H8","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Styrene","C8H8","100-42-5","C8H8","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～11000ppm"]
["Styrene","C8H8","100-42-5","C8H8","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～11000ppm"]
["Styrene","C8H8","100-42-5","C8H8","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～11000ppm"]
["Styrene","C8H8","100-42-5","C8H8","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～11000ppm"]
["Styrene","C8H8","100-42-5","C8H8","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～11000ppm"]
["Styrene","C8H8","100-42-5","C8H8","HW","HW-6213/NC-6213","Fixed","GD-A80 Series","0～100%LEL/0～11000ppm"]
["Styrene","C8H8","100-42-5","C8H8","HW","HW-6213/NC-6213","Fixed","GD-D58(TYPE GP) Series","0～100%LEL/0～11000ppm"]
["Styrene","C8H8","100-42-5","C8H8","HW","HW-6213/NC-6213","Fixed","GD-D58(TYPE NC) Series","0～100%LEL/0～11000ppm"]
["Styrene","C8H8","100-42-5","C8H8","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Styrene","C8H8","100-42-5","C8H8","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Styrene","C8H8","100-42-5","C8H8","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Styrene","C8H8","100-42-5","C8H8","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Styrene","C8H8","100-42-5","C8H8","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Styrene","C8H8","100-42-5","C8H8","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Styrene","C8H8","100-42-5","C8H8","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Styrene","C8H8","100-42-5","C8H8","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["Styrene","C8H8","100-42-5","C8H8","SG","SG-8521","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Styrene","C8H8","100-42-5","C8H8","SG","SG-8521","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Styrene","C8H8","100-42-5","C8H8","SG","SG-8521","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Styrene","C8H8","100-42-5","C8H8","SG","SG-8521","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Sulfur dioxide","SO2","7446-09-5","SO2","ES","ES-1828","Portable","GX-2009","0～20ppm"]
["Sulfur dioxide","SO2","7446-09-5","SO2","SH","SH-8662","Portable","SP-220(TYPE SC)","0～1ppm"]
["Sulfur dioxide","SO2","7446-09-5","SO2","ES","ESS-03DH","Portable","GX-6000","0～99.9ppm"]
["Sulfur dioxide","SO2","7446-09-5","SO2","ES","ESM-01DH-D","Portable","SC-01","0～6ppm"]
["Sulfur dioxide","SO2","7446-09-5","SO2","ES","ESM-238","Portable","SC-8000","0～6ppm"]
["Sulfur dioxide","SO2","7446-09-5","SO2","ES","ESM-238","Portable","SC-8000","0～30ppm"]
["Sulfur dioxide","SO2","7446-09-5","SO2","ES","ESU-238","Fixed","GD-70D Series","0～6ppm"]
["Sulfur dioxide","SO2","7446-09-5","SO2","ES","ESU-238","Fixed","TP-70D","0～6ppm"]
["Sulfur dioxide","SO2","7446-09-5","SO2","ES","ESM-238","Fixed","GD-K88Ai Series","0～6ppm"]
["Sulfur dioxide","SO2","7446-09-5","SO2","ES","ESM-238","Fixed","GD-K88Di Series","0～6ppm"]
["Sulfur dioxide","SO2","7446-09-5","SO2","ES","ESM-238","Fixed","GD-K88Ai Series","0～30ppm"]
["Sulfur dioxide","SO2","7446-09-5","SO2","ES","ESM-238","Fixed","GD-K88Di Series","0～30ppm"]
["Sulfur dioxide","SO2","7446-09-5","SO2","ES","ESM-23E","Fixed","GD-K88Ai Series","0～30ppm"]
["Sulfur dioxide","SO2","7446-09-5","SO2","ES","ESM-23E","Fixed","GD-K88Di Series","0～30ppm"]
["Sulfur dioxide","SO2","7446-09-5","SO2","SG","SG-8511","Fixed","GD-A80V Series","0～500ppm"]
["Sulfur dioxide","SO2","7446-09-5","SO2","SG","SG-8511","Fixed","GD-D58・GH Series","0～500ppm"]
["Sulfur dioxide","SO2","7446-09-5","SO2","SG","SG-8511","Fixed","SD-1GH Series","0～500ppm"]
["Sulfur dioxide","SO2","7446-09-5","SO2","SG","SG-8511","Fixed","SD-D58・GH Series","0～500ppm"]
["Sulfuryl fluoride","SO2F2","2699-79-8","SO2F2","SH","SH-8662","Portable","SP-220(TYPE FUM)","0～800ppm"]
["tert-Butanol","TBA","75-65-0","C4H10O","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["tert-Butanol","TBA","75-65-0","C4H10O","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["tert-Butanol","TBA","75-65-0","C4H10O","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～19000ppm"]
["tert-Butanol","TBA","75-65-0","C4H10O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～19000ppm"]
["tert-Butanol","TBA","75-65-0","C4H10O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～19000ppm"]
["tert-Butanol","TBA","75-65-0","C4H10O","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～19000ppm"]
["tert-Butanol","TBA","75-65-0","C4H10O","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～19000ppm"]
["tert-Butanol","TBA","75-65-0","C4H10O","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["tert-Butanol","TBA","75-65-0","C4H10O","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["tert-Butanol","TBA","75-65-0","C4H10O","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["tert-Butanol","TBA","75-65-0","C4H10O","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["tert-Butanol","TBA","75-65-0","C4H10O","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["tert-Butanol","TBA","75-65-0","C4H10O","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["tert-Butanol","TBA","75-65-0","C4H10O","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["tert-Butanol","TBA","75-65-0","C4H10O","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["tert-Butanol","TBA","75-65-0","C4H10O","SG","SG-8511","Fixed","GD-A80V Series","0～2000ppm/0～3000ppm/0～5000ppm"]
["tert-Butanol","TBA","75-65-0","C4H10O","SG","SG-8511","Fixed","GD-D58・GH Series","0～2000ppm/0～3000ppm/0～5000ppm"]
["tert-Butanol","TBA","75-65-0","C4H10O","SG","SG-8511","Fixed","SD-1GH Series","0～2000ppm/0～3000ppm/0～5000ppm"]
["tert-Butanol","TBA","75-65-0","C4H10O","SG","SG-8511","Fixed","SD-D58・GH Series","0～2000ppm/0～3000ppm/0～5000ppm"]
["tert-Butanol","TBA","75-65-0","C4H10O","SG","SG-8521","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["tert-Butanol","TBA","75-65-0","C4H10O","SG","SG-8521","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["tert-Butanol","TBA","75-65-0","C4H10O","SG","SG-8521","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["tert-Butanol","TBA","75-65-0","C4H10O","SG","SG-8521","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["tert-Butyl Mercaptan","TBM","75-66-1","C4H10S","SG","SG-8564","Fixed","GD-A80V Series","0～10ppm/0～20ppm/0～30ppm/0～50ppm"]
["tert-Butyl Mercaptan","TBM","75-66-1","C4H10S","SG","SG-8564","Fixed","GD-D58・GH Series","0～10ppm/0～20ppm/0～30ppm/0～50ppm"]
["tert-Butyl Mercaptan","TBM","75-66-1","C4H10S","SG","SG-8564","Fixed","SD-1GH Series","0～10ppm/0～20ppm/0～30ppm/0～50ppm"]
["tert-Butyl Mercaptan","TBM","75-66-1","C4H10S","SG","SG-8564","Fixed","SD-D58・GH Series","0～10ppm/0～20ppm/0～30ppm/0～50ppm"]
["Tetrachloroethylene","C2CL4","127-18-4","C2CL4","SG","SG-8523","Fixed","GD-A80V Series","★0～300ppm/★0～500ppm/★0～1000ppm/★0～2000ppm/★0～3000ppm/★0～5000ppm","★Range easily affected by environmental conditions and other"]
["Tetrachloroethylene","C2CL4","127-18-4","C2CL4","SG","SG-8523","Fixed","GD-D58・GH Series","★0～300ppm/★0～500ppm/★0～1000ppm/★0～2000ppm/★0～3000ppm/★0～5000ppm","★Range easily affected by environmental conditions and other"]
["Tetrachloroethylene","C2CL4","127-18-4","C2CL4","SG","SG-8523","Fixed","SD-1GH Series","★0～300ppm/★0～500ppm/★0～1000ppm/★0～2000ppm/★0～3000ppm/★0～5000ppm","★Range easily affected by environmental conditions and other"]
["Tetrachloroethylene","C2CL4","127-18-4","C2CL4","SG","SG-8523","Fixed","SD-D58・GH Series","★0～300ppm/★0～500ppm/★0～1000ppm/★0～2000ppm/★0～3000ppm/★0～5000ppm","★Range easily affected by environmental conditions and other"]
["Tetradecane","C14H30","629-59-4","C14H30","HW","HW-6206","Fixed","SD-2500/SD-2600/SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Tetradecane","C14H30","629-59-4","C14H30","HW","HW-6206","Fixed","SD-2500/SD-2600/SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Tetradecane","C14H30","629-59-4","C14H30","HW","HW-6206","Fixed","SD-2500/SD-2600/SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Tetradecane","C14H30","629-59-4","C14H30","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Tetradecane","C14H30","629-59-4","C14H30","HW","HW-6208","Fixed","SD-2500/SD-2600/SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Tetradecane","C14H30","629-59-4","C14H30","HW","HW-6208","Fixed","SD-2500/SD-2600/SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Tetradecane","C14H30","629-59-4","C14H30","HW","HW-6208","Fixed","SD-2500/SD-2600/SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Tetraethoxysilane","TEOS","78-10-4","C8H20O4Si","ES","ESU-23","Fixed","GD-70D Series","0～15ppm","SS sensor recommended/Can be used as a substitute of SS sensor"]
["Tetraethoxysilane","TEOS","78-10-4","C8H20O4Si","ES","ESU-23","Fixed","TP-70D","0～15ppm","SS sensor recommended/Can be used as a substitute of SS sensor"]
["Tetraethoxysilane","TEOS","78-10-4","C8H20O4Si","SS","SSU-1925","Fixed","GD-70D+PLU Series","0‐15ppm","PLU-70 required"]
["Tetraethoxysilane","TEOS","78-10-4","C8H20O4Si","SS","SSU-1925","Fixed","GD-70DG","0‐15ppm","PLU-70 required"]
["Tetraethoxysilane","TEOS","78-10-4","C8H20O4Si","SS","SSU-1927","Fixed","GD-70D+PLU Series","0‐15ppm","PLU-70 required"]
["Tetraethoxysilane","TEOS","78-10-4","C8H20O4Si","SS","SSU-1927","Fixed","GD-70DG","0‐15ppm","PLU-70 required"]
["Tetrafluoroethylene","C2F4","116-14-3","C2F4","SG","SGU-8521","Fixed","GD-70D Series","0～1000ppm"]
["Tetrafluoroethylene","C2F4","116-14-3","C2F4","SG","SGU-8521","Fixed","TP-70D","0～1000ppm"]
["Tetrafluoroethylene","C2F4","116-14-3","C2F4","SG","SGU-8521","Fixed","GD-70D Series","0～2000ppm"]
["Tetrafluoroethylene","C2F4","116-14-3","C2F4","SG","SGU-8521","Fixed","TP-70D","0～2000ppm"]
["Tetrafluoroethylene","C2F4","116-14-3","C2F4","SG","SGU-8521","Fixed","GD-70D Series","0～5000ppm"]
["Tetrafluoroethylene","C2F4","116-14-3","C2F4","SG","SGU-8521","Fixed","TP-70D","0～5000ppm"]
["Tetrafluoroethylene","C2F4","116-14-3","C2F4","SG","SG-8521","Fixed","GD-A80V Series","★0～500ppm/★0～1000ppm/★0～2000ppm/★0～3000ppm/★0～5000ppm/★0～10000ppm","★Range easily affected by environmental conditions and other"]
["Tetrafluoroethylene","C2F4","116-14-3","C2F4","SG","SG-8521","Fixed","GD-D58・GH Series","★0～500ppm/★0～1000ppm/★0～2000ppm/★0～3000ppm/★0～5000ppm/★0～10000ppm","★Range easily affected by environmental conditions and other"]
["Tetrafluoroethylene","C2F4","116-14-3","C2F4","SG","SG-8521","Fixed","SD-1GH Series","★0～500ppm/★0～1000ppm/★0～2000ppm/★0～3000ppm/★0～5000ppm/★0～10000ppm","★Range easily affected by environmental conditions and other"]
["Tetrafluoroethylene","C2F4","116-14-3","C2F4","SG","SG-8521","Fixed","SD-D58・GH Series","★0～500ppm/★0～1000ppm/★0～2000ppm/★0～3000ppm/★0～5000ppm/★0～10000ppm","★Range easily affected by environmental conditions and other"]
["Tetrahydrofuran","THF","109-99-9","C4H8O","HW","NC-6215","Portable","GP-1000(HC/CH4)","0～100%LEL"]
["Tetrahydrofuran","THF","109-99-9","C4H8O","HW","NC-6307","Portable","NC-1000(HC/CH4)","0～10000ppm"]
["Tetrahydrofuran","THF","109-99-9","C4H8O","RI","DE-3315-2","Fixed","SD-1RI Series","0～100%LEL"]
["Tetrahydrofuran","THF","109-99-9","C4H8O","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Tetrahydrofuran","THF","109-99-9","C4H8O","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Tetrahydrofuran","THF","109-99-9","C4H8O","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～20000ppm"]
["Tetrahydrofuran","THF","109-99-9","C4H8O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～20000ppm"]
["Tetrahydrofuran","THF","109-99-9","C4H8O","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～20000ppm"]
["Tetrahydrofuran","THF","109-99-9","C4H8O","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～20000ppm"]
["Tetrahydrofuran","THF","109-99-9","C4H8O","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～20000ppm"]
["Tetrahydrofuran","THF","109-99-9","C4H8O","HW","NC-6240A","Fixed","GD-A80 Series","0～100%LEL/0～20000ppm"]
["Tetrahydrofuran","THF","109-99-9","C4H8O","HW","NC-6240A","Fixed","GD-D58(TYPE NC) Series","0～100%LEL/0～20000ppm"]
["Tetrahydrofuran","THF","109-99-9","C4H8O","HW","NC-6240A","Fixed","SD-1(TYPE NC) Series","0～100%LEL/0～20000ppm"]
["Tetrahydrofuran","THF","109-99-9","C4H8O","HW","NC-6240A","Fixed","SD-D58(TYPE NC) Series","0～100%LEL/0～20000ppm"]
["Tetrahydrofuran","THF","109-99-9","C4H8O","HW","NC-6245","Fixed","GD-A80 Series","0～100%LEL"]
["Tetrahydrofuran","THF","109-99-9","C4H8O","HW","NC-6245","Fixed","GD-D58(TYPE NC) Series","0～100%LEL"]
["Tetrahydrofuran","THF","109-99-9","C4H8O","HW","NC-6245","Fixed","SD-1(TYPE NC) Series","0～100%LEL"]
["Tetrahydrofuran","THF","109-99-9","C4H8O","HW","NC-6245","Fixed","SD-D58(TYPE NC) Series","0～100%LEL"]
["Tetrahydrofuran","THF","109-99-9","C4H8O","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Tetrahydrofuran","THF","109-99-9","C4H8O","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Tetrahydrofuran","THF","109-99-9","C4H8O","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Tetrahydrofuran","THF","109-99-9","C4H8O","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Tetrahydrofuran","THF","109-99-9","C4H8O","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Tetrahydrofuran","THF","109-99-9","C4H8O","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Tetrahydrofuran","THF","109-99-9","C4H8O","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Tetrahydrofuran","THF","109-99-9","C4H8O","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["Tetrahydrofuran","THF","109-99-9","C4H8O","SG","SG-8521","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～600ppm/0～1000ppm/0～2000ppm"]
["Tetrahydrofuran","THF","109-99-9","C4H8O","SG","SG-8521","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～600ppm/0～1000ppm/0～2000ppm"]
["Tetrahydrofuran","THF","109-99-9","C4H8O","SG","SG-8521","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～600ppm/0～1000ppm/0～2000ppm"]
["Tetrahydrofuran","THF","109-99-9","C4H8O","SG","SG-8521","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～600ppm/0～1000ppm/0～2000ppm"]
["Tetrahydrofuran","THF","109-99-9","C4H8O","SG","SG-8562","Fixed","GD-A80V Series","0～20ppm/0～30ppm/0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Tetrahydrofuran","THF","109-99-9","C4H8O","SG","SG-8562","Fixed","GD-D58・GH Series","0～20ppm/0～30ppm/0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Tetrahydrofuran","THF","109-99-9","C4H8O","SG","SG-8562","Fixed","SD-1GH Series","0～20ppm/0～30ppm/0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Tetrahydrofuran","THF","109-99-9","C4H8O","SG","SG-8562","Fixed","SD-D58・GH Series","0～20ppm/0～30ppm/0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Tetrahydrothiophene","THT","110-01-0","C4H8S","SG","SG-8521","Fixed","GD-A80V Series","0～30ppm/0～50ppm/0～100ppm"]
["Tetrahydrothiophene","THT","110-01-0","C4H8S","SG","SG-8521","Fixed","GD-D58・GH Series","0～30ppm/0～50ppm/0～100ppm"]
["Tetrahydrothiophene","THT","110-01-0","C4H8S","SG","SG-8521","Fixed","SD-1GH Series","0～30ppm/0～50ppm/0～100ppm"]
["Tetrahydrothiophene","THT","110-01-0","C4H8S","SG","SG-8521","Fixed","SD-D58・GH Series","0～30ppm/0～50ppm/0～100ppm"]
["Tetramethylsilane","TMS","75-76-3","C4H12Si","SS","SSU-1925","Fixed","GD-70D+PLU Series","0‐15ppm","PLU-70 required"]
["Tetramethylsilane","TMS","75-76-3","C4H12Si","SS","SSU-1925","Fixed","GD-70DG","0‐15ppm","PLU-70 required"]
["Texanol","C12H24O3","25265-77-4","C12H24O3","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Texanol","C12H24O3","25265-77-4","C12H24O3","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Texanol","C12H24O3","25265-77-4","C12H24O3","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Texanol","C12H24O3","25265-77-4","C12H24O3","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Texanol","C12H24O3","25265-77-4","C12H24O3","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Texanol","C12H24O3","25265-77-4","C12H24O3","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Texanol","C12H24O3","25265-77-4","C12H24O3","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Toluene","C7H8","108-88-3","C7H8","HW","NC-6215","Portable","GX-8000(TYPE LEL)","0～100%LEL"]
["Toluene","C7H8","108-88-3","C7H8","HW","NC-6215","Portable","GP-1000(HC/CH4)","0～100%LEL"]
["Toluene","C7H8","108-88-3","C7H8","HW","NC-6307","Portable","NC-1000(HC/CH4)","0～10000ppm"]
["Toluene","C7H8","108-88-3","C7H8","SH","SH-8662","Portable","SP-220(TYPE SC)","0～10ppm"]
["Toluene","C7H8","108-88-3","C7H8","HW","NCU-6211","Fixed","GD-70D Series","0～100%LEL","Confirm that GD-70D is non-explosion proof"]
["Toluene","C7H8","108-88-3","C7H8","HW","NCU-6211","Fixed","TP-70D","0～100%LEL","Confirm that GD-70D is non-explosion proof"]
["Toluene","C7H8","108-88-3","C7H8","RI","DE-3315-1","Fixed","SD-1RI Series","0～100%LEL"]
["Toluene","C7H8","108-88-3","C7H8","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Toluene","C7H8","108-88-3","C7H8","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Toluene","C7H8","108-88-3","C7H8","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～12000ppm"]
["Toluene","C7H8","108-88-3","C7H8","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～12000ppm"]
["Toluene","C7H8","108-88-3","C7H8","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～12000ppm"]
["Toluene","C7H8","108-88-3","C7H8","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～12000ppm"]
["Toluene","C7H8","108-88-3","C7H8","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～12000ppm"]
["Toluene","C7H8","108-88-3","C7H8","HW","HW-6213/NC-6213","Fixed","GD-A80 Series","0～100%LEL/0～12000ppm"]
["Toluene","C7H8","108-88-3","C7H8","HW","HW-6213/NC-6213","Fixed","GD-D58(TYPE GP) Series","0～100%LEL/0～12000ppm"]
["Toluene","C7H8","108-88-3","C7H8","HW","HW-6213/NC-6213","Fixed","GD-D58(TYPE NC) Series","0～100%LEL/0～12000ppm"]
["Toluene","C7H8","108-88-3","C7H8","HW","NC-6240A","Fixed","GD-A80 Series","0～100%LEL/0～12000ppm"]
["Toluene","C7H8","108-88-3","C7H8","HW","NC-6240A","Fixed","GD-D58(TYPE NC) Series","0～100%LEL/0～12000ppm"]
["Toluene","C7H8","108-88-3","C7H8","HW","NC-6240A","Fixed","SD-1(TYPE NC) Series","0～100%LEL/0～12000ppm"]
["Toluene","C7H8","108-88-3","C7H8","HW","NC-6240A","Fixed","SD-D58(TYPE NC) Series","0～100%LEL/0～12000ppm"]
["Toluene","C7H8","108-88-3","C7H8","HW","NC-6245","Fixed","GD-A80 Series","0～100%LEL"]
["Toluene","C7H8","108-88-3","C7H8","HW","NC-6245","Fixed","GD-D58(TYPE NC) Series","0～100%LEL"]
["Toluene","C7H8","108-88-3","C7H8","HW","NC-6245","Fixed","SD-1(TYPE NC) Series","0～100%LEL"]
["Toluene","C7H8","108-88-3","C7H8","HW","NC-6245","Fixed","SD-D58(TYPE NC) Series","0～100%LEL"]
["Toluene","C7H8","108-88-3","C7H8","HW","NC-6250","Fixed","GD-A80 Series","0～100%LEL/0～12000ppm"]
["Toluene","C7H8","108-88-3","C7H8","HW","NC-6250","Fixed","GD-D58(TYPE NC) Series","0～100%LEL/0～12000ppm"]
["Toluene","C7H8","108-88-3","C7H8","HW","NC-6250","Fixed","GD-A80 Series","0～100%LEL/0～12000ppm"]
["Toluene","C7H8","108-88-3","C7H8","HW","NC-6250","Fixed","GD-D58(TYPE NC) Series","0～100%LEL/0～12000ppm"]
["Toluene","C7H8","108-88-3","C7H8","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Toluene","C7H8","108-88-3","C7H8","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Toluene","C7H8","108-88-3","C7H8","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Toluene","C7H8","108-88-3","C7H8","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Toluene","C7H8","108-88-3","C7H8","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Toluene","C7H8","108-88-3","C7H8","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Toluene","C7H8","108-88-3","C7H8","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Toluene","C7H8","108-88-3","C7H8","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["Toluene","C7H8","108-88-3","C7H8","SG","SG-8521","Fixed","GD-A80V Series","0～200ppm/0～300ppm/0～500ppm/0～600ppm/0～1000ppm/0～2000ppm/0～3000ppm"]
["Toluene","C7H8","108-88-3","C7H8","SG","SG-8521","Fixed","GD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～600ppm/0～1000ppm/0～2000ppm/0～3000ppm"]
["Toluene","C7H8","108-88-3","C7H8","SG","SG-8521","Fixed","SD-1GH Series","0～200ppm/0～300ppm/0～500ppm/0～600ppm/0～1000ppm/0～2000ppm/0～3000ppm"]
["Toluene","C7H8","108-88-3","C7H8","SG","SG-8521","Fixed","SD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～600ppm/0～1000ppm/0～2000ppm/0～3000ppm"]
["Toluene","C7H8","108-88-3","C7H8","SG","SG-8562","Fixed","GD-A80V Series","0～20ppm/0～30ppm/0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["Toluene","C7H8","108-88-3","C7H8","SG","SG-8562","Fixed","GD-D58・GH Series","0～20ppm/0～30ppm/0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["Toluene","C7H8","108-88-3","C7H8","SG","SG-8562","Fixed","SD-1GH Series","0～20ppm/0～30ppm/0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["Toluene","C7H8","108-88-3","C7H8","SG","SG-8562","Fixed","SD-D58・GH Series","0～20ppm/0～30ppm/0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["trans-1,2-Dichloroethylene","C2H2CL2","156-60-5","C2H2CL2","SG","SGU-8513","Fixed","GD-70D Series","0～500ppm"]
["trans-1,2-Dichloroethylene","C2H2CL2","156-60-5","C2H2CL2","SG","SGU-8513","Fixed","TP-70D","0～500ppm"]
["trans-1,2-Dichloroethylene","C2H2CL2","156-60-5","C2H2CL2","SG","SGU-8513","Fixed","GD-70D Series","0～600ppm"]
["trans-1,2-Dichloroethylene","C2H2CL2","156-60-5","C2H2CL2","SG","SGU-8513","Fixed","TP-70D","0～600ppm"]
["trans-1,2-Dichloroethylene","C2H2CL2","156-60-5","C2H2CL2","HW","NC-6250","Fixed","GD-A80 Series","0～30%LEL"]
["trans-1,2-Dichloroethylene","C2H2CL2","156-60-5","C2H2CL2","HW","NC-6250","Fixed","GD-D58(TYPE NC) Series","0～30%LEL"]
["trans-1,2-Dichloroethylene","C2H2CL2","156-60-5","C2H2CL2","SG","SG-8513","Fixed","GD-A80V Series","0～300ppm/0～500ppm/0～600ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["trans-1,2-Dichloroethylene","C2H2CL2","156-60-5","C2H2CL2","SG","SG-8513","Fixed","GD-D58・GH Series","0～300ppm/0～500ppm/0～600ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["trans-1,2-Dichloroethylene","C2H2CL2","156-60-5","C2H2CL2","SG","SG-8513","Fixed","SD-1GH Series","0～300ppm/0～500ppm/0～600ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["trans-1,2-Dichloroethylene","C2H2CL2","156-60-5","C2H2CL2","SG","SG-8513","Fixed","SD-D58・GH Series","0～300ppm/0～500ppm/0～600ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Trans-1,3,3,3-tetrafluoropropene","tC3H2F4","29118-24-9","C3H2F4","RI","DE-2113-35","Fixed","RI-257","0～20000ppm"]
["Trans-1,3,3,3-tetrafluoropropene","tC3H2F4","29118-24-9","C3H2F4","RI","DE-2113-35","Fixed","RI-257","0～2000ppm"]
["Trans-1,3,3,3-tetrafluoropropene","tC3H2F4","29118-24-9","C3H2F4","SG","SG-8511","Fixed","GD-A80V Series","0～2000ppm/0～3000ppm"]
["Trans-1,3,3,3-tetrafluoropropene","tC3H2F4","29118-24-9","C3H2F4","SG","SG-8511","Fixed","GD-D58・GH Series","0～2000ppm/0～3000ppm"]
["Trans-1,3,3,3-tetrafluoropropene","tC3H2F4","29118-24-9","C3H2F4","SG","SG-8511","Fixed","SD-1GH Series","0～2000ppm/0～3000ppm"]
["Trans-1,3,3,3-tetrafluoropropene","tC3H2F4","29118-24-9","C3H2F4","SG","SG-8511","Fixed","SD-D58・GH Series","0～2000ppm/0～3000ppm"]
["Trans-1,3,3,3-tetrafluoropropene","tC3H2F4","29118-24-9","C3H2F4","SG","SG-8563","Fixed","GD-A80V Series","0～200ppm/0～300ppm/0～500ppm"]
["Trans-1,3,3,3-tetrafluoropropene","tC3H2F4","29118-24-9","C3H2F4","SG","SG-8563","Fixed","GD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm"]
["Trans-1,3,3,3-tetrafluoropropene","tC3H2F4","29118-24-9","C3H2F4","SG","SG-8563","Fixed","SD-1GH Series","0～200ppm/0～300ppm/0～500ppm"]
["Trans-1,3,3,3-tetrafluoropropene","tC3H2F4","29118-24-9","C3H2F4","SG","SG-8563","Fixed","SD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm"]
["trans-1-Chloro-3,3,3-trigluoropropene","1233zd","102687-65-0","C3H2F3CL","SG","SG-8513","Fixed","GD-A80V Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["trans-1-Chloro-3,3,3-trigluoropropene","1233zd","102687-65-0","C3H2F3CL","SG","SG-8513","Fixed","GD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["trans-1-Chloro-3,3,3-trigluoropropene","1233zd","102687-65-0","C3H2F3CL","SG","SG-8513","Fixed","SD-1GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["trans-1-Chloro-3,3,3-trigluoropropene","1233zd","102687-65-0","C3H2F3CL","SG","SG-8513","Fixed","SD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Trichloroethylene","C2HCL3","79-01-6","C2HCL3","SH","SH-8662","Portable","SP-220(TYPE SC)","0～10ppm"]
["Trichloroethylene","C2HCL3","79-01-6","C2HCL3","SG","SGU-8523","Fixed","GD-70D Series","0～3000ppm"]
["Trichloroethylene","C2HCL3","79-01-6","C2HCL3","SG","SGU-8523","Fixed","TP-70D","0～3000ppm"]
["Trichloroethylene","C2HCL3","79-01-6","C2HCL3","SG","SG-8523","Fixed","GD-A80V Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Trichloroethylene","C2HCL3","79-01-6","C2HCL3","SG","SG-8523","Fixed","GD-D58・GH Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Trichloroethylene","C2HCL3","79-01-6","C2HCL3","SG","SG-8523","Fixed","SD-1GH Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Trichloroethylene","C2HCL3","79-01-6","C2HCL3","SG","SG-8523","Fixed","SD-D58・GH Series","0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Trichlorofluoromethane","R-11","75-69-4","CFCL3","RI","DE-2113-56","Fixed","RI-557","0～5000ppm"]
["Trichlorofluoromethane","R-11","75-69-4","CFCL3","SG","SG-8513","Fixed","GD-A80V Series","0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Trichlorofluoromethane","R-11","75-69-4","CFCL3","SG","SG-8513","Fixed","GD-D58・GH Series","0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Trichlorofluoromethane","R-11","75-69-4","CFCL3","SG","SG-8513","Fixed","SD-1GH Series","0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Trichlorofluoromethane","R-11","75-69-4","CFCL3","SG","SG-8513","Fixed","SD-D58・GH Series","0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Triethylamine","C6H15N","121-44-8","C6H15N","ES","ESM-23RVM","Fixed","GD-K88Ai Series","0～15ppm","Updated against electrolyte reduction"]
["Triethylamine","C6H15N","121-44-8","C6H15N","ES","ESM-23RVM","Fixed","GD-K88Di Series","0～15ppm","Updated against electrolyte reduction"]
["Triethylamine","C6H15N","121-44-8","C6H15N","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Triethylamine","C6H15N","121-44-8","C6H15N","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Triethylamine","C6H15N","121-44-8","C6H15N","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～12000ppm"]
["Triethylamine","C6H15N","121-44-8","C6H15N","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～12000ppm"]
["Triethylamine","C6H15N","121-44-8","C6H15N","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～12000ppm"]
["Triethylamine","C6H15N","121-44-8","C6H15N","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～12000ppm"]
["Triethylamine","C6H15N","121-44-8","C6H15N","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～12000ppm"]
["Triethylamine","C6H15N","121-44-8","C6H15N","SG","SG-8511","Fixed","GD-A80V Series","0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Triethylamine","C6H15N","121-44-8","C6H15N","SG","SG-8511","Fixed","GD-D58・GH Series","0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Triethylamine","C6H15N","121-44-8","C6H15N","SG","SG-8511","Fixed","SD-1GH Series","0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Triethylamine","C6H15N","121-44-8","C6H15N","SG","SG-8511","Fixed","SD-D58・GH Series","0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Triethylamine","C6H15N","121-44-8","C6H15N","SG","SG-8521","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["Triethylamine","C6H15N","121-44-8","C6H15N","SG","SG-8521","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["Triethylamine","C6H15N","121-44-8","C6H15N","SG","SG-8521","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["Triethylamine","C6H15N","121-44-8","C6H15N","SG","SG-8521","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["Triethylborate","TEB","150-46-9","C6H15BO3","SS","SSU-1925","Fixed","GD-70D+PLU Series","0～1000ppm","PLU-70 required/Export limited：unable to measure under 6%FS(0.18ppm)"]
["Triethylborate","TEB","150-46-9","C6H15BO3","SS","SSU-1925","Fixed","GD-70DG","0～1000ppm","PLU-70 required"]
["Triethylene glycol dimethyl ether","DMTG","112-49-2","C8H18O4","SG","SG-8521","Fixed","GD-A80V Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Triethylene glycol dimethyl ether","DMTG","112-49-2","C8H18O4","SG","SG-8521","Fixed","GD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Triethylene glycol dimethyl ether","DMTG","112-49-2","C8H18O4","SG","SG-8521","Fixed","SD-1GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Triethylene glycol dimethyl ether","DMTG","112-49-2","C8H18O4","SG","SG-8521","Fixed","SD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Triethylphosphate","TEOP","78-40-0","C6H15O4P","SS","SSU-1925","Fixed","GD-70D+PLU Series","0～2ppm","PLU-70 required"]
["Triethylphosphate","TEOP","78-40-0","C6H15O4P","SS","SSU-1925","Fixed","GD-70DG","0～2ppm","PLU-70 required"]
["Trifluoromethane","HFC-23","75-46-7","CHF3","SH","SH-8661","Portable","SP-220(TYPE F)","0～5000ppm"]
["Trifluoromethane","HFC-23","75-46-7","CHF3","RI","DE-2113-35","Fixed","RI-257","0～10000ppm"]
["Trifluoromethanesulfonyl fluoride","TfF","335-05-7","CO2F4S","RI","DE-2113-37","Fixed","RI-257","0～6000ppm"]
["Trimethoxysilane","TRIMOS","2487-90-3","C3H10O3Si","SS","SSU-1925","Fixed","GD-70D+PLU Series","0‐15ppm","PLU-70 required"]
["Trimethoxysilane","TRIMOS","2487-90-3","C3H10O3Si","SS","SSU-1925","Fixed","GD-70DG","0‐15ppm","PLU-70 required"]
["Trimethyl benzene","C9H12","108-67-8,25551-13-7(all isomer)","C9H12","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Trimethyl benzene","C9H12","108-67-8,25551-13-7(all isomer)","C9H12","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Trimethyl benzene","C9H12","108-67-8,25551-13-7(all isomer)","C9H12","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Trimethyl benzene","C9H12","108-67-8,25551-13-7(all isomer)","C9H12","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Trimethyl benzene","C9H12","108-67-8,25551-13-7(all isomer)","C9H12","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Trimethyl benzene","C9H12","108-67-8,25551-13-7(all isomer)","C9H12","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Trimethyl benzene","C9H12","108-67-8,25551-13-7(all isomer)","C9H12","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Trimethyl benzene","C9H12","108-67-8,25551-13-7(all isomer)","C9H12","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["Trimethyl benzene","C9H12","108-67-8,25551-13-7(all isomer)","C9H12","SG","SG-8521","Fixed","GD-A80V Series","0～30ppm/0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm","Standard sensor: SG-8562"]
["Trimethyl benzene","C9H12","108-67-8,25551-13-7(all isomer)","C9H12","SG","SG-8521","Fixed","GD-D58・GH Series","0～30ppm/0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm","Standard sensor: SG-8562"]
["Trimethyl benzene","C9H12","108-67-8,25551-13-7(all isomer)","C9H12","SG","SG-8521","Fixed","SD-1GH Series","0～30ppm/0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm","Standard sensor: SG-8562"]
["Trimethyl benzene","C9H12","108-67-8,25551-13-7(all isomer)","C9H12","SG","SG-8521","Fixed","SD-D58・GH Series","0～30ppm/0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm","Standard sensor: SG-8562"]
["Trimethyl benzene","C9H12","108-67-8,25551-13-7(all isomer)","C9H12","SG","SG-8562","Fixed","GD-A80V Series","0～20ppm/0～30ppm/0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Trimethyl benzene","C9H12","108-67-8,25551-13-7(all isomer)","C9H12","SG","SG-8562","Fixed","GD-D58・GH Series","0～20ppm/0～30ppm/0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Trimethyl benzene","C9H12","108-67-8,25551-13-7(all isomer)","C9H12","SG","SG-8562","Fixed","SD-1GH Series","0～20ppm/0～30ppm/0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Trimethyl benzene","C9H12","108-67-8,25551-13-7(all isomer)","C9H12","SG","SG-8562","Fixed","SD-D58・GH Series","0～20ppm/0～30ppm/0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Trimethyl phosphite","TMP","121-45-9","C3H9O3P","SS","SSU-1925","Fixed","GD-70D+PLU Series","0.18～3ppm","PLU-70 required/Export limited：unable to measure under 6%FS(0.18ppm)"]
["Trimethyl phosphite","TMP","121-45-9","C3H9O3P","SS","SSU-1925","Fixed","GD-70DG","0.18～3ppm","PLU-70 required/Export limited：unable to measure under 6%FS(0.18ppm)"]
["Trimethylamine","TMA","75-50-3","C3H9N","ES","ESU-23RV","Fixed","GD-70D Series","0～15ppm"]
["Trimethylamine","TMA","75-50-3","C3H9N","ES","ESU-23RV","Fixed","TP-70D","0～15ppm"]
["Trimethylamine","TMA","75-50-3","C3H9N","ES","ESU-23RVM","Fixed","GD-70D Series","0～15ppm","Updated against electrolyte reduction"]
["Trimethylamine","TMA","75-50-3","C3H9N","ES","ESU-23RVM","Fixed","TP-70D","0～15ppm","Updated against electrolyte reduction"]
["Trimethylamine","TMA","75-50-3","C3H9N","ES","ESM-23RV","Fixed","GD-K88Ai Series","0～15ppm"]
["Trimethylamine","TMA","75-50-3","C3H9N","ES","ESM-23RV","Fixed","GD-K88Di Series","0～15ppm"]
["Trimethylamine","TMA","75-50-3","C3H9N","ES","ESM-23RVM","Fixed","GD-K88Ai Series","0～15ppm","Updated against electrolyte reduction"]
["Trimethylamine","TMA","75-50-3","C3H9N","ES","ESM-23RVM","Fixed","GD-K88Di Series","0～15ppm","Updated against electrolyte reduction"]
["Trimethylamine","TMA","75-50-3","C3H9N","SG","SG-8521","Fixed","GD-A80V Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["Trimethylamine","TMA","75-50-3","C3H9N","SG","SG-8521","Fixed","GD-D58・GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["Trimethylamine","TMA","75-50-3","C3H9N","SG","SG-8521","Fixed","SD-1GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["Trimethylamine","TMA","75-50-3","C3H9N","SG","SG-8521","Fixed","SD-D58・GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm"]
["Trimethylborate","TMB","121-43-7","C3H9BO3","SS","SSU-1925","Fixed","GD-70D+PLU Series","0～1000ppm","PLU-70 required"]
["Trimethylborate","TMB","121-43-7","C3H9BO3","SS","SSU-1925","Fixed","GD-70DG","0～1000ppm","PLU-70 required"]
["Trimethylphosphate","TMOP","512-56-1","C3H9O4P","SS","SSU-1925","Fixed","GD-70D+PLU Series","0～10ppm","PLU-70 required"]
["Trimethylphosphate","TMOP","512-56-1","C3H9O4P","SS","SSU-1925","Fixed","GD-70DG","0～10ppm","PLU-70 required"]
["Trimethylsilane","TRIMS","993-07-7","C3H10Si","SS","SSU-1925","Fixed","GD-70D+PLU Series","0‐15ppm","PLU-70 required"]
["Trimethylsilane","TRIMS","993-07-7","C3H10Si","SS","SSU-1925","Fixed","GD-70DG","0‐15ppm","PLU-70 required"]
["Trisilylamine","Si3H9N","13862-16-3","Si3H9N","ES","ESU-23DH","Fixed","GD-70D Series","0～15ppm"]
["Trisilylamine","Si3H9N","13862-16-3","Si3H9N","ES","ESU-23DH","Fixed","TP-70D","0～15ppm"]
["Trisilylamine","Si3H9N","13862-16-3","Si3H9N","ES","ESM-23DH","Fixed","GD-K88Ai Series","0～15ppm"]
["Trisilylamine","Si3H9N","13862-16-3","Si3H9N","ES","ESM-23DH","Fixed","GD-K88Di Series","0～15ppm"]
["Turpentine Oil","C10H16","8006-64-2","-","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～50%LEL/～4000ppm"]
["Turpentine Oil","C10H16","8006-64-2","-","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～50%LEL/～4000ppm"]
["Turpentine Oil","C10H16","8006-64-2","-","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～50%LEL/～4000ppm"]
["Turpentine Oil","C10H16","8006-64-2","-","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～50%LEL/～4000ppm"]
["Turpentine Oil","C10H16","8006-64-2","-","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～50%LEL/～4000ppm"]
["Turpentine Oil","C10H16","8006-64-2","-","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Turpentine Oil","C10H16","8006-64-2","-","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Turpentine Oil","C10H16","8006-64-2","-","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Turpentine Oil","C10H16","8006-64-2","-","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Turpentine Oil","C10H16","8006-64-2","-","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Turpentine Oil","C10H16","8006-64-2","-","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Turpentine Oil","C10H16","8006-64-2","-","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Turpentine Oil","C10H16","8006-64-2","-","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["Turpentine Oil","C10H16","8006-64-2","-","SG","SG-8521","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Turpentine Oil","C10H16","8006-64-2","-","SG","SG-8521","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Turpentine Oil","C10H16","8006-64-2","-","SG","SG-8521","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Turpentine Oil","C10H16","8006-64-2","-","SG","SG-8521","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Undecane","C11H24","1120-21-4","C11H24","HW","NC-6211","Fixed","GD-A80 Series","～30%LEL/～2000ppm"]
["Undecane","C11H24","1120-21-4","C11H24","HW","NC-6211","Fixed","GD-D58(TYPE GP) Series","～30%LEL/～2000ppm"]
["Undecane","C11H24","1120-21-4","C11H24","HW","NC-6211","Fixed","GD-D58(TYPE NC) Series","～30%LEL/～2000ppm"]
["Undecane","C11H24","1120-21-4","C11H24","HW","NC-6211","Fixed","SD-1(TYPE NC) Series","～30%LEL/～2000ppm"]
["Undecane","C11H24","1120-21-4","C11H24","HW","NC-6211","Fixed","SD-D58(TYPE NC) Series","～30%LEL/～2000ppm"]
["Undecane","C11H24","1120-21-4","C11H24","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Undecane","C11H24","1120-21-4","C11H24","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Undecane","C11H24","1120-21-4","C11H24","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Undecane","C11H24","1120-21-4","C11H24","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Undecane","C11H24","1120-21-4","C11H24","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Undecane","C11H24","1120-21-4","C11H24","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Undecane","C11H24","1120-21-4","C11H24","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Undecane","C11H24","1120-21-4","C11H24","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["Undecane","C11H24","1120-21-4","C11H24","SG","SG-8521","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Undecane","C11H24","1120-21-4","C11H24","SG","SG-8521","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Undecane","C11H24","1120-21-4","C11H24","SG","SG-8521","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Undecane","C11H24","1120-21-4","C11H24","SG","SG-8521","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Vinyl acetate","VAc","108-05-4","C4H6O2","HW","NC-6215","Portable","GP-1000(Specified cal.gas)","0～100%LEL"]
["Vinyl acetate","VAc","108-05-4","C4H6O2","HW","NC-6307","Portable","NC-1000(Specified cal. Gas)","0～10000ppm"]
["Vinyl acetate","VAc","108-05-4","C4H6O2","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Vinyl acetate","VAc","108-05-4","C4H6O2","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Vinyl acetate","VAc","108-05-4","C4H6O2","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～26000ppm"]
["Vinyl acetate","VAc","108-05-4","C4H6O2","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～26000ppm"]
["Vinyl acetate","VAc","108-05-4","C4H6O2","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～26000ppm"]
["Vinyl acetate","VAc","108-05-4","C4H6O2","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～26000ppm"]
["Vinyl acetate","VAc","108-05-4","C4H6O2","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～26000ppm"]
["Vinyl acetate","VAc","108-05-4","C4H6O2","SG","SG-8521","Fixed","GD-A80V Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Vinyl acetate","VAc","108-05-4","C4H6O2","SG","SG-8521","Fixed","GD-D58・GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Vinyl acetate","VAc","108-05-4","C4H6O2","SG","SG-8521","Fixed","SD-1GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Vinyl acetate","VAc","108-05-4","C4H6O2","SG","SG-8521","Fixed","SD-D58・GH Series","0～50ppm/0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Vinyl chloride","VCM","75-01-4","C2H3CL","SH","SH-8662","Portable","SP-220(TYPE SC)","0～1ppm"]
["Vinyl chloride","VCM","75-01-4","C2H3CL","SG","SGU-8513","Fixed","GD-70D Series","0～1000ppm"]
["Vinyl chloride","VCM","75-01-4","C2H3CL","SG","SGU-8513","Fixed","TP-70D","0～1000ppm"]
["Vinyl chloride","VCM","75-01-4","C2H3CL","HW","NCU-6250","Fixed","GD-70D Series","0～100%LEL","Confirm that GD-70D is non-explosion proof"]
["Vinyl chloride","VCM","75-01-4","C2H3CL","HW","NCU-6250","Fixed","TP-70D","0～100%LEL","Confirm that GD-70D is non-explosion proof"]
["Vinyl chloride","VCM","75-01-4","C2H3CL","HW","NC-6250","Fixed","GD-A80 Series","0～100%LEL/0～38000ppm"]
["Vinyl chloride","VCM","75-01-4","C2H3CL","HW","NC-6250","Fixed","GD-D58(TYPE NC) Series","0～100%LEL/0～38000ppm"]
["Vinyl chloride","VCM","75-01-4","C2H3CL","SG","SG-8513","Fixed","GD-A80V Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm"]
["Vinyl chloride","VCM","75-01-4","C2H3CL","SG","SG-8513","Fixed","GD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm"]
["Vinyl chloride","VCM","75-01-4","C2H3CL","SG","SG-8513","Fixed","SD-1GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm"]
["Vinyl chloride","VCM","75-01-4","C2H3CL","SG","SG-8513","Fixed","SD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm"]
["Vinyl chloride","VCM","75-01-4","C2H3CL","SG","SG-8582","Fixed","GD-A80V Series","0～300ppm/0～500ppm/0～1000ppm"]
["Vinyl chloride","VCM","75-01-4","C2H3CL","SG","SG-8582","Fixed","GD-D58・GH Series","0～300ppm/0～500ppm/0～1000ppm"]
["Vinyl chloride","VCM","75-01-4","C2H3CL","SG","SG-8582","Fixed","SD-1GH Series","0～300ppm/0～500ppm/0～1000ppm"]
["Vinyl chloride","VCM","75-01-4","C2H3CL","SG","SG-8582","Fixed","SD-D58・GH Series","0～300ppm/0～500ppm/0～1000ppm"]
["Vinyl cyclohexene","C8H12","100-40-3","C8H12","SG","SG-8511","Fixed","GD-A80V Series","0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Vinyl cyclohexene","C8H12","100-40-3","C8H12","SG","SG-8511","Fixed","GD-D58・GH Series","0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Vinyl cyclohexene","C8H12","100-40-3","C8H12","SG","SG-8511","Fixed","SD-1GH Series","0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Vinyl cyclohexene","C8H12","100-40-3","C8H12","SG","SG-8511","Fixed","SD-D58・GH Series","0～500ppm/0～1000ppm/0～2000ppm/0～3000ppm/0～5000ppm"]
["Vinylidene chloride","PVC","75-35-4","C2H2CL2","SG","SG-8513","Fixed","GD-A80V Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Vinylidene chloride","PVC","75-35-4","C2H2CL2","SG","SG-8513","Fixed","GD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Vinylidene chloride","PVC","75-35-4","C2H2CL2","SG","SG-8513","Fixed","SD-1GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Vinylidene chloride","PVC","75-35-4","C2H2CL2","SG","SG-8513","Fixed","SD-D58・GH Series","0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Vinylidene fluoride","VDF","75-38-7","C2H2F2","SG","SGU-8521","Fixed","GD-70D Series","0～500ppm"]
["Vinylidene fluoride","VDF","75-38-7","C2H2F2","SG","SGU-8521","Fixed","TP-70D","0～500ppm"]
["Vinylidene fluoride","VDF","75-38-7","C2H2F2","SG","SGU-8521","Fixed","GD-70D Series","0～1000ppm"]
["Vinylidene fluoride","VDF","75-38-7","C2H2F2","SG","SGU-8521","Fixed","TP-70D","0～1000ppm"]
["Vinylidene fluoride","VDF","75-38-7","C2H2F2","SG","SG-8521","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Vinylidene fluoride","VDF","75-38-7","C2H2F2","SG","SG-8521","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Vinylidene fluoride","VDF","75-38-7","C2H2F2","SG","SG-8521","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Vinylidene fluoride","VDF","75-38-7","C2H2F2","SG","SG-8521","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm"]
["Xylene","C8H10","1330-20-7(all isomer),95-47-6(-o),108-38-3(-m),106-42-3(-p)","C8H10","HW","NC-6215","Portable","GP-1000(HC/CH4)","0～100%LEL"]
["Xylene","C8H10","1330-20-7(all isomer),95-47-6(-o),108-38-3(-m),106-42-3(-p)","C8H10","HW","NC-6307","Portable","NC-1000(HC/CH4)","0～10000ppm"]
["Xylene","C8H10","1330-20-7(all isomer),95-47-6(-o),108-38-3(-m),106-42-3(-p)","C8H10","SH","SH-8662","Portable","SP-220(TYPE SC)","0～10ppm"]
["Xylene","C8H10","1330-20-7(all isomer),95-47-6(-o),108-38-3(-m),106-42-3(-p)","C8H10","RI","DE-3315-1","Fixed","SD-1RI Series","0～100%LEL"]
["Xylene","C8H10","1330-20-7(all isomer),95-47-6(-o),108-38-3(-m),106-42-3(-p)","C8H10","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["Xylene","C8H10","1330-20-7(all isomer),95-47-6(-o),108-38-3(-m),106-42-3(-p)","C8H10","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["Xylene","C8H10","1330-20-7(all isomer),95-47-6(-o),108-38-3(-m),106-42-3(-p)","C8H10","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～10000ppm"]
["Xylene","C8H10","1330-20-7(all isomer),95-47-6(-o),108-38-3(-m),106-42-3(-p)","C8H10","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～10000ppm"]
["Xylene","C8H10","1330-20-7(all isomer),95-47-6(-o),108-38-3(-m),106-42-3(-p)","C8H10","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～10000ppm"]
["Xylene","C8H10","1330-20-7(all isomer),95-47-6(-o),108-38-3(-m),106-42-3(-p)","C8H10","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～10000ppm"]
["Xylene","C8H10","1330-20-7(all isomer),95-47-6(-o),108-38-3(-m),106-42-3(-p)","C8H10","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～10000ppm"]
["Xylene","C8H10","1330-20-7(all isomer),95-47-6(-o),108-38-3(-m),106-42-3(-p)","C8H10","HW","HW-6213/NC-6213","Fixed","GD-A80 Series","0～100%LEL/0～10000ppm"]
["Xylene","C8H10","1330-20-7(all isomer),95-47-6(-o),108-38-3(-m),106-42-3(-p)","C8H10","HW","HW-6213/NC-6213","Fixed","GD-D58(TYPE GP) Series","0～100%LEL/0～10000ppm"]
["Xylene","C8H10","1330-20-7(all isomer),95-47-6(-o),108-38-3(-m),106-42-3(-p)","C8H10","HW","HW-6213/NC-6213","Fixed","GD-D58(TYPE NC) Series","0～100%LEL/0～10000ppm"]
["Xylene","C8H10","1330-20-7(all isomer),95-47-6(-o),108-38-3(-m),106-42-3(-p)","C8H10","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Xylene","C8H10","1330-20-7(all isomer),95-47-6(-o),108-38-3(-m),106-42-3(-p)","C8H10","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Xylene","C8H10","1330-20-7(all isomer),95-47-6(-o),108-38-3(-m),106-42-3(-p)","C8H10","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Xylene","C8H10","1330-20-7(all isomer),95-47-6(-o),108-38-3(-m),106-42-3(-p)","C8H10","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["Xylene","C8H10","1330-20-7(all isomer),95-47-6(-o),108-38-3(-m),106-42-3(-p)","C8H10","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Xylene","C8H10","1330-20-7(all isomer),95-47-6(-o),108-38-3(-m),106-42-3(-p)","C8H10","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Xylene","C8H10","1330-20-7(all isomer),95-47-6(-o),108-38-3(-m),106-42-3(-p)","C8H10","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["Xylene","C8H10","1330-20-7(all isomer),95-47-6(-o),108-38-3(-m),106-42-3(-p)","C8H10","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["Xylene","C8H10","1330-20-7(all isomer),95-47-6(-o),108-38-3(-m),106-42-3(-p)","C8H10","SG","SG-8521","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～600ppm/0～1000ppm"]
["Xylene","C8H10","1330-20-7(all isomer),95-47-6(-o),108-38-3(-m),106-42-3(-p)","C8H10","SG","SG-8521","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～600ppm/0～1000ppm"]
["Xylene","C8H10","1330-20-7(all isomer),95-47-6(-o),108-38-3(-m),106-42-3(-p)","C8H10","SG","SG-8521","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～600ppm/0～1000ppm"]
["Xylene","C8H10","1330-20-7(all isomer),95-47-6(-o),108-38-3(-m),106-42-3(-p)","C8H10","SG","SG-8521","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～600ppm/0～1000ppm"]
["α-Pinene","PINENE","80-56-8","C10H16","HW","HW-6211","Fixed","SD-1(TYPE GP) Series","～100%LEL"]
["α-Pinene","PINENE","80-56-8","C10H16","HW","HW-6211","Fixed","SD-D58(TYPE GP) Series","～100%LEL"]
["α-Pinene","PINENE","80-56-8","C10H16","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～100%LEL/～6900ppm"]
["α-Pinene","PINENE","80-56-8","C10H16","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～100%LEL/～6900ppm"]
["α-Pinene","PINENE","80-56-8","C10H16","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～100%LEL/～6900ppm"]
["α-Pinene","PINENE","80-56-8","C10H16","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～100%LEL/～6900ppm"]
["α-Pinene","PINENE","80-56-8","C10H16","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～100%LEL/～6900ppm"]
["α-Terpinene","ATRP","99-86-5","C10H16","HW","HW-6211/NC-6211","Fixed","GD-A80 Series","～75%LEL/～5175ppm"]
["α-Terpinene","ATRP","99-86-5","C10H16","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE GP) Series","～75%LEL/～5175ppm"]
["α-Terpinene","ATRP","99-86-5","C10H16","HW","HW-6211/NC-6211","Fixed","GD-D58(TYPE NC) Series","～75%LEL/～5175ppm"]
["α-Terpinene","ATRP","99-86-5","C10H16","HW","HW-6211/NC-6211","Fixed","SD-1(TYPE NC) Series","～75%LEL/～5175ppm"]
["α-Terpinene","ATRP","99-86-5","C10H16","HW","HW-6211/NC-6211","Fixed","SD-D58(TYPE NC) Series","～75%LEL/～5175ppm"]
["γ-Butyrolactone","GBL","96-48-0","C4H6O2","HW","HW-6206","Fixed","SD-2500","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["γ-Butyrolactone","GBL","96-48-0","C4H6O2","HW","HW-6206","Fixed","SD-2600","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["γ-Butyrolactone","GBL","96-48-0","C4H6O2","HW","HW-6206","Fixed","SD-2700","0～100%LEL","Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["γ-Butyrolactone","GBL","96-48-0","C4H6O2","HW","HW-6207","Fixed","GD-A2400","0～100%LEL","Upper limit of operating temperature of instrument: GD-A2400=160℃"]
["γ-Butyrolactone","GBL","96-48-0","C4H6O2","HW","HW-6208","Fixed","SD-2500","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["γ-Butyrolactone","GBL","96-48-0","C4H6O2","HW","HW-6208","Fixed","SD-2600","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["γ-Butyrolactone","GBL","96-48-0","C4H6O2","HW","HW-6208","Fixed","SD-2700","0～100%LEL","HW-6206 temperature sorted sensor, Upper limit of operating temperature of instrument: SD-2500=160℃/SD-2600=200℃/SD-2700：250℃"]
["γ-Butyrolactone","GBL","96-48-0","C4H6O2","HW","HW-6212","Fixed","GD-A80-70 Series","0～100%LEL"]
["γ-Butyrolactone","GBL","96-48-0","C4H6O2","SG","SG-8521","Fixed","GD-A80V Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["γ-Butyrolactone","GBL","96-48-0","C4H6O2","SG","SG-8521","Fixed","GD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["γ-Butyrolactone","GBL","96-48-0","C4H6O2","SG","SG-8521","Fixed","SD-1GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["γ-Butyrolactone","GBL","96-48-0","C4H6O2","SG","SG-8521","Fixed","SD-D58・GH Series","0～100ppm/0～200ppm/0～300ppm/0～500ppm/0～1000ppm/0～2000ppm"]
["Nitrogen Dioxide","NO2","10102-44-0","NO2","ES","ESF-A24A","Fixed","GD-84D  Series","0 - 15 ppm","There are restrictions on the combination of sensors."]
["Hydrogen Chloride","HCL","7647-01-0","HCL","ES","ESF-A24E2","Fixed","GD-84D  Series","0 - 6 ppm","There are restrictions on the combination of sensors."]
["Ammonia","NH3","7664-41-7","NH3","ES","ESF-B242","Fixed","GD-84D  Series","0 - 75 ppm","There are restrictions on the combination of sensors."]
["Chlorine","CL2","7782-50-5","CL2","ES","ESF-B24A","Fixed","GD-84D  Series","0 - 0.3 ppm","There are restrictions on the combination of sensors."]
["Oxygen","O2","7782-44-7","O2","ES","ESF-X24P","Fixed","GD-84D  Series","0 - 25 %","There are restrictions on the combination of sensors."]
["Phosphine","PH3","7803-51-2","PH3","ES","ESF-A24D","Fixed","GD-84D  Series","0 - 1 ppm","There are restrictions on the combination of sensors."]
["Silane","SiH4","7803-62-5","SiH4","ES","ESF-A24D","Fixed","GD-84D  Series","0 - 15 ppm","There are restrictions on the combination of sensors."]
["Disilane","Si2H6","1590-87-0","Si2H6","ES","ESF-A24D","Fixed","GD-84D  Series","0 - 15 ppm","There are restrictions on the combination of sensors."]
["Sulfur dioxide","SO2","7446-09-5","SO2","ES","ESF-A24D","Fixed","GD-84D  Series","0 - 6 ppm","There are restrictions on the combination of sensors."]
["Nitrogen Monoxide","NO","10102-43-9","NO","ES","ESF-A24D2","Fixed","GD-84D  Series","0 - 100 ppm","There are restrictions on the combination of sensors."]
["Hydrogen Bromide","HBr","10035-10-6","HBr","ES","ESF-A24E2","Fixed","GD-84D  Series","0 - 6 ppm","There are restrictions on the combination of sensors."]
["Diethylamine","DEA","109-89-7","C4H11N","ES","ESF-B241","Fixed","GD-84D  Series","0 - 15 ppm","There are restrictions on the combination of sensors."]
["Dimethylamine","DMA","124-40-3","C2H7N","ES","ESF-B241","Fixed","GD-84D  Series","0 - 15 ppm","There are restrictions on the combination of sensors."]
["Ethylmethylamine","EMA","624-78-2","C3H9N","ES","ESF-B241","Fixed","GD-84D  Series","0 - 15 ppm","There are restrictions on the combination of sensors."]
["Fluorine","F2","7782-41-4","F2","ES","ESF-B248","Fixed","GD-84D  Series","0 - 3 ppm","There are restrictions on the combination of sensors."]
["Hydrogen Fluoride","HF","7664-39-3","HF","ES","ESF-B248","Fixed","GD-84D  Series","0 - 1.5 ppm","There are restrictions on the combination of sensors."]
["Ozone","O3","10028-15-6","O3","ES","ESF-B249","Fixed","GD-84D  Series","0 - 0.6 ppm","There are restrictions on the combination of sensors."]
["Chlorine Trifluoride","CLF3","7790-91-2","CLF3","ES","ESF-B24A","Fixed","GD-84D  Series","0 - 0.3 ppm","There are restrictions on the combination of sensors."]
["Methane","CH4","74-82-8","CH4","SH","SHF-8601","Fixed","GD-84D  Series","0 - 5000 ppm","There are restrictions on the combination of sensors."]
["Isobutane","i-C4H10","75-28-5","C4H10","SH","SHF-8601","Fixed","GD-84D  Series","0 - 2000 ppm","There are restrictions on the combination of sensors."]
["Ethylene","C2H4","74-85-1","C2H4","SH","SHF-8601","Fixed","GD-84D  Series","0 - 2000 ppm","There are restrictions on the combination of sensors."]
["Acetylene","C2H2","74-86-2","C2H2","SH","SHF-8601","Fixed","GD-84D  Series","0 - 2000 ppm","There are restrictions on the combination of sensors."]
["Propylene","C3H6","115-07-1","C3H6","SH","SHF-8601","Fixed","GD-84D  Series","0 - 2000 ppm","There are restrictions on the combination of sensors."]
["n-Hexane","n-C6H14","110-54-3","C6H14","SH","SHF-8601","Fixed","GD-84D  Series","0 - 200 ppm","There are restrictions on the combination of sensors."]
["n-Octane","C8H18","111-65-9","C8H18","SH","SHF-8601","Fixed","GD-84D  Series","0 - 2000 ppm","There are restrictions on the combination of sensors."]
["Monofluoromethane","R-41","593-53-3","CH3F","SH","SHF-8601","Fixed","GD-84D  Series","0 - 2000 ppm","There are restrictions on the combination of sensors."]
["Difluoromethane","R-32","75-10-5","CH2F2","SH","SHF-8601","Fixed","GD-84D  Series","0 - 2000 ppm","There are restrictions on the combination of sensors."]
["Difluoromethane","R-32","75-10-5","CH2F2","SH","SHF-8601","Fixed","GD-84D  Series","0 - 5000 ppm","There are restrictions on the combination of sensors."]
["Isopropyl Alcohol","IPA","67-63-0","C3H8O","SH","SHF-8601","Fixed","GD-84D  Series","0 - 2000 ppm","There are restrictions on the combination of sensors."]
["Hexafluoro-1,3-butadiene","C4F6","685-63-2","C4F6","SH","SHF-8601","Fixed","GD-84D  Series","0 - 2000 ppm","There are restrictions on the combination of sensors."]
["trans-1,2-Dichloroethylene","C2H2CL2","156-60-5","C2H2CL2","SH","SHF-8601","Fixed","GD-84D  Series","0 - 600 ppm","There are restrictions on the combination of sensors."]
["Carbon Monoxide","CO","630-08-0","CO","SH","SHF-8601","Fixed","GD-84D  Series","0 - 1000ppm","There are restrictions on the combination of sensors."]
["Isobutane","i-C4H10","75-28-5","C4H10","SH","SHF-8602","Fixed","GD-84D  Series","0 - 2000 ppm","There are restrictions on the combination of sensors."]
["Hydrogen","H2","1333-74-0","H2","SH","SHF-8603","Fixed","GD-84D  Series","0 - 500 ppm","There are restrictions on the combination of sensors."]
["Hydrogen","H2","1333-74-0","H2","SH","SHF-8603","Fixed","GD-84D  Series","0 - 1000 ppm","There are restrictions on the combination of sensors."]
["Deuterium","D2","7782-39-0","-","SH","SHF-8603","Fixed","GD-84D  Series","0 - 2000 ppm","There are restrictions on the combination of sensors."]
["Hydrogen","H2","1333-74-0","H2","SH","SHF-8603","Fixed","GD-84D  Series","0 - 2000 ppm","There are restrictions on the combination of sensors."]
["Methane","CH4","74-82-8","CH4","SG","SGF-8581","Fixed","GD-84D  Series","0 - 2000 ppm","There are restrictions on the combination of sensors."]
["Difluoromethane","R-32","75-10-5","CH2F2","SG","SGF-8581","Fixed","GD-84D  Series","0 - 2000 ppm","There are restrictions on the combination of sensors."]
["Methane","CH4","74-82-8","CH4","SG","SGF-8581","Fixed","GD-84D  Series","0 - 5000 ppm","There are restrictions on the combination of sensors."]
["Carbonyl sulfide","COS","463-58-1","COS","SG","SGF-8562","Fixed","GD-84D  Series","0 - 2000 ppm","There are restrictions on the combination of sensors."]
["Carbon disulfide","CS2","75-15-0","CS2","SG","SGF-8562","Fixed","GD-84D  Series","0 - 200ppm","There are restrictions on the combination of sensors."]
["Ethylene oxide","EO","75-21-8","C2H4O","SG","SGF-8563","Fixed","GD-84D  Series","0 - 100ppm","There are restrictions on the combination of sensors."]
["Hydrogen Sulfide","H2S","7783-06-4","H2S","SG","SGF-8562","Fixed","GD-84D  Series","0 - 100ppm","There are restrictions on the combination of sensors."]
["Ethanol","C2H5OH","64-17-5","C2H6O","SG","SGF-8562","Fixed","GD-84D  Series","0 - 2000 ppm","There are restrictions on the combination of sensors."]
["Isobutane","i-C4H10","75-28-5","C4H10","HW","NCF-6318","Fixed","GD-84D  Series","0 - 100 %LEL","There are restrictions on the combination of sensors."]
["Hydrogen","H2","1333-74-0","H2","HW","NCF-6318","Fixed","GD-84D  Series","0 - 2 vol%","There are restrictions on the combination of sensors."]
["Hydrogen","H2","1333-74-0","H2","HW","NCF-6318","Fixed","GD-84D  Series","0 - 100 %LEL","There are restrictions on the combination of sensors."]
["n-Hexane","n-C6H14","110-54-3","C6H14","HW","NCF-6318","Fixed","GD-84D  Series","0 - 2000 ppm","There are restrictions on the combination of sensors."]
["Hydrogen","H2","1333-74-0","H2","HW","NCF-6318","Fixed","GD-84D  Series","0 - 1 vol%","There are restrictions on the combination of sensors."]
["Isopropyl Alcohol","IPA","67-63-0","C3H8O","HW","NCF-6318","Fixed","GD-84D  Series","0 - 100 %LEL","There are restrictions on the combination of sensors."]
["Ethane","C2H6","74-84-0","C2H6","HW","NCF-6318","Fixed","GD-84D  Series","0～100%LEL","There are restrictions on the combination of sensors."]
["Toluene","C7H8","108-88-3","C7H8","HW","NCF-6318","Fixed","GD-84D  Series","0 - 100 %LEL","There are restrictions on the combination of sensors."]
["Acetone","C3H6O","67-64-1","C3H6O","HW","NCF-6318","Fixed","GD-84D  Series","0 - 100 %LEL","There are restrictions on the combination of sensors."]
["Hydrogen","H2","1333-74-0","H2","HW","NCF-6318","Fixed","GD-84D  Series","0 - 4 vol%","There are restrictions on the combination of sensors."]
["N,N-Dimethylacetamide","DMAC","127-19-5","C4H9NO","HW","NCF-6318","Fixed","GD-84D  Series","0 - 4000ppm","There are restrictions on the combination of sensors."]
["Acetylene","C2H2","74-86-2","C2H2","HW","NCF-6318","Fixed","GD-84D  Series","0 - 100 %LEL","There are restrictions on the combination of sensors."]
["Ethylene","C2H4","74-85-1","C2H4","HW","NCF-6318","Fixed","GD-84D  Series","0 - 100 %LEL","There are restrictions on the combination of sensors."]
["Propane","C3H8","74-98-6","C3H8","HW","NCF-6318","Fixed","GD-84D  Series","0 - 100 %LEL","There are restrictions on the combination of sensors."]
["n-Octane","C8H18","111-65-9","C8H18","HW","NCF-6318","Fixed","GD-84D  Series","0 - 100 %LEL","There are restrictions on the combination of sensors."]
["Ethanol","C2H5OH","64-17-5","C2H6O","HW","NCF-6318","Fixed","GD-84D  Series","0 - 100 %LEL","There are restrictions on the combination of sensors."]
["Methanol","CH3OH","67-56-1","CH4O","HW","NCF-6318","Fixed","GD-84D  Series","0 - 100 %LEL","There are restrictions on the combination of sensors."]
["Propylene","C3H6","115-07-1","C3H6","HW","NCF-6318","Fixed","GD-84D  Series","0 - 100 %LEL","There are restrictions on the combination of sensors."]
["Methane","CH4","74-82-8","CH4","HW","NCF-6318","Fixed","GD-84D  Series","0 - 100 %LEL","There are restrictions on the combination of sensors."]
["Methane","CH4","74-82-8","CH4","HW","NCF-6318","Fixed","GD-84D  Series","0 - 2 vol%","There are restrictions on the combination of sensors."]
["Methane","CH4","74-82-8","CH4","HW","NCF-6318","Fixed","GD-84D  Series","0 - 20000 ppm","There are restrictions on the combination of sensors."]
["Hydrogen","H2","1333-74-0","H2","HW","NCF-6320","Fixed","GD-84D  Series","0 - 100 %LEL","There are restrictions on the combination of sensors."]
["Hydrogen","H2","1333-74-0","H2","HW","NCF-6320","Fixed","GD-84D  Series","2 vol%","There are restrictions on the combination of sensors."]
["Hydrogen","H2","1333-74-0","H2","HW","NCF-6320","Fixed","GD-84D  Series","0 - 2000 ppm","There are restrictions on the combination of sensors."]
["Isobutane","i-C4H10","75-28-5","C4H10","HW","NCF-6319","Fixed","GD-84D  Series","0 - 100%LEL","There are restrictions on the combination of sensors."]
["Hydrogen","H2","1333-74-0","H2","HW","NCF-6319","Fixed","GD-84D  Series","0 - 2vol%","There are restrictions on the combination of sensors."]
["Hydrogen","H2","1333-74-0","H2","HW","NCF-6319","Fixed","GD-84D  Series","0 - 100%LEL","There are restrictions on the combination of sensors."]
["n-Hexane","n-C6H14","110-54-3","C6H14","HW","NCF-6319","Fixed","GD-84D  Series","0 - 2000ppm","There are restrictions on the combination of sensors."]
["Hydrogen","H2","1333-74-0","H2","HW","NCF-6319","Fixed","GD-84D  Series","0 - 1vol%","There are restrictions on the combination of sensors."]
["Isopropyl Alcohol","IPA","67-63-0","C3H8O","HW","NCF-6319","Fixed","GD-84D  Series","0 - 100%LEL","There are restrictions on the combination of sensors."]
["Toluene","C7H8","108-88-3","C7H8","HW","NCF-6319","Fixed","GD-84D  Series","0 - 100%LEL","There are restrictions on the combination of sensors."]
["Acetone","C3H6O","67-64-1","C3H6O","HW","NCF-6319","Fixed","GD-84D  Series","0 - 100%LEL","There are restrictions on the combination of sensors."]
["Hydrogen","H2","1333-74-0","H2","HW","NCF-6319","Fixed","GD-84D  Series","0 - 4vol%","There are restrictions on the combination of sensors."]
["N,N-Dimethylacetamide","DMAC","127-19-5","C4H9NO","HW","NCF-6319","Fixed","GD-84D  Series","0 - 4000ppm","There are restrictions on the combination of sensors."]
["Acetylene","C2H2","74-86-2","C2H2","HW","NCF-6319","Fixed","GD-84D  Series","0 - 100%LEL","There are restrictions on the combination of sensors."]
["Ethylene","C2H4","74-85-1","C2H4","HW","NCF-6319","Fixed","GD-84D  Series","0 - 100%LEL","There are restrictions on the combination of sensors."]
["n-Octane","C8H18","111-65-9","C8H18","HW","NCF-6319","Fixed","GD-84D  Series","0 - 100%LEL","There are restrictions on the combination of sensors."]
["Ethanol","C2H5OH","64-17-5","C2H6O","HW","NCF-6319","Fixed","GD-84D  Series","0 - 100%LEL","There are restrictions on the combination of sensors."]
["Methanol","CH3OH","67-56-1","CH4O","HW","NCF-6319","Fixed","GD-84D  Series","0 - 100%LEL","There are restrictions on the combination of sensors."]
["Propylene","C3H6","115-07-1","C3H6","HW","NCF-6319","Fixed","GD-84D  Series","0 - 100%LEL","There are restrictions on the combination of sensors."]
["Vinyl chloride","VCM","75-01-4","C2H3CL","HW","NCF-6319","Fixed","GD-84D  Series","0 - 100%LEL","There are restrictions on the combination of sensors."]
["Isobuten","i-C4H8","115-11-7","C4H8","HW","NCF-6319","Fixed","GD-84D  Series","0 - 100%LEL","There are restrictions on the combination of sensors."]
["1,3-Butadiene","C4H6","106-99-0","C4H6","HW","NCF-6319","Fixed","GD-84D  Series","0 - 100%LEL","There are restrictions on the combination of sensors."]
["Methane","CH4","74-82-8","CH4","HW","NCR-6309","Portable","GX-3R/GX-3R Pro/GX-2100","0～100%LEL"]
["Isobutane","i-C4H10","75-28-5","C4H10","HW","NCR-6309","Portable","GX-3R/GX-3R Pro/GX-2100","0～100%LEL"]
["Oxygen","O2","7782-44-7","O2","ES","ESR-X13P","Portable","GX-3R/GX-3R Pro","0～25vol%"]
["Hydrogen Sulfide","H2S","7783-06-4","H2S","ES","ESR-A1DP","Portable","GX-3R/GX-3R Pro/GX-2100","0～30ppm","Dual sensor for H2S and CO"]
["Carbon Monoxide","CO","630-08-0","CO","ES","ESR-A1DP","Portable","GX-3R/GX-3R Pro/GX-2100","0～500ppm","Dual sensor for H2S and CO"]
["Carbon Monoxide","CO","630-08-0","CO","ES","ESR-A1CP","Portable","GX-3R/GX-3R Pro","0～500ppm","Hydrogen interference reduction"]
["Sulfur dioxide","SO2","7446-09-5","SO2","ES","ESR-A13D","Portable","GX-3R Pro","0～20ppm"]
["Hydrogen Sulfide","H2S","7783-06-4","H2S","ES","ESR-A13i","Portable","GX-3R/GX-3R Pro","0～100ppm"]
["Carbon Monoxide","CO","630-08-0","CO","ES","ESR-A13P","Portable","GX-3R/GX-3R Pro","0～500ppm"]
["Hydrogen Cyanide","HCN","74-90-8","HCN","ES","ESR-A13D","Portable","GX-3R Pro","0～30ppm"]
["Nitrogen Dioxide","NO2","10102-44-0","NO2","ES","ESR-A13D","Portable","GX-3R Pro","0～20ppm"]
["Phosphine","PH3","7803-51-2","PH3","ES","ESR-A13D2","Portable","GX-3R Pro","0～20ppm"]
["Anmonia","NH3","7664-41-7","NH3","ES","ESR-B134","Portable","GX-3R Pro","0～400ppm"]
["Carbon Dioxide","CO2","124-38-9","CO2","RI","IRR-0409","Portable","GX-3R Pro","0～5vol％"]
["Carbon Dioxide","CO2","124-38-9","CO2","RI","IRR-0433","Portable","GX-3R Pro","0～10000ppm"]
["Oxygen","O2","7782-44-7","O2","OX","OS-BM2C","Portable","OX-04G","0～25vol%"]
["Oxygen","O2","7782-44-7","O2","ES","ESR-X13P","Portable","OX-04","0～25vol%"]
["Hydrogen Sulfide","H2S","7783-06-4","H2S","ES","ESR-A13i","Portable","HS-04","0～100ppm"]
["Carbon Monoxide","CO","630-08-0","CO","ES","ESR-A13P","Portable","CO-04","0～500ppm"]
["Carbon Monoxide","CO","630-08-0","CO","ES","ESR-A1CP","Portable","CO-04(C-)","0～500ppm","Hydrogen interference reduction"]
["Carbon Monoxide","CO","630-08-0","CO","ES","ESR-X1DP","Portable","CX-04","0～500ppm","Dual sensor for CO and O2"]
["Oxygen","O2","7782-44-7","O2","ES","ESR-X1DP","Portable","CX-04","0～25vol%","Dual sensor for CO and O2"]
["Sulfur dioxide","SO2","7446-09-5","SO2","ES","ESR-A13D","Portable","SC-04","0～20ppm"]
["Nitrogen Dioxide","NO2","10102-44-0","NO2","ES","ESR-A13D","Portable","SC-04","0～20ppm"]
["Hydrogen Cyanide","HCN","74-90-8","HCN","ES","ESR-A13D","Portable","SC-04","0～30ppm"]
["Phosphine","PH3","7803-51-2","PH3","ES","ESR-A13D2","Portable","SC-04","0～20ppm"]
["Anmonia","NH3","7664-41-7","NH3","ES","ESR-B134","Portable","SC-04","0～300ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESR-B136","Portable","SC-04","0～10ppm"]
["Carbon Monoxide","CO","630-08-0","CO","ES","ESR-A1CP","Portable","CO-04BT(C-)","0～500ppm","Hydrogen interference reduction"]
["Carbon Monoxide","CO","630-08-0","CO","ES","ESR-X1DP","Portable","CX-04BT","0～500ppm","Dual sensor for CO and O2"]
["Oxygen","O2","7782-44-7","O2","ES","ESR-X1DP","Portable","CX-04BT","0～25vol%","Dual sensor for CO and O2"]
["Oxygen","O2","7782-44-7","O2","OS","OS-BM2C","Portable","GW-3(O2)","0～25vol%"]
["Oxygen","O2","7782-44-7","O2","ES","ESR-X13P2","Portable","GW-3(OX)","0～25vol%"]
["Hydrogen Sulfide","H2S","7783-06-4","H2S","ES","ESR-A13i","Portable","GW-3(HS)","0～100ppm"]
["Carbon Monoxide","CO","630-08-0","CO","ES","ESR-A13P","Portable","GW-3(CO)","0～500ppm"]
["Carbon Monoxide","CO","630-08-0","CO","ES","ESR-A1CP","Portable","GW-3(C-)","0～500ppm","Hydrogen interference reduction"]
["Oxygen","O2","7782-44-7","O2","ES","ESR-X1DP","Portable","GW-3(CX)","0～25vol%","Dual sensor for O2 and CO"]
["Carbon Monoxide","CO","630-08-0","CO","ES","ESR-X1DP","Portable","GW-3(CX)","0～500ppm","Dual sensor for O2S and CO"]
["Methane","CH4","74-82-8","CH4","RI","IRF-1301","Fixed","SD-3 Series","0-100%LEL"]
["Isobutane","i-C4H10","75-28-5","C4H10","RI","IRF-1303","Fixed","SD-3 Series","0-100%LEL"]
["Propane","C3H8","74-98-6","C3H8","RI","IRF-1315","Fixed","SD-3 Series","0-100%LEL"]
["Carbon Dioxide","CO2","124-38-9","CO2","RI","IRF-1435","Fixed","SD-3 Series","0-2000ppm"]
["Carbon Dioxide","CO2","124-38-9","CO2","RI","IRF-1436","Fixed","SD-3 Series","0-5000ppm"]
["Carbon Dioxide","CO2","124-38-9","CO2","RI","IRF-1433","Fixed","SD-3 Series","0-10000ppm"]
["Carbon Dioxide","CO2","124-38-9","CO2","RI","IRF-1437","Fixed","SD-3 Series","0-2vol%"]
["Carbon Dioxide","CO2","124-38-9","CO2","RI","IRF-1438","Fixed","SD-3 Series","0-5vol%"]
["Carbon Dioxide","CO2","124-38-9","CO2","RI","IRF-1439","Fixed","SD-3 Series","0-10vol%"]
["Methane","CH4","74-82-8","CH4","RI","IRF-1334","Fixed","SD-3 Series","0-100vol%"]
["Ethylene","C2H4","74-85-1","C2H4","RI","IRF-1316","Fixed","SD-3 Series","0-100%LEL"]
["Isobutene","i-C4H8","115-11-7","C4H8","RI","IRF-1340","Fixed","SD-3 Series","0-100%LEL"]
["1,3-Butadiene","C4H6","106-99-0","C4H6","RI","IRF-1332","Fixed","SD-3 Series","0-100%LEL"]
["Ethane","C2H6","74-84-0","C2H6","HW","NCF-6318","Fixed","SD-3 Series","0～100%LEL"]
["Propane","C3H8","74-98-6","C3H8","HW","NCF-6318","Fixed","SD-3 Series","0～100%LEL"]
["Methane","CH4","74-82-8","CH4","HW","NCF-6318","Fixed","SD-3 Series","0～100%LEL"]
["Methane","CH4","74-82-8","CH4","HW","NCF-6318","Fixed","SD-3 Series","0～2vol%"]
["Methane","CH4","74-82-8","CH4","HW","NCF-6318","Fixed","SD-3 Series","0～20000ppm"]
["Hydrogen","H2","1333-74-0","H2","HW","NCF-6320","Fixed","SD-3 Series","0～100%LEL"]
["Hydrogen","H2","1333-74-0","H2","HW","NCF-6320","Fixed","SD-3 Series","0～2vol%"]
["Hydrogen","H2","1333-74-0","H2","HW","NCF-6320","Fixed","SD-3 Series","0～2000ppm"]
["Isobutane","i-C4H10","75-28-5","C4H10","HW","NCF-6319","Fixed","SD-3 Series","0～100%LEL"]
["Hydrogen","H2","1333-74-0","H2","HW","NCF-6319","Fixed","SD-3 Series","0～2vol%"]
["Hydrogen","H2","1333-74-0","H2","HW","NCF-6319","Fixed","SD-3 Series","0～100%LEL"]
["n-Hexane","n-C6H14","110-54-3","C6H14","HW","NCF-6319","Fixed","SD-3 Series","0～2000ppm"]
["Hydrogen","H2","1333-74-0","H2","HW","NCF-6319","Fixed","SD-3 Series","0～1vol%"]
["Isopropyl Alcohol","IPA","67-63-0","C3H8O","HW","NCF-6319","Fixed","SD-3 Series","0～100%LEL"]
["Toluene","C7H8","108-88-3","C7H8","HW","NCF-6319","Fixed","SD-3 Series","0～100%LEL"]
["Acetone","C3H6O","67-64-1","C3H6O","HW","NCF-6319","Fixed","SD-3 Series","0～100%LEL"]
["Hydrogen","H2","1333-74-0","H2","HW","NCF-6319","Fixed","SD-3 Series","0～4vol%"]
["N,N-Dimethylacetamide","DMAC","127-19-5","C4H9NO","HW","NCF-6319","Fixed","SD-3 Series","0～4000ppm"]
["Acetylene","C2H2","74-86-2","C2H2","HW","NCF-6319","Fixed","SD-3 Series","0～100%LEL"]
["Ethylene","C2H4","74-85-1","C2H4","HW","NCF-6319","Fixed","SD-3 Series","0～100%LEL"]
["n-Octane","C8H18","111-65-9","C8H18","HW","NCF-6319","Fixed","SD-3 Series","0～100%LEL"]
["Ethanol","C2H5OH","64-17-5","C2H6O","HW","NCF-6319","Fixed","SD-3 Series","0～100%LEL"]
["Methanol","CH3OH","67-56-1","CH4O","HW","NCF-6319","Fixed","SD-3 Series","0～100%LEL"]
["Propylene","C3H6","115-07-1","C3H6","HW","NCF-6319","Fixed","SD-3 Series","0～100%LEL"]
["Vinyl chloride","VCM","75-01-4","C2H3CL","HW","NCF-6319","Fixed","SD-3 Series","0～100%LEL"]
["Hydrogen Sulfide","H2S","7783-06-4","H2S","SG","SGF-8562","Fixed","SD-3 Series","0～100ppm"]
["Carbon Monoxide","CO","630-08-0","CO","SH","SHF-8601","Fixed","SD-3 Series","0～1000ppm"]
["Hydrogen","H2","1333-74-0","H2","SH","SHF-8603","Fixed","SD-3 Series","0～500ppm"]
["Hydrogen","H2","1333-74-0","H2","SH","SHF-8603","Fixed","SD-3 Series","0～1000ppm"]
["Hydrogen","H2","1333-74-0","H2","SH","SHF-8603","Fixed","SD-3 Series","0～2000ppm"]
["Deuterium","D2","7782-39-0","-","SH","SHF-8603","Fixed","SD-3 Series","0～2000ppm"]
["Hydrogen Sulfide","H2S","7783-06-4","H2S","ES","ESF-A24RH","Fixed","SD-3 Series","0～30ppm","Sensor for high humidity/Range: 40～95%RH"]
["Hydrogen Sulfide","H2S","7783-06-4","H2S","ES","ESF-A24R","Fixed","SD-3 Series","0～100ppm"]
["Methane","CH4","74-82-8","CH4","HW","NCF-6322P","Portable","GX-9000/GX-9000H","0～100%LEL"]
["Isobutane","i-C4H10","75-28-5","C4H10","HW","NCF-6322P","Portable","GX-9000","0～100%LEL"]
["Hydrogen","H2","1333-74-0","H2","HW","NCF-6322P","Portable","GX-9000","0～100%LEL"]
["Acetylene","C2H2","74-86-2","C2H2","HW","NCF-6322P","Portable","GX-9000","0～100%LEL"]
["Methane","CH4","74-82-8","CH4","TE","TEF-7520P","Portable","GX-9000/GX-9000H","0～100vol%"]
["Isobutane","i-C4H10","75-28-5","C4H10","TE","TEF-7520P","Portable","GX-9000","0～100vol%"]
["Hydrogen","H2","1333-74-0","H2","TE","TEF-7520P","Portable","GX-9000","0～100vol%"]
["Methane","CH4","74-82-8","CH4","RI","IRF-4341","Portable","GX-9000/GX-9000H","0～100%LEL～100vol%"]
["Isobutane","i-C4H10","75-28-5","C4H10","RI","IRF-4345","Portable","GX-9000/GX-9000H","0～100%LEL～100vol%"]
["Carbon Dioxide","CO2","124-38-9","CO2","RI","IRF-4443","Portable","GX-9000","0～20vol%"]
["Oxygen","O2","7782-44-7","O2","ES","ESR-X13P","Portable","GX-9000/GX-9000H","0～25vol%"]
["Hydrogen Sulfide","H2S","7783-06-4","H2S","ES","ESR-A13i","Portable","GX-9000/GX-9000H","0～100ppm"]
["Carbon Monoxide","CO","630-08-0","CO","ES","ESR-A13P","Portable","GX-9000/GX-9000H","0～500ppm"]
["Hydrogen Sulfide","H2S","7783-06-4","H2S","ES","ESF-A24R2","Portable","GX-9000H","0～1000ppm"]
["Anmonia","NH3","7664-41-7","NH3","ES","ESF-B242","Portable","GX-9000","0～75ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESF-C92","Portable","GX-9000","0～1.5ppm"]
["Ozone","O3","10028-15-6","O3","ES","ESF-B249","Portable","GX-9000","0～0.6ppm"]
["Hydrogen Chloride","HCL","7647-01-0","HCL","ES","ESF-A24E2","Portable","GX-9000","0～6ppm"]
["Sulfur dioxide","SO2","7446-09-5","SO2","ES","ESF-A24D4","Portable","GX-9000","0～100ppm"]
["VOC","VOC","-","-","PID","PIF-001","Portable","GX-9000/GX-9000H","0～40000ppb"]
["VOC","VOC","-","-","PID","PIF-002","Portable","GX-9000/GX-9000H","0～4000ppm"]
["VOC","VOC","-","-","PID","PIF-003","Portable","GX-9000","0～100ppm"]
["Methane","CH4","74-82-8","CH4","HW","NCR-6309","Portable","GX-Force","0～100%LEL"]
["Isobutane","i-C4H10","75-28-5","C4H10","HW","NCR-6309","Portable","GX-Force","0～100%LEL"]
["Oxygen","O2","7782-44-7","O2","ES","ESR-X13P","Portable","GX-Force","0～25vol%"]
["Hydrogen Sulfide","H2S","7783-06-4","H2S","ES","ESR-A1DP","Portable","GX-Force","0～30ppm","Dual sensor for H2S and CO"]
["Carbon Monoxide","CO","630-08-0","CO","ES","ESR-A1DP","Portable","GX-Force","0～500ppm","Dual sensor for H2S and CO"]
["Hydrogen Sulfide","H2S","7783-06-4","H2S","ES","ESR-A13i","Portable","GX-Force","0～100ppm"]
["Carbon Monoxide","CO","630-08-0","CO","ES","ESR-A13P","Portable","GX-Force","0～500ppm"]
["Carbon Monoxide","CO","630-08-0","CO","ES","ESR-A1CP","Portable","GX-Force","0～500ppm","Hydrogen interference reduction"]
["Oxygen","O2","7782-44-7","O2","ES","OS-BM1E","Portable","OX-08","0～40vol%","Hydrogen interference reduction"]
["Carbon Monoxide","CO","630-08-0","CO","SG","SG-8751","Fixed","GD-1V  Series","0～75ppm/0～100ppm/0～150ppm/0～200ppm"]
["Oxygen","O2","7782-44-7","O2","ES","OS-B11E-A","Fixed","GD-1OX  Series","0～5vol%/0～10vol%/0～25vol%"]
["Carbon Dioxide","CO2","124-38-9","CO2","RI","IRF-1443","Fixed","SD-3 Series","0-20vol%"]
["Carbon Dioxide","CO2","124-38-9","CO2","RI","IRF-1456","Fixed","SD-3 Series","0-50vol%"]
["Carbon Dioxide","CO2","124-38-9","CO2","RI","IRF-1457","Fixed","SD-3 Series","0-100vol%"]
["Carbon Monoxide","CO","630-08-0","CO","RI","IRF-1458","Fixed","SD-3 Series","0-5vol%"]
["Carbon Monoxide","CO","630-08-0","CO","RI","IRF-1459","Fixed","SD-3 Series","0-10vol%"]
["Carbon Monoxide","CO","630-08-0","CO","RI","IRF-1460","Fixed","SD-3 Series","0-20vol%"]
["Carbon Monoxide","CO","630-08-0","CO","RI","IRF-1461","Fixed","SD-3 Series","0-50vol%"]
["Carbon Monoxide","CO","630-08-0","CO","RI","IRF-1462","Fixed","SD-3 Series","0-100vol%"]
["Toluene","C7H8","108-88-3","C7H8","RI","IRF-1310","Fixed","SD-3 Series","0-100%LEL"]
["Ethylbenzene","C8H10","100-41-4","C8H10","RI","IRF-1348","Fixed","SD-3 Series","0-100%LEL"]
["Propylene","C3H6","115-07-1","C3H6","RI","IRF-1347","Fixed","SD-3 Series","0-100%LEL"]
["Acetone","C3H6O","67-64-1","C3H6O","RI","IRF-1327","Fixed","SD-3 Series","0-100%LEL"]
["Benzene","C6H6","71-43-2","C6H6","RI","IRF-1318","Fixed","SD-3 Series","0-100%LEL"]
["Difluoromethane","R-32","75-10-5","CH2F2","RI","IRF-1352","Fixed","SD-3 Series","0-20000ppm"]
["Propane","C3H8","74-98-6","C3H8","RI","IRF-1315","Fixed","SD-3 Series","0-100vol%"]
["Isobutane","i-C4H10","75-28-5","C4H10","RI","IRF-1320","Fixed","SD-3 Series","0-100vol%"]
["Isobutene","i-C4H8","115-11-7","C4H8","RI","IRF-1355","Fixed","SD-3 Series","0-100vol%"]
["Isobutane","i-C4H10","75-28-5","C4H10","RI","IRF-1303","Fixed","SD-3 Series","0-100%LEL"]
["Propane","C3H8","74-98-6","C3H8","RI","IRF-1317","Fixed","SD-3 Series","0-100%LEL"]
["n-Hexane","n-C6H14","110-54-3","C6H14","RI","IRF-1308","Fixed","SD-3 Series","0-100%LEL"]
["Pentane","n-C5H12","109-66-0","C5H12","RI","IRF-1329","Fixed","SD-3 Series","0-100%LEL"]
["Ethane","C2H6","74-84-0","C2H6","RI","IRF-1331","Fixed","SD-3 Series","0-100%LEL"]
["n-Butane","n-C4H10","106-97-8","C4H10","RI","IRF-1346","Fixed","SD-3 Series","0-100%LEL"]
["Methanol","CH3OH","67-56-1","CH4O","RI","IRF-1311","Fixed","SD-3 Series","0-100%LEL"]
["Ethanol","C2H5OH","64-17-5","C2H6O","RI","IRF-1306","Fixed","SD-3 Series","0-100%LEL"]
["Isopropyl Alcohol","IPA","67-63-0","C3H8O","RI","IRF-1307","Fixed","SD-3 Series","0-100%LEL"]
["n-Heptane","n-C7H16","142-82-5","C7H16","RI","IRF-1319","Fixed","SD-3 Series","0-100%LEL"]
["Cyclohexane","C6H12","110-82-7","C6H12","RI","IRF-1349","Fixed","SD-3 Series","0-100%LEL"]
["n-Propanol","C3H8O","71-23-8","C3H8O","RI","IRF-1351","Fixed","SD-3 Series","0-100%LEL"]
["Tetrahydrofuran","THF","109-99-9","C4H8O","RI","IRF-1325","Fixed","SD-3 Series","0-100%LEL"]
["Ethanol","C2H5OH","64-17-5","C2H6O","RI","IRF-1363","Fixed","SD-3 Series","0-10vol%"]
["Methyl ethyl ketone","MEK","78-93-3","C4H8O","RI","IRF-1313","Fixed","SD-3 Series","0-100%LEL"]
["Ethyl Acetate","EtAc","141-78-6","C4H8O2","RI","IRF-1314","Fixed","SD-3 Series","0-100%LEL"]
["Methyl isobutyl ketone","MIBK","108-10-1","C6H12O","RI","IRF-1350","Fixed","SD-3 Series","0-100%LEL"]
["Cyclohexane","C6H12","110-82-7","C6H12","RI","IRF-1365","Fixed","SD-3 Series","0-5000ppm"]
["Nitrogen Dioxide","NO2","10102-44-0","NO2","ES","ESF-A24A","Fixed","SD-3 Series","0～15ppm"]
["Oxygen","O2","7782-44-7","O2","ES","ESF-X24P2","Fixed","SD-3 Series","0～25vol%"]
["Carbon Monoxide","CO","630-08-0","CO","ES","ESF-A24P","Fixed","SD-3 Series","0～150ppm"]
["Anmonia","NH3","7664-41-7","NH3","ES","ESF-B22","Fixed","SD-3 Series","0～75ppm"]
["Anmonia","NH3","7664-41-7","NH3","ES","ESF-B22","Fixed","SD-3 Series","0～150ppm"]
["Anmonia","NH3","7664-41-7","NH3","ES","ESF-B22","Fixed","SD-3 Series","0～400ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESF-C92","Fixed","SD-3 Series","0～1.5ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESF-C92","Fixed","SD-3 Series","0～3ppm"]
["Chlorine","CL2","7782-50-5","CL2","ES","ESF-C92","Fixed","SD-3 Series","0～10ppm"]
["Oxygen","O2","7782-44-7","O2","OS","OS-BM1D","Fixed","OX-600","0～25vol%/0～50vol%"]
["Carbon Monoxide","CO","630-08-0","CO","ES","ES-031M","Fixed","EC-600","0～150ppm"]
["Carbon Dioxide","CO2","124-38-9","CO2","RI","DES-3311-5","Fixed","RI-600","0～2000ppm/0～5000ppm/0～10000ppm"]
["Carbon Dioxide","CO2","124-38-9","CO2","RI","DES-3311-6","Fixed","RI-600","0～2vol%/0～5vol%"]
["Arsine","AsH3","7784-42-1","AsH3","FP","FT-002C","Fixed","FP-270As","0～15ppb","1 month specification. Detection cycle: 30 sec."]
["Arsine","AsH3","7784-42-1","AsH3","FP","FT-002D","Fixed","FP-270As","0～15ppb","2 months specification. Detection cycle: 30 sec."]
["Ethyl(methyl)azanide;af","TEMAH","352535-01-4","Hf[N(C2H5)CH3]4","FP","FT-010","Fixed","FP-270","0～0.9ppm","Detection cycle: 45 sec"]
["Trimethylaluminum","TMAL","75-24-1","C3H9AL","FP","FT-202","Fixed","FP-270","1.5～6ppm","Detection cycle: 60 sec"]
["Hydrogen Chloride","HCL","7647-01-0","HCL","FP","FC-004","Fixed","FP-300  Series","0.25～1ppm","Detection cycle: 90 sec"]
["Hydrogen Bromide","HBr","10035-10-6","HBr","FP","FC-004","Fixed","FP-300  Series","0～2ppm","Detection cycle: 30 sec"]
["Hydrogen Chloride","HCL","7647-01-0","HCL","FP","FC-005","Fixed","FP-300  Series","1.5～8ppm","Detection cycle: 30 sec"]
["Hydrogen Fluoride","HF","7664-39-3","HF","FP","FC-006","Fixed","FP-300  Series","0～9ppm","Detection cycle: 20 sec"]
["Chlorine Trifluoride","CLF3","7790-91-2","CLF3","FP","FC-006","Fixed","FP-300  Series","0～500ppb","Detection cycle: 60 sec"]
["Anmonia","NH3","7664-41-7","NH3","FP","FC-010","Fixed","FP-300  Series","0.5～4ppm","Detection cycle: 180 sec"]
["Ethyl(methyl)azanide;af","TEMAH","352535-01-4","Hf[N(C2H5)CH3]4","FP","FC-010","Fixed","FP-300  Series","0～6ppm","Detection cycle: 180 sec"]
["Trimethylamine","TMA","75-50-3","C3H9N","FP","FC-010","Fixed","FP-300  Series","0～1ppm","Detection cycle: 300 sec"]
["Chlorine","CL2","7782-50-5","CL2","FP","FC-303","Fixed","FP-300  Series","0～1.5ppm","Detection cycle: 60 sec"]
["Chlorine","CL2","7782-50-5","CL2","FP","FC-303","Fixed","FP-300  Series","0～100ppb","Detection cycle: 300 sec"]
["Ruthenium Oxide","RuO4","20427-56-9","RuO4","FP","FC-303","Fixed","FP-300  Series","0～1000ppb","Detection cycle: 60 sec"]
["Arsine","AsH3","7784-42-1","AsH3","FP","FCL-001","Fixed","FP-300  Series","0～150ppb","Detection cycle: 60 sec"]
["Hydrogen Sulfide","H2S","7783-06-4","H2S","FP","FCL-001","Fixed","FP-300  Series","0～100ppb","Detection cycle: 600 sec"]
["Hydrogen Sulfide","H2S","7783-06-4","H2S","FP","FCL-001","Fixed","FP-300  Series","0～10ppm","Detection cycle: 20 sec"]
["Phosphine","PH3","7803-51-2","PH3","FP","FCL-001","Fixed","FP-300  Series","0～500ppb","Detection cycle: 60 sec"]
["Hydrogen Selenide","H2Se","7783-07-5","H2Se","FP","FCL-001","Fixed","FP-300  Series","0～200ppb","Detection cycle: 60 sec"]
["Arsine","AsH3","7784-42-1","AsH3","FP","FCL-001","Fixed","FP-300  Series","0～15ppb","Detection cycle: 180 sec"]
["Silane","SiH4","7803-62-5","SiH4","FP","FCL-002E","Fixed","FP-300  Series","0～15ppm","Detection cycle: 60 sec"]
["Diborane","B2H6","19287-45-7","B2H6","FP","FCL-002E","Fixed","FP-300  Series","0～300ppb","Detection cycle: 60 sec"]
["Phosphine","PH3","7803-51-2","PH3","FP","FCL-002E","Fixed","FP-300  Series","0～900ppb","Detection cycle: 30 sec"]
["Phosphine","PH3","7803-51-2","PH3","FP","FCL-002E","Fixed","FP-300  Series","0～0.3ppm","Detection cycle: 50 sec"]
["Arsine","AsH3","7784-42-1","AsH3","FP","FCL-002E","Fixed","FP-300  Series","0～150ppb","Detection cycle: 60 sec"]
["Disilane","Si2H6","1590-87-0","Si2H6","FP","FCL-002E","Fixed","FP-300  Series","0～10ppm","Detection cycle: 20 sec"]
["Tertiarybutylarsine","TBAs","4262-43-5","C4H11As","FP","FCL-002E","Fixed","FP-300  Series","0～150ppb","Detection cycle: 180 sec"]
["Hydrogen Sulfide","H2S","7783-06-4","H2S","FP","FCL-002E","Fixed","FP-300  Series","0～100ppb","Detection cycle: 600 sec"]
["Hydrogen Sulfide","H2S","7783-06-4","H2S","FP","FCL-002E","Fixed","FP-300  Series","0～10ppm","Detection cycle: 20 sec"]
["Hydrogen Sulfide","H2S","7783-06-4","H2S","FP","FCL-002E","Fixed","FP-300  Series","0～1000ppb","Detection cycle: 50 sec"]
["Chlorine","CL2","7782-50-5","CL2","FP","FCL-015E","Fixed","FP-300  Series","0～0.8ppm","Detection cycle: 30 sec"]
["Chlorine","CL2","7782-50-5","CL2","FP","FCL-015E","Fixed","FP-300  Series","0～1.5ppm","Detection cycle: 10 sec"]
["Gelmane","GeH4","7782-65-2","GeH4","FP","FCL-202E","Fixed","FP-300  Series","0～6ppm","Detection cycle: 90 sec"]
["Gelmane","GeH4","7782-65-2","GeH4","FP","FCL-202E","Fixed","FP-300  Series","0～2ppm","Detection cycle: 90 sec"]
["Phosphine","PH3","7803-51-2","PH3","FP","FCL-001","Fixed","FP-300  Series","0～900ppb","Detection cycle: 30 sec"]
["Phosgene","COCL2","75-44-5","COCL2","FP","FC-108A","Fixed","FP-300  Series","0～300ppb","Detection cycle: 60 sec"]
["Phosgene","COCL2","75-44-5","COCL2","FP","FC-108A","Fixed","FP-300  Series","0.2～4ppm","Detection cycle: 60 sec"]
["Octafluorocyclopentene","C5F8","559-40-0","C5F8","FP","FC-023A","Fixed","FP-300AGZS","0～5ppm","Detection cycle: 20 sec"]
["Hexafluoro-1,3-butadiene","C4F6","685-63-2","C4F6","FP","FC-023A","Fixed","FP-300AGZS","0～5ppm","Detection cycle: 20 sec"]
["1,3,3,4,4,5,5-Heptafluorocyclopentene","C5HF7","1892-03-1","C5HF7","FP","FC-023A","Fixed","FP-300AGZS","0～5ppm","Detection cycle: 20 sec"]
["Hexafluoropropylene","C3F6","116-15-4","C3F6","FP","FC-023A","Fixed","FP-300AGZS","0～5ppm","Detection cycle: 20 sec"]
["Octafluorocyclopentene","C5F8","559-40-0","C5F8","FP","FC-023D","Fixed","FP-300AGZS","0～5ppm","Detection cycle: 20 sec"]
["Hexafluoro-1,3-butadiene","C4F6","685-63-2","C4F6","FP","FC-023D","Fixed","FP-300AGZS","0～5ppm","Detection cycle: 20 sec"]
["Formaldehyde","HCHO","50-00-0","CH2O","FP","FCL-018","Fixed","FP-330/FP-331","0～0.5ppm","Detection cycle: 1800 sec"]
["Formaldehyde","HCHO","50-00-0","CH2O","FP","FCL-018","Fixed","FP-330/FP-331","0～1ppm","Detection cycle: 600 sec"]
["Formaldehyde","HCHO","50-00-0","CH2O","FP","FCL-018","Fixed","FP-330/FP-331","0～5ppm","Detection cycle: 180 sec"]